{"text_format":"1","workbook":"xlsx","n_sheets":34,"sheets":["Sheet3","All Admins","Country names","Admins analyzes","Ranges summary","Sheet1","below 2 GHz","2-3 GHz","3-4,2 GHz","4,4-5 GHz","5,7-5,95 GHz","5,9-7,1 GHz","7,1-8,5 GHz","10-10,68 GHz","10,7-12,5 GHz","12,75-13,25 GHz","14-16 GHz","17-17,7 GHz","17-20,2 GHz","21,2-22 GHz","22-23,6 GHz","22,6-23 GHz","24,25-24,5 GHz","24,5-26,5 GHz","26,5-27,5 GHz","27,5-29,5 GHz","31-31,3 GHz","31,8-33,4 GHz","36-37 GHz","37-39,5 GHz","39,5-40,5 GHz","40,5-43,5 GHz","above 43,5 GHz","Alf Admins"],"not_rendered":{"charts":1,"images":0,"macros":1,"external_links":1,"defined_names":26,"comments":10,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet3","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"All Admins","index":1,"n_rows":1023,"n_cols":55,"rows_kept":1023,"cut":false,"hidden":false,"merged":[[1,19,1,24],[1,25,1,28],[2,8,2,9],[2,10,2,11],[2,19,2,21],[2,22,2,24],[1,4,1,7],[1,8,1,9],[1,10,1,14],[1,15,1,16],[1,18,3,18],[499,12,500,12],[499,13,500,13],[499,14,500,14],[499,19,500,19],[499,4,500,4],[499,26,500,26],[499,27,500,27],[499,28,500,28],[499,20,500,20],[499,21,500,21],[499,25,500,25]]}
[1,{"$f":"A1+1","v":2},{"$f":"B1+1","v":3},4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,{"$f":"AO1+1","v":42},43,44,45,46,47,48,49,50,51,52,53,54,55]
["Respondent","Country code","Band index","Frequency band (MHz)","Licensing regime",null,null,null," Topo-logy",null,"Application",null,null,null,null,"Number of P-P links",null,"Number of CS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends (e.g. in the next 5 years)"]
[null,null,null,null,null,null,null,null,"FWA",null,"Network Infrastruc-ture",null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop length (km)"]
[null,null,null,null,"Link by link","Block","Light licensed","Licence exempt","P-P","P-MP","Mobile backhaul","Others","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","Currently congested","Planned reallocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["Bosnia and Herzegovina","BIH",0,"370-400","X",null,null,null,null,null,null,null,"X",null,null,129,null,null,null,"X",null,null,1,30,100,null,null,null,"370-400 MHz: Planned migration of P-P links to 1350-1375/1492-1517 and 1375-1400/1427-1452 MHz"]
["Bosnia and Herzegovina","BIH",0,"1350-1375 and 1492-1517","X",null,null,null,null,null,null,null,"X",null,null,48,null,null,"T/R 13-01 Annex A","X",null,null,"0.5",7,70,"+15"]
["switzerland","CHE",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,"X",null,null,15,null,"T/R 13-01 Annex A",15,null,null,20,null,30.5,"reduction"]
["Cyprus","CYP",0,"1350-1375 and 1492-1517","X",null,null,null," ",null,null,null,"X",null,null,13,null,null,"T/R 13-01 Annex A","X",null,null,0.9,null,58.65]
["Cyprus","CYP",0,"1350-1375 and 1492-1517","X",null,null,null," ",null,null,null,"X",null,null,17,null,null,null,"X",null,null,0.9,null,73.55]
["Czech Republic","CZE",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"T/R 13-01 Annex A"]
["Denmark","DNK",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Estonia","EST",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Finland","FIN",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A",null,null,null,null,null,null,null,null,null,"Planned opening 2011-2012"]
["France","FRA",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["UK","GBR",0,"1350-1375 and 1492-1517","X",null,null,null,null,null,null,null,null,"X",null,860,null,null,"T/R 13-01 Annex A","X"]
["Croatia","HRV",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Hungary","HUN",0,"1350-1375 and 1492-1517","X",null,null,null,"X","X","X",null,null,null,"Non-Civil P-P, P-MP systems",null,null,null,"T/R 13-01 Annex A",null,null,null,null,null,null,0.1]
["Iceland","ICE",0,"1350-1375 and 1492-1517","x",null,null,null,"X",null,null,null,null,null,null,null,0,null,"T/R 13-01 Annex A",null,null,null,null,null,null,0]
["Ireland","IRL",0,"1350-1375 and 1492-1517"," X",null,null,null,null,null," X",null,null,null,null,0,69,null,"T/R 13-01 Annex A"," X","X","X",0.02,23,83,48,null," X"]
["Ireland","IRL",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009 "]
["Italy","ITA",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Lithuania","LTU",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"T/R 13-01 Annex A"]
["Lithuania","LTU",0,"1350-1375 and 1492-1517",null,"X",null,null,null,"X","X",null,null,null,null,null,null,8,"local",null,null,null,null,null,null,-100]
["Luxembourg","LUX",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"T/R 13-01 Annex A","X",null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Latvia","LVA",0,"1350-1375 and 1492-1517",null,"X",null,null,null,"X",null,null,null,null,null,null,null,30,"national plan","X",null,null,null,null,null,-50]
["Netherlands","NLD",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Norway","NOR",0,"1350-1375 and 1492-1517","X",null,null,null,null,null,null,null,null,"X",null,8,46,null,"T/R 13-01 Annex A","x",null,null,1,12,42]
["Portugal","PRT",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,null,null,null,55,null,"T/R 13-01 Annex A","X",null,null,12,"40",57,5]
["Portugal","PRT",0,"1350-1375 and 1492-1517","X",null,null,null,null,"X",null,null,null,null,null,null,null,9,"T/R 13-01 Annex A","X",null,null,2,"10",18,0]
["Russia","RUS",0,"1350-1375 and 1492-1517","X","X",null,null,null,null,"X",null,null,null,null,null,25,49,"T/R 13-01 Annex A","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Serbia","SRB",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,"X",null,null,52,null,null,"T/R 13-01 Annex A","x",null,null,2,15,52,100,null,null,"From band 1517.5 - 1530 MHz"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517",null,"X",null,null,null,null,null,null,null,"X",null,null,"N/A",null,"T/R 13-01 Annex A","x",null,null,5,20,90,0,"x",null,null,"assigned all SVN (2MHz Ch.1)"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517","X",null,null,null,null,"X","X",null,null,null,null,null,null,17,"T/R 13-01 Annex A","x",null,null,5,15,50,2,"x"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,"X",null,null,null,null,null,20,null,"T/R 13-01 Annex A","x",null,null,5,20,90,10,"x"]
["Telia","TELIASON",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Austria","AUT",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,null,8,null,"T/R 13-01 Annex B","x",null,null,3,20,60]
["Bosnia and Herzegovina","BIH",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,null,null,"X",null,null,5,null,null,"T/R 13-01 Annex B","X",null,null,5,20,90,"+15"]
["switzerland","CHE",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,"X",null,null,152,null,"T/R 13-01 Annex B",152,null,null,20,null,61.9,"reduction"]
["Cyprus","CYP",0,"1375-1400 and 1427-1452","X",null,null,null," ",null,null,null,"X",null,null,6,null,null,"T/R 13-01 Annex B","X",null,null,3.52,null,35.47]
["Cyprus","CYP",0,"1375-1400 and 1427-1452","X",null,null,null," ",null,null,null,"X",null,null,8,null,null,null,"X",null,null,22.62,null,74.209999999999994]
["Czech Republic","CZE",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"T/R 13-01 Annex B"]
["Denmark","DNK",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Estonia","EST",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Finland","FIN",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,"X",null,null,null,null,null,4,null,"T/R 13-01 Annex B","X","X",null,null,null,null,null,null,null,"Planned closing 2011-2012"]
["France","FRA",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,null,1259,null,"T/R 13-01 Annex B",1259,null,null,0.1,null,95,"+ 10 %"]
["Croatia","HRV",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Hungary","HUN",0,"1375-1400 and 1427-1452","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"T/R 13-01 Annex B","X",null,null,null,20,null,0.1]
["Hungary","HUN",0,"1375-1400 and 1427-1452","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"X",null,null,null,20]
["Iceland","ICE",0,"1375-1400 and 1427-1452","x",null,null,null,"X",null,null,null,null,null,null,null,2,null,"T/R 13-01 Annex B",null,null,null,null,25,null,0]
["Ireland","IRL",0,"1375-1400 and 1427-1452"," X",null,null,null,null,null," X",null,null,null,null,37,18,null,"T/R 13-01 Annex B"," X",null,null,0.45,23,69," 0",null," X"]
["Ireland","IRL",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009 "]
["Italy","ITA",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Lithuania","LTU",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"T/R 13-01 Annex B"]
["Lithuania","LTU",0,"1375-1400 and 1427-1452",null,"X",null,null,null,"X","X",null,null,null,null,null,null,8,"local",null,null,null,null,null,null,-100]
["Luxembourg","LUX",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"T/R 13-01 Annex B","X",null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Netherlands","NLD",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Netherlands","NLD",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,null,null,null,"X",null,2,7,null,"nat. plan 1427 - 1517","x",null,null,39.299999999999997,58.9,71.400000000000006,10]
["Norway","NOR",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,null,null,null,"X",null,1,26,null,"T/R 13-01 Annex B","x",null,null,1,18,42.5]
["Portugal","PRT",0,"1375-1400 and 1427-1452","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"T/R 13-01 Annex B","X",null,null,null,"40",null,"No use at the moment."]
["Russia","RUS",0,"1375-1400 and 1427-1452","X","X",null,null,null,null,"X",null,null,null,null,null,30,49,"T/R 13-01 Annex B","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Serbia","SRB",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["Slovak Republic","SVK",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovenia","SVN",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,"X",null,null,12,null,null,"T/R 13-01 Annex B","x",null,null,2,15,52,200,null,null,"From band 1517.5 - 1530 MHz"]
["Slovenia","SVN",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,null,1,null,"T/R 13-01 Annex B",null,null,null,5,10,30,200]
["Sweden","SWE",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,null,null,59,99,null,"T/R 13-01 Annex B",null,null,null,null,null,null,null,"N"]
["Telia","TELIASON",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,"X",null,null,null,null,null,17,null,"T/R 13-01 Annex B","X",null,null,4,null,19,0,null,null,null,"IDR140"]
["Italy","ITA",0,"1400-1525","X",null,null,null,null,null,"X",null,null,null,null,null,530,null,"national","X"]
["Slovak Republic","SVK",0,"1427-1530","X",null,null,null,null,"X",null,null,null,null,null,null,null,null,"Rep.CCIR 379-5, DS 65,5MHz","x",null,null,null,null,null,-100,null,"x","no new links"]
["Slovak Republic","SVK",0,"1427-1530",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"relocation to other band"]
["Slovenia","SVN",0,"1517-1525","X",null,null,null,"X",null,null,null,"X",null,null,92,null,null,"national (500kHz)","x",null,null,2,15,52,-50,null,"x","realocated into 1.4 GHz bands"]
["Portugal","PRT",0,"1517-1525","X",null,null,null,null,null,null,null,"X",null,null,365,null,null,"National plan (STL)","X",null,null,null,"15",null,5]
["Slovenia","SVN",0,"1525-1530","X",null,null,null,"X",null,null,null,"X",null,null,6,null,null,"national (500kHz)","x",null,null,2,15,52,-100,null,"x","realocated into 1.4 GHz bands"]
["Greece","GRC",0,"1700-1710 and 1785-1800","X",null,null,null,null,null,null,null,"X",null,null,615,null,null,"national plan","X","X",null,0.4,14,90,null,"congested in urban areas"]
["Austria","AUT",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"T/R 13-01 Annex C"]
["Austria","AUT",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Bosnia and Herzegovina","BIH",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,"X",null,null,27,null,null,"T/R 13-01 Annex C","X",null,null,"1",55,99,"+10"]
["switzerland","CHE",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,"No civil FS use",null,null,null,"T/R 13-01 Annex C"]
["Cyprus","CYP",0,"2025-2110 and 2200-2290",null,null,null," ",null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,"X"]
["Czech Republic","CZE",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X",null,null,null,null,"MD shared",null,null,110,"T/R 13-01 Annex C",null,null,null,null,null,null,0]
["Denmark","DNK",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Estonia","EST",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Finland","FIN",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,"X",null,null,null,null,null,12,null,"T/R 13-01 Annex C","X","X"]
["France","FRA",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["UK","GBR",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,null,"row missing in the questionnaire"]
["Greece","GRC",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,"X",null,null,null,null,null,206,null,"T/R 13-01 Annex C","X","X",null,0.6,21,60,"reduction"]
["Croatia","HRV",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,"X",null,null,182,null,null,"National plan","X",null,null,0.09,8.9,55.6]
["Hungary","HUN",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,"2070-2110 and 2245-2290 MHz Non-Civil digital P-P links",null,3,null,"T/R 13-01 Annex C","X","X",null,null,20]
["Iceland","ICE",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,null,null,90,null,"T/R 13-01 Annex C",45,45,null,20,40,70,0]
["Ireland","IRL",0,"2025-2110 and 2200-2290","X",null,null,null,null,null," X",null,null,null,null,null,47,null,"T/R 13-01 Annex C"," X","X",null,1.5,24,66," 0"]
["Ireland","IRL",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X","X",null,null,null,null,12,21,null,"T/R 13-01 Annex C","x",null,null,6.71,30.92,64.77,0.15]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X","X",null,null,null,null,95,3,null,"T/R 13-01 Annex C",null,"x",null,3.28,52.12,238.26,0.15]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X","X",null,null,null,null,null,122,null,"T/R 13-01 Annex C",null,null,"x",0.49,67.06,238.26,0.15]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X",null,null,null,null,null,null,null,10,"T/R 13-01 Annex C","X",null,null,null,null,null,0.05,"stable"]
["Lithuania","LTU",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,"X",null,null,5,null,"T/R 13-01 Annex C",5]
["Luxembourg","LUX",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Latvia","LVA",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,null,null,3,null,"T/R 13-01 Annex C","X",null,null,5,null,41]
["Netherlands","NLD",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Norway","NOR",0,"2025-2110 and 2200-2290","X","X",null,null,null,null,null,null,null,null,"X",null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,null,"SAP/SAB"]
["Norway","NOR",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,null,"X",null,null,2,null,null,null,"x",null,17,19.7,22,null,null,null,"Offshore"]
["Portugal","PRT",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,"TCR, SAP/SAB",null,11,null,"T/R 13-01 Annex C","X",null,null,2,"40",193,0]
["Portugal","PRT",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,"TCR, SAP/SAB",null,2,null,"National plan",null,"X",null,20,"40",64,0]
["Russia","RUS",0,"2025-2110 and 2200-2290","X","X",null,null,null,null,"X",null,null,null,null,null,73,1,"T/R 13-01 Annex C","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Serbia","SRB",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defense systems"]
["Slovak Republic","SVK",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovenia","SVN",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Sweden","SWE",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Telia","TELIASON",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Italy","ITA",0,"2300-2400","X",null,null,null,"X",null,null,null,null,null,null,null,275,null,"national","X"]
["Austria","AUT",0,"3400-3600","X",null,null,null,null,"X","X",null,null,null,null,null,null,240,"ERC/REC 14-03","X",null,null,3,15,30]
["Bosnia and Herzegovina","BIH",0,"3400-3600","X",null,null,null,null,null,"X",null,"X",null,null,9,1,null,"ERC/REC 14-03 Annex B","X","X",null,null,2,null,null,null,null,"3400-3600 MHz: Only two channels are available for P-P links out of FWA systems. We still do not have active implemented FWA systems.\n3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Bosnia and Herzegovina","BIH",0,"3400-3600",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,null,null,"X","X",null,null,null,"+25",null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["switzerland","CHE",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ERC/REC 14-03"]
["Cyprus","CYP",0,"3400-3600","P.C.",null,null,null,null,null,null,null,null,null,null,null,null,null,"2008/411/EC"]
["Czech Republic","CZE",0,"3400-3600","X","X",null,null,"X","X",null,null,null,null,null,null,null,667,"ERC/REC 14-03",null,null,null,null,null,null,100,null,null,"P-MP, FWA planned"]
["Denmark","DNK",0,"3400-3600","X",null,null,null,null,null,null,null,null,null,null,null,null,29,"ERC/REC 14-03"]
["Denmark","DNK",0,"3400-3600",null,"X",null,null,null,null,null,null,null,null,null,null,null,null," ",null,null,null,null,null,null,null,null,null,"No info"]
["Estonia","EST",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,null,null,null,"No info"]
["Finland","FIN",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,540,"ERC/REC 14-03"]
["France","FRA",0,"3400-3600","X","X",null,null,"X","X","X",null,null,null,null,null,236,1135,"ERC/REC 14-03",236,null,null,2,"20<x>80",135,"-30"]
["Germany","GER",0,"3400-3600",null,"x",null,null,null,"x",null,null,null,null,null,null,null,392,"ERC/REC 14-03",null,"x"]
["Greece","GRC",0,"3400-3600",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC 14-03","-",null,null,null,null,null,"4 issued licenses"]
["Croatia","HRV",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,67,"ERC/REC 14-03",null,null,null,null,null,null,-30]
["Hungary","HUN",0,"3400-3600",null," ",null," ",null," ",null,null,null,null,null,null,null,null,"ERC/REC 14-03"]
["Hungary","HUN",0,"3400-3600",null,"X",null,"X",null,"X",null,null,null,null,null,null,null,383,"ECC/DEC/(07)02",null,null,null,null,null,null,"20"]
["Iceland","ICE",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,20,"ERC/REC 14-03",null,null,null,null,10]
["Ireland","IRL",0,"3400-3600"," X",null,null,null,null," X",null,null,null,null,null,null,null,120,"ERC/REC 14-03",null,null,null,null,null,null," 66"]
["Italy","ITA",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,null,null,null,"No info"]
["Lithuania","LTU",0,"3400-3600","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 14-03"]
["Lithuania","LTU",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,402,"ERC/REC 14-03",null,null,null,null,null,null,50,null,null,"Fixed and mobile P-MP (BWA)"]
["Luxembourg","LUX",0,"3400-3600",null,"X",null,null,null,"X","X",null,null,null,null,null,null,3,"Nat. freq. Plan",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,69,"ERC/REC 14-03",null,"X",null,null,10,null,50]
["Netherlands","NLD",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03"]
["Portugal","PRT",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,64,"ERC/REC 14-03","X",null,null,null,"20",null," BWA"]
["Russia","RUS",0,"3400-3600","X","X",null,null,null,"X","X",null,"X",null,null,null,2190,8033,"ERC/REC 14-03","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Serbia","SRB",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,51,"ERC/REC 14-03",null,null,null,null,null,null,50]
["Slovak Republic","SVK",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,198,"ERC/REC 14-03","X",null,null,null,null,null,10]
["Slovenia","SVN",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,"BWA",null,null,10,"ERC/REC 14-03",null,"X",null,5,30,70,400]
["Sweden","SWE",0,"3400-3600",null,"X",null,null,"X","X","X",null,"X",null,"X",null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,"Y","N",null,"IMT-?"]
["Telia","TELIASON",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03"]
["Norway","NOR",0,"3410-3600",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 14-03 Annex A"]
["Norway","NOR",0,"3410-3600","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Bosnia and Herzegovina","BIH",0,"3600-3800","X",null,null,null,null,null,null,null,"X",null,null,9,null,null,"ERC/REC 12-08",null,"X","X",null,null,null,null,null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Bosnia and Herzegovina","BIH",0,"3600-3800",null,"X",null,null,"X","X",null,null,null,null,null,null,null,65,null,null,null,"X",null,null,null,"+25"]
["Czech Republic","CZE",0,"3600-3800","X",null,null,null,"X",null,null,null,null,null,null,null,150,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,"X","DEC EC/411/EC"]
["Germany","GER",0,"3600-3800",null,"x",null,null,null,"x",null,null,null,null,null,null,null,0,"ERC/REC 14-03",null,"x"]
["Norway","NOR",0,"3600-3800",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-08"]
["Norway","NOR",0,"3600-3800","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Serbia","SRB",0,"3600-3800",null,"X",null,null,null,"X",null,null,null,null,null,null,null,1,"ERC/REC 12-08"]
["Slovenia","SVN",0,"3600-3800","X",null,null,null,"X",null,null,null,"X",null,null,null,2,null,"ERC/REC 12-08",null,null,"X",null,null,null,-100,null,"x","BWA"]
["Slovenia","SVN",0,"3600-3800","X",null,null,null,"X",null,null,null,"X",null,null,1,null,null,"ERC/REC 12-08",null,null,"X",10,45,90,-100,null,"x","BWA"]
["Slovenia","SVN",0,"3600-3800",null,"X",null,null,null,"X",null,null,null,null,"BWA",null,null,"planned","ERC/REC 12-08",null,"X",null,null,null,null,">400",null,null,"BWA"]
["Austria","AUT",0,"3600-4200","X",null,null,null,"X",null,"X",null,null,null,null,null,90,null,"ERC/REC 12-08",null,"X",null,13,50,100]
["switzerland","CHE",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ERC/REC 12-08"]
["Cyprus","CYP",0,"3600-4200","P.C. (3.6-3.8 GHz)",null,null,null,null,null,null,null,null,null,null,null,null,null,"2008/411/EC"]
["Denmark","DNK",0,"3600-4200","X",null,null,null,null,null,null,null,null,null,null,null,null,21,"ERC/REC 12-08"]
["Denmark","DNK",0,"3600-4200",null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No info"]
["Estonia","EST",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"No info"]
["Finland","FIN",0,"3600-4200","X",null,null,null,null,null,"X",null,"X",null,null,null,160,null,"ERC/REC 12-08",null,null,"X"]
["Finland","FIN",0,"3600-4200",null,null,null,null,null,null,null,null,"X",null,null,40,null,null,"National","Analog","Analog",null,null,null,null,null,null,null,"Will be phased out"]
["Finland","FIN",0,"3600-4200","X",null,null,null,null,null,null,null,"X",null,null,120,null,null,"ITU-R F.382","Analog","Analog",null,null,null,null,null,null,null,"Will be phased out"]
["France","FRA",0,"3600-4200","X",null,null,null,"X",null,"X",null,null,null,null,null,11,null,"ERC/REC 12-08",null,null,11,2,"20<x>80",135,"-20"]
["UK","GBR",0,"3600-4200","X",null,null,null,null,null,null,null,null,"X",null,40,null,null,"ERC/REC 12-08",null,"X","X"]
["Croatia","HRV",0,"3600-4200","X",null,null,null,null,null,null,null,"X",null,null,null,9,null,"ERC/REC 12-08",null,"X"]
["Croatia","HRV",0,"3600-4200","X",null,null,null,null,null,"X",null,null,null,null,1,70,null,null,null,null,"X",20.2,44.2,91.4,10]
["Hungary","HUN",0,"3600-4200","X"," ",null," ","X",null,null,null,null,null,null,null,20,null,"ERC/REC 12-08",null,null,"X",null,30,null,"25"]
["Hungary","HUN",0,"3600-4200"]
["Iceland","ICE",0,"3600-4200","X",null,null,null,"X",null,null,null,null,null,null,null,7,null,"ERC/REC 12-08",null,null,7,20,30,40,0]
["Ireland","IRL",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
["Italy","ITA",0,"3600-4200","X",null,null,null,"X",null,"X",null,null,null,null,null,77,null,"ERC/REC 12-08",null,null,"X",13.6,60,238,-5]
["Italy","ITA",0,"3600-4200","X",null,null,null,null,null,"X",null,"X",null,null,105,9,null,"ERC/REC 12-08",null,"X","X",17.46,88.5,238.26,-5]
["Italy","ITA",0,"3600-4200",null,"X",null,null,null,null,"X",null,"X",null,null,null,210,null,"ERC/REC 12-08",null,null,"X",13.6,67.34,238.26,-5]
["Lithuania","LTU",0,"3600-4200","X",null,null,null,"X",null,null,null,null,"X",null,null,30,null,"ERC/REC 12-08",null,null,30]
["Lithuania","LTU",0,"3600-4200",null,"X",null,null,null,"X",null,null,null,"X",null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"3600-3800 future for BWA"]
["Luxembourg","LUX",0,"3600-4200","X",null,null,null,"X",null,"X",null,"X",null,null,1,0,null,"Nat. freq. Plan",null,"X","X",null,"20-80",null,"N/A","NO","NO"]
["Latvia","LVA",0,"3600-4200",null,"X",null,null,null,"X",null,null,null,null,null,null,null,154,"ERC/REC 12-08",null,"X",null,null,10,null,50]
["Netherlands","NLD",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
["Portugal","PRT",0,"3600-4200",null,"X",null,null,null,"X",null,null,null,null,"VSAT (3.8-4.2 GHz)",null,null,null,"ERC/REC 12-08","X","X",null,null,"20",null,null,null,null,"BWA in 3.3 -3.6GHz and FSS in 3.8-4.2GHz"]
["Russia","RUS",0,"3600-4200","X","X",null,null,null,null,"X",null,"X",null,null,null,688,null,"ERC/REC 12-08","X","X","X",40,80,90]
["Russia","RUS",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.635 ITU-R"]
["Slovak Republic","SVK",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"N.A. FWA planned"]
["Sweden","SWE",0,"3600-4200",null,"X",null,null,"X","X","X",null,"X",null,"X",null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,"Y","N",null,"IMT-?"]
["Telia","TELIASON",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
["Bosnia and Herzegovina","BIH",0,"3800-4200","X",null,null,null,null,null,null,null,"X",null,null,11,3,null,"ERC/REC 12-08 Annex B",null,null,null,27,35,85,"+40"]
["Czech Republic","CZE",0,"3800-4200","X",null,null,null,"X",null,null,null,null,null,null,null,479,null,"ERC/REC 12-08"]
["Germany","GER",0,"3800-4200","x",null,null,null,"x",null,null,null,null,null,null,269,null,null,"ERC/REC 12-08",null,null,"x",14.4,42,64.8]
["Greece","GRC",0,"3800-4200","X",null,null,null,null,null,"X",null,null,null,null,null,163,null,"ERC/REC 12-08 Annex B",null,"X","X",5,55,101,"reduction"]
["Norway","NOR",0,"3800-4200",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-08"]
["Norway","NOR",0,"3800-4200","X",null,null,null,null,null,null,null,null,"X",null,null,2,null,null,null,"X",null,2.5,2.7,2.9,null,null,null,null,null,"Offshore"]
["Serbia","SRB",0,"3800-4200","X",null,null,null,null,null,"X",null,null,null,null,null,3,null,"ITU-R F.382-8",null,null,"X",72.09,74.02,77.89]
["Slovenia","SVN",0,"3800-4200","X",null,null,null,"X",null,null,null,"X",null,null,null,18,null,"ERC/REC 12-08",null,null,"X",30,60,90,null,"X*",null,"congested in backbone directions"]
["Slovenia","SVN",0,"3800-4200","X",null,null,null,"X",null,null,null,"X",null,null,18,null,null,"ERC/REC 12-08",null,null,"X",10,30,90,null,"X*",null,"congested in backbone directions"]
["Austria","AUT",0,"4400-5000","X",null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Austria","AUT",0,"4400-5000"]
["switzerland","CHE",0,"4400-5000",null,null,null,null,null,null,null,null,null,null,"No civil FS use"]
["switzerland","CHE",0,"4400-5000"]
["Cyprus","CYP",0,"4400-5000",null,null,null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X"]
["Cyprus","CYP",0,"4400-5000"]
["Czech Republic","CZE",0,"4400-5000",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,null,null,null,null,null,null,null,null,null,null,"civil/MD sharing"]
["Czech Republic","CZE",0,"4400-5000"]
["Hungary","HUN",0,"4400-5000","X",null,null,null,"X","X",null,null,null,null,"Harmonized NATO band type 1. Land military systems, Tactical Radio Relay",null,140,null,null,"X","X","X",null,null,null,null,null,null,"non-civil usage"]
["Hungary","HUN",0,"4400-5000"]
["Latvia","LVA",0,"4400-5000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band"]
["Portugal","PRT",0,"4400-5000",null,null,null,null,null,null,null,null,null,"X","Military"]
["Portugal","PRT",0,"4400-5000"]
["Russia","RUS",0,"4400-5000","X","X",null,null,null,null,"X",null,"X",null,null,null,344,null,"F.382 ITU-R","X","X","X",40,80,90]
["Serbia","SRB",0,"4400-5000",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["Serbia","SRB",0,"4400-5000"]
["Norway","NOR",0,"5725-5795 and 5815-5850",null,null,null,"X",null,null,null,null,null,"X",null,null,null,null,"National plan"]
["Bosnia and Herzegovina","BIH",0,"5850-5925"]
["switzerland","CHE",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast"]
["Cyprus","CYP",0,"5850-5925","X",null,null,null,null,null,null,null,"X",null,null,2,null,null,null,null,"X"," ","PORTABLE"]
["Czech Republic","CZE",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,null,null,null,null,null,null,null,null,null,null,"civil/MD sharing"]
["Denmark","DNK",0,"5850-5925"]
["Estonia","EST",0,"5850-5925"]
["Finland","FIN",0,"5850-5925"]
["France","FRA",0,"5850-5925"]
["Greece","GRC",0,"5850-5925"]
["Croatia","HRV",0,"5850-5925"]
["Hungary","HUN",0,"5850-5925","X",null,null,null,"X","X","X",null,null,null,"Non-Civil BFWA systems",null,null,null,"ECC/DEC/(06)04"]
["Hungary","HUN",0,"5850-5925","X",null,null,null,"X"]
["Iceland","ICE",0,"5850-5925"]
["Ireland","IRL",0,"5850-5925"]
["Italy","ITA",0,"5850-5925","X",null,null,null,"X",null,null,null,"X",null,null,71,null,null,"national",null,null,"x",20,50,238,1,"yes"]
["Italy","ITA",0,"5850-5925",null,"X",null,null,null,null,"X",null,"X",null,null,116,null,null,"national",null,"x",null,9.4700000000000006,61.58,121.23,1,"yes"]
["Lithuania","LTU",0,"5850-5925","X",null,null,null,"X",null,"X",null,null,null,null,null,29,null,null,29]
["Lithuania","LTU",0,"5850-5925",null,null,null,null,null,"X",null,null,null,"X",null,null,null,null,"5/10/20MHz",null,null,null,null,null,null,null,null,null,"5850-5875, 5905-5925 future P-MP"]
["Luxembourg","LUX",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Latvia","LVA",0,"5850-5925",null,"X",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Planning BFWA  within 5725-5875 MHz band. BFWA  5905-5925 MHz"]
["Netherlands","NLD",0,"5850-5925"]
["Netherlands","NLD",0,"5850-5925"]
["Portugal","PRT",0,"5850-5925",null,null,null,"X",null,null,null,null,null,null,"ISM, SRD"]
["Russia","RUS",0,"5850-5925","X","X",null,null,null,"X","X",null,"X",null,null,null,1350,623,null,"X","X","X",30,70,90]
["Serbia","SRB",0,"5850-5925",null,null,null,"X",null,null,null,null,null,null,"X",null,null,null,"ERC/REC 70-03",null,null,null,null,null,null,null,null,null,"SRD"]
["Slovak Republic","SVK",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovenia","SVN",0,"5850-5925"]
["Sweden","SWE",0,"5850-5925"]
["Telia","TELIASON",0,"5850-5925"]
["Latvia","LVA",0,"5925-6245 and  6425-7125","X",null,null,null,"X",null,null,null,null,null,null,null,39,null,"ERC/REC 14-01 ",null,null,"X",22,30,36,100]
["Latvia","LVA",0,"5925-6245 and  6425-7125","X",null,null,null,"X",null,null,null,null,null,null,null,17,null,"ERC/REC 14-02",null,null,"X",28,35,52,100]
["UK","GBR",0,"5925-6425","X",null,null,null,null,null,null,null,null,"X",null,220,null,null,"ERC/REC 14-01 ",null,null,"X"]
["Germany","GER",0,"5925-6425","x",null,null,null,"x",null,null,null,null,null,null,994,null,null,"ERC/REC 14-01",null,null,"x",11.1,40,67.3]
["Slovak Republic","SVK",0,"5925-6425","X",null,null,null,"X",null,"X",null,null,null,null,null,81,null,"ERC/REC 14-01 ",null,null,"X",8.5,20,54,25]
["Slovenia","SVN",0,"5925–6425 ","X",null,null,null,"X",null,"X",null,null,null,null,null,6,null,"ERC/REC 14-01 ",null,null,"X",12,50,75,30]
["Slovenia","SVN",0,"5925–6425 ","X",null,null,null,"X",null,null,null,"X",null,null,null,2,null,"ERC/REC 14-01 ",null,null,null,20,55,65,50]
["Slovenia","SVN",0,"5925–6425 ",null,"X",null,null,"X",null,null,null,"X",null,null,null,4,null,"ERC/REC 14-01 ",null,null,null,5,25,65,0,"x"]
["Austria","AUT",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,336,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",5,45,70]
["Bosnia and Herzegovina","BIH",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,5,302,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",8,60,134,null,"X"]
["Switzerland","CHE",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,60,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,60,30,39.700000000000003,81.7,"growth"]
["Cyprus","CYP",0,"5925-7125","X",null,null,null,null,null,"X",null,"X",null,null,17,27,null,"ERC/REC 14-01 and ERC/REC 14-02","X","X"," ",7.19,null,53]
["Czech Republic","CZE",0,"5925-7125","X",null,null,null,"X",null,null,null,null,null,null,null,1642,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Denmark","DNK",0,"5925-7125","X",null,null,null,null,null,null,null,null,null,null,null,22,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Estonia","EST",0,"5925-7125",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Finland","FIN",0,"5925-7125","X",null,null,null,null,null,"X",null,"X",null,null,null,160,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",10,30,63,0.8]
["France","FRA",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,3491,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,3491,0.5,"20-80",105,"+ 5 % ","X"]
["Greece","GRC",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,638,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",8,45,102,"stable"]
["Croatia","HRV",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,98,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",10.7,34.1,70.8,20,"x"]
["Hungary","HUN",0,"5925-7125","X",null,null,null,"X",null,null,null,null,null,null,null,299,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,null,null,null,null,0.1]
["Iceland","ICE",0,"5925-7125","X",null,null,null,"X",null,null,null,"X",null,null,6,16,null,"ERC/REC 14-01 and ERC/REC 14-02",3,null,15,10,30,50,0]
["Ireland","IRL",0,"5925-7125"," X",null,null,null,null,null," X",null,null,null,null,2,356,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null," X",8,40,90," 28"]
["Italy","ITA",0,"5925-7125","X",null,null,null,"X",null,"X",null,"X",null,null,102,808,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",6.32,44,83,0.15,"almost"]
["Lithuania","LTU",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,137,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Lithuania","LTU",0,"5925-7125",null,null,null,null,null,"X",null,null,null,"X",null,null,null,null,"5/10/20MHz",null,null,null,null,null,null,null,null,null,"5925-6425 future for P-MP"]
["Luxembourg","LUX",0,"5925-7125","X",null,null,null,"X",null,"X",null,"X",null,null,10,2,null,"ERC/REC 14-01 and ERC/REC 14-02 and national plan",null,"X","X",3.4,"20-80",63,"N/A","NO","NO"]
["Netherlands","NLD",0,"5925-7125","X",null,null,null,null,null,null,null,null,"X",null,null,51,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",21.41,31.11,49.3,20]
["Norway","NOR",0,"5925-7125","X","X",null,null,null,null,null,null,null,"X",null,null,146,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",2.8,37.5,123]
["Portugal","PRT",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,"VSAT, SRD",2,8,null,"ERC/REC 14-01 ",null,"X","X",40,40,88,50]
["Portugal","PRT",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,"VSAT, SRD",null,59,null,"ERC/REC 14-02",null,"X","X",15,40,84,10]
["Russia","RUS",0,"5925-7125","X","X",null,null,"X","X","X",null,"X",null,null,null,3411,1942,"ERC/REC 14-01 and ERC/REC 14-02","X","X","X",30,55,65]
["Russia","RUS",0,"5925-7125",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.383 ITU-R"]
["Serbia","SRB",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,205,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",17,45,79,30]
["Sweden","SWE",0,"5925-7125","X",null,null,null,"X",null,null,null,null,null,null,null,952,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,null,null,null,null,null,"Y"]
["Telia","TELIASON",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,19,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,19,6,null,40,null,"X"]
["UK","GBR",0,"6425-7125","X",null,null,null,null,null,null,null,null,"X",null,330,null,null,"ERC/REC 14-02",null,"X","X"]
["Germany","GER",0,"6425-7125","x",null,null,null,"x",null,null,null,null,null,null,2565,null,null,"ERC/REC 14-02",null,null,"x",4.3,30,103.9]
["Slovenia","SVN",0,"6425-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,14,null,"ERC/REC 14-02",null,null,"X",20,40,50,50]
["Slovak Republic","SVK",0,"6430-7110","X",null,null,null,"X",null,"X",null,null,null,null,null,2,null,"ERC/REC 14-02",null,null,"X",44,49,54,"0-100 ",null,null,"expected growth"]
["Germany","GER",0,"7125-7425","x",null,null,null,"x",null,null,null,null,null,null,917,null,null,"ECC REC (02)06",null,"x",null,4.2,28,89.9]
["Norway","NOR",0,"7125-7425","X",null,null,null,null,null,null,null,null,"X",null,null,135,null,null,null,null,"X",4.2,35.5,96]
["Slovak Republic","SVK",0,"7125-7425","X",null,null,null,"X",null,"X",null,null,null,null,null,30,null,"ECC REC (02)06",null,null,"X",17,25,44.5,50]
["Slovak Republic","SVK",0,"7125-7425","X",null,null,null,"X",null,"X",null,null,null,null,null,14,null,"ITU-R F.385, DS 161MHz","X","X",null,7,25,58,-100,null,"x","no new links"]
["Slovenia","SVN",0,"7125-7425","X",null,null,null,"X",null,"X",null,null,null,null,null,23,null,"ECC REC (02)06",null,null,"X",10,25,45,10,"x"]
["Slovenia","SVN",0,"7125-7425","X",null,null,null,"X",null,null,null,"X",null,null,null,43,null,"ECC REC (02)06",null,null,"X",5,25,65,5,"x"]
["Serbia","SRB",0,"7125-7725","X",null,null,null,null,null,"X",null,null,null,null,null,138,null,"ITU-R F.385-9 base","X","X","X",11.67,37.979999999999997,104.2,150]
["Telia","TELIASON",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,22,null,"ECC REC (02)06",null,22,null,15,null,42,null,"X",null,null,"NEC 770"]
["Telia","TELIASON",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,128,null,null,74,54,null,7,null,80,null,"X",null,null,"Eric sson ML"]
["Austria","AUT",0,"7125-7750","X",null,null,null,"X",null,null,null,null,null,null,null,570,null,"ECC REC (02)06",null,"X","X",1,40,78]
["Bosnia and Herzegovina","BIH",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,113,null,"ECC REC (02)06",null,"X","X",4,40,90,null,"X"]
["Bosnia and Herzegovina","BIH",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,10,62,null,"ITU-R F.385",null,"X","X"]
["Croatia","HRV",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,171,null,"Bands 7125 - 7425 and 7425 - 7725 with diff. ch. arrangements",null,"X","X",3.8,37.700000000000003,91.4,30,"x"]
["Czech Republic","CZE",0,"7125-7750","X",null,null,null,"X",null,null,null,null,null,null,null,1050,null,"ECC REC (02)06",null,null,null,null,null,null,null,null,"x","civil/MD sharing"]
["Cyprus","CYP",0,"7125-7750","X",null,null,null,null,null,"X",null,"x",null,null,8,48,null,"ECC REC (02)06","X","X"," ",0.49,null,63.77]
["Denmark","DNK",0,"7125-7750","X",null,null,null,null,null,null,null,null,null,null,null,225,null,"ECC REC (02)06",null,null,null,20]
["Estonia","EST",0,"7125-7750",null,null,null,null,null,null,null,null,null,null,null,null,62,null,"ECC REC (02)06",null,62,null,17,35,81]
["Finland","FIN",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,130,null,"ITU-R F.385",null,"X","X",13,36,65,0.05]
["Finland","FIN",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,330,null,"National (ITU-R F.385 mod.)",null,"X","X",2,27,70,0.1]
["France","FRA",0,"7125-7750",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["Hungary","HUN",0,"7125-7750","X",null,null,null,"X",null,null,null,"X",null,"7125-7250 MHz Non-Civil P-P links;  7125-7425 MHz Emergency Services\n7425-7725 MHz Civil P-P links 7725-7750 MHz Civil broadcasting infrastructure",null,171,null,"ECC REC (02)06","X","X","X",null,20]
["Hungary","HUN",0,"7125-7750",null,null,null,null,null,null,null,null,null,null,"7250-7750 MHz Satellite Systems downlink (military); Harmonized NATO band type 1."]
["Iceland","ICE",0,"7125-7750","X",null,null,null,"X",null,null,null,"X",null,null,23,65,null,"ECC REC (02)06",32,28,28,10,30,60,0]
["Ireland","IRL",0,"7125-7750"," X",null,null,null,null,null," X",null,null,null,null,1,279,null,"ECC REC (02)06"," X","X","X",7,36,76," 57"]
["Lithuania","LTU",0,"7125-7750","X",null,null,null,"X",null,null,null,null,null,null,null,197,null,"ECC REC (02)06"]
["Luxembourg","LUX",0,"7125-7750","X",null,null,null,"X",null,"X",null,"X",null,null,0,26,null,"ECC REC (02)06",null,"X","X",7.9,"20-80",55.9,"N/A","NO","NO"]
["Netherlands","NLD",0,"7125-7750","X",null,null,null,null,null,null,null,null,"X",null,null,113,null,"ECC REC (02)06","X","X","X",10.4,27.7,55.6,20]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS, Military (7.25-7.3 GHz)",null,7,null,"7 LOW: ITU-R F.385","X",null,null,15,"30",53,0]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS, Military (7.25-7.3 GHz)",null,287,null,"7 LOW: ECC REC (02)06","X","X","X",6,"30",63,10]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,40,null,"7 HIGH: ITU-R F.385","X","X",null,3,"22",71,-50]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,30,null,"7 HIGH: ECC REC (02)06","X","X","X",15,"30",78,50]
["Russia","RUS",0,"7125-7750","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",10495,null,"F.385 ITU-R","X","X","X",30,55,65]
["Switzerland","CHE",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,null,null,171,null,"ECC REC (02)06",70,81,20,20,30.2,99.5,"growth"]
["Latvia","LVA",0,"7125-7800","X",null,null,null,"X",null,null,null,null,null,null,null,104,null,"ITU-R F.385",null,null,"X",14,35,54,50,null,null,"Military band 7250-7331 MHz"]
["Slovenia","SVN",0,"7425–7725","X",null,null,null,"X",null,"X",null,null,null,null,null,26,null,"ECC REC (02)06",null,null,"X",10,25,45,20]
["Slovenia","SVN",0,"7425–7725","X",null,null,null,"X",null,null,null,"X",null,null,null,5,null,"ECC REC (02)06",null,null,"X",3,25,60,30]
["Germany","GER",0,"7425-7725","x",null,null,null,"x",null,null,null,null,null,null,3157,null,null,"ECC REC (02)06",null,null,"x",5.5,26,71.099999999999994,null,"x"]
["Norway","NOR",0,"7425-7725","X",null,null,null,null,null,null,null,null,"X",null,null,446,null,null,null,null,"X",1.2,32.299999999999997,113]
["Slovak Republic","SVK",0,"7425-7725","X",null,null,null,"X",null,"X",null,null,null,null,null,70,null,"ITU-R F.385-9, DS 161MHz","X","X",null,5,25,55,10]
["Sweden","SWE",0,"7425-7725","X",null,null,null,"X",null,null,null,null,null,null,null,1421,null,null,null,"X",null,null,null,null,null,"Y"]
["Greece","GRC",0,"7425-7725","X",null,null,null,null,null,"X",null,null,null,null,null,1222,null,"ECC REC (02)06 Annex1","X","X","X",1,31,98,0.1]
["UK","GBR",0,"7425-7900","X",null,null,null,null,null,null,null,null,"X",null,940,null,null,"ITU-R F.385-9","X","X","X"]
["Slovak Republic","SVK",0,"7700-8300","X",null,null,null,"X",null,"X",null,null,null,null,null,35,null,"ITU-R F.386-4, Annex 1",null,null,"X",8,30,58,-100,null,"x","no new links"]
["Slovenia","SVN",0,"7725–8275","X",null,null,null,"X",null,null,null,"X",null,null,6,42,null,"ITU-R F 386-8 An6  (29.65 MHz, DS 311.32 MHz)",null,null,"X",15,35,60,5,"x*",null,"congested in backbone directions"]
["Bosnia and Herzegovina","BIH",0,"7725–8275","X",null,null,null,null,null,"X",null,"X",null,null,34,143,null,"ITU-R F.386, Annex 6",null,"X","X",4,38,83,null,"X",null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Serbia","SRB",0,"7725–8275","X",null,null,null,null,null,"X",null,null,null,null,null,8,null,"ITU-R F.386-8 annex 6",null,"X","X",9.44,35.68,70.27,300]
["Greece","GRC",0,"7725–8275","X",null,null,null,null,null,"X",null,null,null,null,null,1157,null,"ITU-R F. 386-6 Annex 1",null,"X","X",2,40,150,0.1]
["Telia","TELIASON",0,"7750-7900"]
["Austria","AUT",0,"7750-7900",null,null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Croatia","HRV",0,"7750-7900","X",null,null,null,null,null,"X",null,"X",null,null,null,146,null,"Band 7725 - 8275",null,null,"X",21.1,50.3,91.4,null,"x"]
["Czech Republic","CZE",0,"7750-7900",null,null,null,null,null,null,null,null,null,null,"MD"]
["Cyprus","CYP",0,"7750-7900",null,null,null," "]
["Denmark","DNK",0,"7750-7900"]
["Estonia","EST",0,"7750-7900"]
["Finland","FIN",0,"7750-7900","X",null,null,null,null,null,null,null,"X",null,null,45,7,null,"National  ",null,"X"]
["France","FRA",0,"7750-7900"]
["Hungary","HUN",0,"7750-7900","X",null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,40,null,0.15]
["Iceland","ICE",0,"7750-7900"]
["Ireland","IRL",0,"7750-7900"]
["Italy","ITA",0,"7750-7900"]
["Lithuania","LTU",0,"7750-7900","X",null,null,null,"X",null,null,null,null,null,null,null,0,null,"local"]
["Luxembourg","LUX",0,"7750-7900","X",null,null,null,"X",null,"X",null,"X",null,null,0,0,null,"Nat. freq. plan",null,"X","X",null,null,null,"N/A","NO","NO"]
["Netherlands","NLD",0,"7750-7900"]
["Portugal","PRT",0,"7750-7900","X",null,null,null,"X",null,"X",null,null,null,null,null,26,null,"8 LOW: ITU-R F.386",null,"X","X",2,"30",75,50]
["Russia","RUS",0,"7750-7900","No","No"]
["Switzerland","CHE",0,"7750-7900",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast"]
["Latvia","LVA",0,"7800-7900",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band 7850-7900 MHz"]
["Norway","NOR",0,"7900-8200",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ECC REC (02)06"]
["Telia","TELIASON",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,8,null,"ECC REC (02)06",null,8,null,16,null,68,null,"X",null,null,"NEC 770"]
["Telia","TELIASON",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,37,null,null,null,11,26,13,null,68,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,1,null,null,null,null,1,null,34,null,"++",null,null,null,"Ericsson TN"]
["Austria","AUT",0,"7900-8500","X",null,null,null,"X",null,"X",null,"X",null,null,null,73,null,"ECC REC (02)06",null,"X","X",1,35,60]
["Croatia","HRV",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,14,null,"Band 8275 - 8500",null,"X",null,7.5,20.100000000000001,31.4]
["Czech Republic","CZE",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"ECC REC (02)06"]
["Cyprus","CYP",0,"7900-8500","X",null,null,null,null,null,null,null,"X",null,null,14,null,null,"ECC REC (02)06","X","X"," ",8.2899999999999991,null,40.020000000000003]
["Denmark","DNK",0,"7900-8500","X",null,null,null,null,null,null,null,null,null,null,null,4," ","ECC REC (02)06",null,null,null,20]
["Estonia","EST",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,45,null,"ECC REC (02)06",null,45,null,15,35,40,"+20"]
["Finland","FIN",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["France","FRA",0,"7900-8500","X",null,null,null,"X",null,"X",null,null,null,null,null,2529,null,"ECC REC (02)06",1322,947,260,0.04,"15<x>60",105,"- 10 %"]
["France","FRA",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UIT-RF-386-4"]
["Hungary","HUN",0,"7900-8500","X",null,null,null,null,null,null,null,null,null,"7900-8400 MHz Satellite Systems uplink (military); Harmonized NATO band type 1.",null,null,null,"ECC REC (02)06"]
["Hungary","HUN",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,3,null,null,"X","X",null,null,20]
["Iceland","ICE",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["Ireland","IRL",0,"7900-8500"," X",null,null,null,null,null," X",null,null,null,null,null,315,null,"ECC REC (02)06"," X","X","X",5,36,81," 48"]
["Italy","ITA",0,"7900-8500","X",null,null,null,"X",null,"X",null,null,null,null,null,2231,null,"national",null,"X","X",null,30,null,0.1,"almost"]
["Italy","ITA",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,5,null,"national",null,null,"X"]
["Latvia","LVA",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,152,null,"ECC REC (02)06",null,null,"X",12,35,50,50,null,null,"Military band 7975-8024 MHz"]
["Lithuania","LTU",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,116,null,"ECC REC (02)06"]
["Luxembourg","LUX",0,"7900-8500","X",null,null,null,"X",null,"X",null,"X",null,null,4,6,null,"ECC REC (02)06",null,"X","X",5.0999999999999996,"20-80",62,"N/A","NO","NO"]
["Netherlands","NLD",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["Portugal","PRT",0,"7900-8500","X",null,null,null,"X",null,null,null,"X",null,"FSS, EESS, Military (7.975-8.025 GHz)",7,9,null,"8 HIGH: ITU-R F.386","X",null,null,6,"40",88,-100]
["Russia","RUS",0,"7900-8500","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",4584,null,"F.386 ITU-R","X","X","X",30,55,65]
["Sweden","SWE",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,494,null,"ECC REC (02)06",null,"X",null,null,null,null,"Y","N"]
["Switzerland","CHE",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ECC REC (02)06"]
["Bosnia and Herzegovina","BIH",0,"8275-8500","X",null,null,null,null,null,"X",null,null,null,null,null,17,null,"ITU-R F.386, Annex 2",null,"X",null,7,25,65,null,"X"]
["Serbia","SRB",0,"8275-8500","X",null,null,null,null,null,"X",null,null,null,null,null,10,null,"ITU-R F.386-8 annex 2",null,"X","X",21,53.77,98.71,300]
["Slovenia","SVN",0,"8275-8500","X",null,null,null,"X",null,"X",null,null,null,null,null,14,null,"ITU-R F.386-8 An2 (28 MHz , DS 119 MHz, 14 MHz, DS 126 MHz)",null,"X",null,20,35,70,30,"x*",null,"congested in backbone directions"]
["Greece","GRC",0,"8275-8500 ","X",null,null,null,null,null,"X",null,null,null,null,null,170,null,"ITU-R F. 386-6 Annex 3","X","X",null,1.8,47,120,"stable"]
["Austria","AUT",0,"10000-10680","X",null,null,null,"X",null,"X",null,null,null,null,null,158,null,"ERC/REC 12-05",null,"x",null,1,30,80]
["Bosnia and Herzegovina","BIH",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,103,null,null,"ERC/REC 12-05","X","X",null,1,27,80,"+15",null,null,"10000-10680 MHz: Shared band between P-P links and FWA. We still do not have active implemented FWA systems."]
["Bosnia and Herzegovina","BIH",0,"10000-10680",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC 12-05 Annex A"]
["Switzerland","CHE",0,"10000-10680","X",null,null,null,"X",null,"X",null,null,null,null,null,64,null,"ERC/REC 12-05",18,46,null,15,18.3,48.5,"growth"]
["Cyprus","CYP",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,56,null,null,"ERC/REC 12-05","X","X"," ",0.53,null,70]
["Czech Republic","CZE",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"ERC/REC 12-05"]
["Czech Republic","CZE",0,"10000-10680","X",null,null,"X","X",null,null,null,null,null,null,null,21]
["Denmark","DNK",0,"10000-10680","X",null,null,null,null,null,null,null,null,null,null,null,null,47,"ERC/REC 12-05"]
["Denmark","DNK",0,"10000-10680",null,"X",null,null,null,null,null,null,null,null,null,null,"No info"]
["Denmark","DNK",0,"10000-10680","X",null,null,null,null,null,null,null,null,null,null,null,1]
["Estonia","EST",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Finland","FIN",0,"10000-10680","X",null,null,null,null,"X",null,null,null,null,null,null,null,11,"ERC/REC 12-05",null,"X"]
["France","FRA",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["UK","GBR",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Greece","GRC",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,107,null,null,"national plan",null,null,null,1.2,19,75]
["Croatia","HRV",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,2,null,null,"ERC/REC 12-05",null,"x"]
["Croatia","HRV",0,"10000-10680",null,"X",null,null,null,"X"]
["Hungary","HUN",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,93,null,null,"ERC/REC 12-05",null,null,null,null,40]
["Iceland","ICE",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Ireland","IRL",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Ireland","IRL",0,"10000-10680"," X",null,null,null," X",null,null,null,null,null,null,null,null,30,"National Legislation: S.I. 79 of 2003\nNational Legislation: S.I. 530 of 2003 European Legislation: Decision 2008/411/EC ",null,null,null,null,null,null," 75"]
["Italy","ITA",0,"10000-10680","X",null,null,null,null,null,"X",null,"X",null,null,{"$f":"935+529+446","v":1910},34,null,"ERC/REC 12-05",null,"X",null,3,25,84,1,"yes"]
["Italy","ITA",0,"10000-10680","X",null,null,null,null,null,"X",null,"X",null,null,{"$f":"236+24","v":260},80,null,"ERC/REC 12-05",null,null,"x",5.5,35,50,1,"yes"]
["Luxembourg","LUX",0,"10000-10680","X",null,null,null,"X",null,"X",null,"X",null,null,2,0,null,"ERC/REC 12-05",null,"X","X",32,"10-50",62,"N/A","NO","NO"]
["Luxembourg","LUX",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"10000-10680","X",null,null,null,"X",null,null,null,null,null,null,null,105,null,"ERC/REC 12-05","X",null,null,null,null,null,-80,null,null,"10300-10500 MHz"]
["Latvia","LVA",0,"10000-10680",null,"X",null,null,null,"X",null,null,null,null,null,null,null,66,"ERC/REC 12-05 and ERC/REC 13-04",null,"X",null,null,10,null,50]
["Netherlands","NLD",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Norway","NOR",0,"10000-10680",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-05"]
["Portugal","PRT",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,"AM, SAP/SAB, SRD",null,null,null,"ERC/REC 12-05"]
["Russia","RUS",0,"10000-10680","X","X",null,null,null,"X","X",null,"X",null,null,"less than 1%",247,1490,"ERC/REC 12-05","X","X","X",15,30,40]
["Serbia","SRB",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,76,3,null,"national plan","X",null,null,0.7,24.72,114.99,20]
["Slovak Republic","SVK",0,"10000-10680",null,"X",null,null,null,"X",null,null,null,null,null,null,null,110,"ERC/REC 12-05","x","x",null,null,null,null,10]
["Slovenia","SVN",0,"10000-10680","X",null,null,null,"X",null,null,null,"X",null,null,53,null,null,"ERC/REC 12-05",null,"x","x",2,25,65,-100,null,"x","BWA when SAP/SAB P to P video links analogue cease operation"]
["Slovenia","SVN",0,"10000-10680","X",null,null,null,"X",null,null,null,"X",null,null,null,8,null,"ERC/REC 12-05",null,"x","x",2,25,62,-100,null,"x","BWA when SAP/SAB P to P video links analogue cease operation"]
["Sweden","SWE",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05\nNew ITU-R Rec under dev.",null,null,null,null,null,null,"Y","N",null,"Blockassignment?"]
["Telia","TELIASON",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Lithuania","LTU",0,"10150-10300 and 10500-10650","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-05"]
["Lithuania","LTU",0,"10150-10300 and 10500-10650",null,"X",null,null,null,"X",null,null,null,null,null,null,null,6,"ERC/REC 12-05",null,null,null,null,null,null,100]
["Lithuania","LTU",0,"10300-10500","X",null,null,null,"X",null,"X",null,null,null,null,null,420,null,"ERC/REC 12-05",420]
["Austria","AUT",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,21,null,"ERC/REC 12-06"]
["Bosnia and Herzegovina","BIH",0,"10700-11700","X",null,null,null,null,null,"X",null,"X",null,null,37,38,null,"ERC/REC 12-06","X","X",null,1,25,64,"+15",null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Switzerland","CHE",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,80,null,"ERC/REC 12-06",null,null,80,10,14.9,34.9,"growth",null,null,"heavily used by FSS"]
["Cyprus","CYP",0,"10700-11700","X",null,null,null,null,null,"X",null,"X",null,null,3,30,null,"ERC/REC 12-06",null,"X"," ",2.0099999999999998,null,34.130000000000003]
["Czech Republic","CZE",0,"10700-11700","X",null,null,null,null,"X",null,null,null,null,null,null,null,1845,"ERC/REC 12-06",null,null,null,null,null,null,20]
["Denmark","DNK",0,"10700-11700","X",null,null,null,null,null,null,null,null,null,null,null,null,1,"ERC/REC 12-06"]
["Estonia","EST",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Finland","FIN",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["France","FRA",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,524,null,"ERC/REC 12-06",null,null,524,1.5,"15<x>50",46,"+ 26 %"]
["Greece","GRC",0,"10700-11700","X",null,null,null,null,null,"X",null,null,null,null,null,785,null,"ERC/REC 12-06",null,null,"X",1.7,19,63,0.3]
["Croatia","HRV",0,"10700-11700","X",null,null,null,null,null,"X",null,null,null,null,null,8,null,"ERC/REC 12-06",null,null,"x",7.5,20.2,29.8]
["Hungary","HUN",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Hungary","HUN",0,"10700-11700","X",null,null,null,"X",null,null,null,null,null,null,null,186,null,"ERC/DEC/(00)08",null,null,"X",null,14]
["Iceland","ICE",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Ireland","IRL",0,"10700-11700"," X",null,null,null,null,null,"X",null,null,null,null,null,648,null,"ERC/REC 12-06",null,"X","X",1.5,24,56," 39"]
["Ireland","IRL",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null," National Legislation: S.I. 370 of 2009"]
["Italy","ITA",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,3110,null,"ERC/REC 12-06",null,"X","X",null,18,null,0.15,"yes"]
["Italy","ITA",0,"10700-11700","X",null,null,null,null,null,"X",null,"X",null,null,58,99,null,"ERC/REC 12-06",null,"X","X",3,22,60,0.15,"yes"]
["Lithuania","LTU",0,"10700-11700","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 12-06"]
["Luxembourg","LUX",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Latvia","LVA",0,"10700-11700","X",null,null,null,null,null,null,null,"X",null,null,38,null,null,"ITU-R F.387",null,null,null,0.3,10,32,-50,null,null,"Analog fixed links"]
["Netherlands","NLD",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Norway","NOR",0,"10700-11700",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ITU rec F.387-10"]
["Norway","NOR",0,"10700-11700","X",null,null,null,null,null,null,null,null,"X",null,null,234,null,null,null,null,"x",0.5,23,66.5]
["Portugal","PRT",0,"10700-11700","X",null,null,null,"X",null,"X",null,"X",null,"FSS, VSAT, SNG, SIT, AES, Euteltracs",null,117,null,"ERC/REC 12-06",null,"X","X",2,"20",41,5]
["Russia","RUS",0,"10700-11700","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",1207,null,"ERC/REC 12-06","X","X","X",15,30,40]
["Russia","RUS",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.387 ITU-R"]
["Serbia","SRB",0,"10700-11700","X",null,null,null,null,null,"X",null,null,null,null,null,48,null,"ERC/REC 12-06",null,null,"X",7.13,15.72,37.700000000000003,300]
["Slovak Republic","SVK",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,0,null,"ERC/REC 12-06",null,null,"x",null,null,null,100,null,null,"operation expected"]
["Slovenia","SVN",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,13,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",7,40,46,50,null,null,null,"In accordance with CEPT and ITU limitations"]
["Slovenia","SVN",0,"10700-11700","X",null,null,null,"X",null,null,null,"X",null,null,3,null,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",35,40,46,5,null,null,null,"In accordance with CEPT and ITU limitations"]
["Slovenia","SVN",0,"10700-11700","X",null,null,null,"X",null,null,null,"X",null,null,null,3,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",33,40,47,5,null,null,null,"In accordance with CEPT and ITU limitations"]
["Sweden","SWE",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,7,1,null,"ERC/REC 12-06"]
["Telia","TELIASON",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Austria","AUT",0,"11700-12500"]
["Bosnia and Herzegovina","BIH",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/DEC(00)08"]
["Bosnia and Herzegovina","BIH",0,"11700-12500",null,"X",null,null,null,null,null,null,"X",null,null,null,null,16,null,null,null,null,null,null,null,"+10"]
["Switzerland","CHE",0,"11700-12500"]
["Cyprus","CYP",0,"11700-12500","X",null,null,null,null,null,null,null,"X",null,null,10,null,null,null,null,"X"," ",2.75,null,30.18]
["Czech Republic","CZE",0,"11700-12500","X",null,null,null,"X",null,null,null,null,null,null,31,null,null,null,null,null,null,null,null,null,10]
["Denmark","DNK",0,"11700-12500"]
["Estonia","EST",0,"11700-12500"]
["Finland","FIN",0,"11700-12500"]
["France","FRA",0,"11700-12500"]
["UK","GBR",0,"11700-12500"]
["Greece","GRC",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Croatia","HRV",0,"11700-12500"]
["Hungary","HUN",0,"11700-12500",null,null,null,"X",null,null,null,null,"X",null,null,null,null,144,null,null,null,null,null,null,null,null,"x"]
["Iceland","ICE",0,"11700-12500"]
["Ireland","IRL",0,"11700-12500"]
["Italy","ITA",0,"11700-12500","X",null,null,null,null,null,"X",null,null,null,null,22,1,null,null,null,"x",null,1.97,27.6,62.94]
["Lithuania","LTU",0,"11700-12500"]
["Luxembourg","LUX",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Latvia","LVA",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BROADCASTING-SATELLITE"]
["Netherlands","NLD",0,"11700-12500"]
["Portugal","PRT",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,"RAD-S, SIT"]
["Russia","RUS",0,"11700-12500","No","No"]
["Serbia","SRB",0,"11700-12500",null,"X",null,null,null,null,null,null,"X",null,null,null,null,15,null,null,null,"X"]
["Slovak Republic","SVK",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovenia","SVN",0,"11700-12500",null,"X",null,null,null,"X",null,null,null,null,"MMDS",null,null,20,"National (200/400 MHz)",null,null,"x",5,30,40,10,null,null,null,"assigned for local/regional coverage"]
["Sweden","SWE",0,"11700-12500"]
["Telia","TELIASON",0,"11700-12500"]
["Telia","TELIASON",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,302,null,"ERC/REC 12-02",210,null,92,3,null,50,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,22,null,null,null,null,22,9,null,42,"-",null,null,null,"NERA Citylink"]
["Telia","TELIASON",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,80,null,null,32,48,null,5,null,29,0,null,null,null,"Eric sson ML"]
["Austria","AUT",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,137,null,"ERC/REC 12-02",null,null,"x",3,25,52]
["Bosnia and Herzegovina","BIH",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,31,null,"ERC/REC 12-02","X","X","X",2,20,34,"+15"]
["Croatia","HRV",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,244,null,"ERC/REC 12-02",null,"x",null,1.5,19.2,49.2,20,"x"]
["Croatia","HRV",0,"12750-13250","X",null,null,null,null,null,null,null,"X",null,null,1]
["Czech Republic","CZE",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,1288,null,"ERC/REC 12-02",null,null,null,null,null,null,10]
["Cyprus","CYP",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,278,null,"ERC/REC 12-02","X","X"," ",0.28999999999999998,null,40.94,null,"X"]
["Denmark","DNK",0,"12750-13250","X",null,null,null,null,null,null,null,null,null,null,null,4,null,"ERC/REC 12-02",null,null,null,12]
["Estonia","EST",0,"12750-13250",null,null,null,null,null,null,null,null,null,null,null,null,80,null,"ERC/REC 12-02",null,80,null,11,22,34]
["Finland","FIN",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,2120,null,"ERC/REC 12-02",null,"X","X",0.4,14,49,0.2,"x",null,"Local congestion"]
["France","FRA",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,6613,null,"ERC/REC 12-02",2401,3711,501,0.1,"5<x>35",103,"+ 2 %","X"]
["Germany","GER",0,"12750-13250","x",null,null,null,"x",null,null,null,null,null,null,4100,null,null,"ERC/REC 12-02",null,null,"x",0.99,12,48.5]
["Greece","GRC",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,1004,null,"ERC/REC 12-02","X","X","X",1.5,16,55,0.5]
["Hungary","HUN",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,1710,null,"ERC/REC 12-02",null,"X",null,null,12,null,null,"x"]
["Iceland","ICE",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,12,null,"ERC/REC 12-02",null,6,6,10,20,30,0]
["Ireland","IRL",0,"12750-13250"," X",null,null,null,null,null,"X",null,null,null,null,2,1078,null,"ERC/REC 12-02","X","X","X",1.5,19,53," 27"," X"]
["Ireland","IRL",0,"12750-13250",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Italy","ITA",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,6106,null,"ERC/REC 12-02",null,"X","X",7,16,30,0.15,"yes"]
["Latvia","LVA",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,630,null,"ERC/REC 12-02",null,"X",null,2,35,47,20]
["Latvia","LVA",0,"12750-13250",null,"X",null,null,null,null,null,null,"X",null,null,null,null,7,"national plan","X",null,null,null,5,null,null,null,null,"MMDS"]
["Lithuania","LTU",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,222,null,"ERC/REC 12-02"]
["Luxembourg","LUX",0,"12750-13250","X",null,null,null,"X",null,"X",null,"X",null,null,8,22,null,"ERC/REC 12-02",null,"X","X",5.6,"5-35",32,"N/A","NO","NO"]
["Luxembourg","LUX",0,"12750-13250",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Netherlands","NLD",0,"12750-13250","X",null,null,null,null,null,null,null,null,"X",null,null,201,null,"ERC/REC 12-02",null,"X","X",8.35,18.2,31.5]
["Norway","NOR",0,"12750-13250",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-02"]
["Norway","NOR",0,"12750-13250","X",null,null,null,null,null,null,null,null,"X",null,null,1240,null,null,null,"X","X",0.1,14.7,90]
["Portugal","PRT",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,49,null,"ITU-R F.497","X",null,null,2,"25",46,-50]
["Portugal","PRT",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,368,null,"ERC/REC 12-02","X","X","X",1,"15",57,10]
["Russia","RUS",0,"12750-13250","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",16553,null,"ERC/REC 12-02 e ITU-R F.497","X","X","X",10,25,35]
["Serbia","SRB",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,564,null,"ERC/REC 12-02","X","X","X",2.15,19.579999999999998,58.65,50]
["Slovak Republic","SVK",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,620,null,"ERC/REC 12-02","X","X","X",4,15,48,20]
["Slovenia","SVN",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,178,null,"ERC/REC 12-02",null,"X","X",2,25,54,5,"x"]
["Slovenia","SVN",0,"12750-13250","X",null,null,null,"X",null,null,null,"X",null,null,null,21,null,"ERC/REC 12-02",null,null,"X",5,20,40,5,"x"]
["Sweden","SWE",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,775,null,"ERC/REC 12-02",null,null,null,null,null,null,null,"Y"]
["Switzerland","CHE",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,470,null,"ERC/REC 12-02",174,290,6,10,14.2,46.4,"unchanged",null,null,"heavily used by FSS"]
["UK","GBR",0,"12750-13250","X",null,null,null,null,null,null,null,null,"X",null,3840,340,null,"ERC/REC 12-02","X","X","X"]
["Telia","TELIASON",0,"14250-14500"]
["Austria","AUT",0,"14250-14500"]
["Bosnia and Herzegovina","BIH",0,"14250-14500"]
["Croatia","HRV",0,"14250-14500"]
["Czech Republic","CZE",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"sat. services planned"]
["Cyprus","CYP",0,"14250-14500","X",null,null,null,null,null,null,null,"X",null,null,14,null,null,"ERC/REC 13-03",null,"X"," ",8.2899999999999991,null,36.46]
["Denmark","DNK",0,"14250-14500"]
["Estonia","EST",0,"14250-14500"]
["Finland","FIN",0,"14250-14500"]
["France","FRA",0,"14250-14500","X",null,null,null,"X",null,"X",null,null,null,null,null,374,null,null,374,null,null,10,"5<x>35",100,"-5%"]
["Greece","GRC",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Hungary","HUN",0,"14250-14500"]
["Iceland","ICE",0,"14250-14500"]
["Ireland","IRL",0,"14250-14500"]
["Italy","ITA",0,"14250-14500","X",null,null,null,null,null,null,null,"X",null,null,1030,null,null,"national",null,null,"X",3,11,27,0.05,"yes"]
["Latvia","LVA",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIXED-SATELLITE"]
["Lithuania","LTU",0,"14250-14500"]
["Luxembourg","LUX",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Netherlands","NLD",0,"14250-14500"]
["Norway","NOR",0,"14250-14500"]
["Portugal","PRT",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,"FSS, VSAT, SNG, AES"]
["Russia","RUS",0,"14250-14500","X","X",null,null,null,null,null,null,null,null,null,null,150,null,null,"X","X","X",8,20,30]
["Serbia","SRB",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it have not been used yet"]
["Slovak Republic","SVK",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovenia","SVN",0,"14250-14500"]
["Sweden","SWE",0,"14250-14500"]
["Switzerland","CHE",0,"14250-14500"]
["UK","GBR",0,"14250-14500"]
["Bosnia and Herzegovina","BIH",0,"14400-15350","X",null,null,null,null,null,"X",null,null,null,null,null,162,null,"ITU-R F.636","X","X",null,1,15,45,null,null,null,"14400-15350 MHz: Planned leaving of ITU rec. and fully harmonization according to ERC/REC 12-07"]
["Telia","TELIASON",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,944,null,"ERC/REC 12-07",620,324,null,1,null,39,"-",null,null,null,"Eric sson ML"]
["Telia","TELIASON",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,93,null,null,93,null,null,3,null,30,null,"X",null,null,"NEC Pasolink"]
["Austria","AUT",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,631,null,"ERC/REC 12-07","x","x","x",1,15,44]
["Bosnia and Herzegovina","BIH",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,278,null,"ERC/REC 12-07","X","X",null,1,15,45]
["Croatia","HRV",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,"X",null,null,20,null,null,"ERC/REC 12-07",null,null,null,0.6,9.9,22.7]
["Czech Republic","CZE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,20,null,"ERC/REC 12-07"]
["Cyprus","CYP",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,"X",null,null,12,null,null,"ERC/REC 12-07",null,"X",null,0.45,null,38.17]
["Denmark","DNK",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,null,null,null,null,299,null,"ERC/REC 12-07",null,null,null,12]
["Estonia","EST",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,60,null,"ERC/REC 12-07",null,60,null,12,23,33,"- 5"]
["Finland","FIN",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07"]
["Finland","FIN",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,1950,null,"ITU-R F.636",null,"X",null,0.1,8.6999999999999993,10.9,-0.15]
["France","FRA",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07"]
["Germany","GER",0,"14500-14620 and 15230-15350","x",null,null,null,"x",null,null,null,null,null,null,10235,null,null,"ERC/REC 12-07",null,"x",null,2.25,14,54.5,null,"x"]
["Greece","GRC",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,2863,null,"ERC/REC 12-07","X","X","X",0.5,15,75,0.5,"heavily used"]
["Hungary","HUN",0,"14500-14620 and 15230-15350"," ",null,null,null," ",null,null,null,null,null,null,null," ",null,"ERC/REC 12-07",null,null,null,null," "]
["Hungary","HUN",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,"15230-15350 MHz Non-Civil Digital P-P links",null,120,null,null,"X","X",null,null," ",null,null,"x",null,"non-civil usage"]
["Iceland","ICE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,120,null,"ERC/REC 12-07",57,57,6,5,15,25,25]
["Ireland","IRL",0,"14500-14620 and 15230-15350"," X",null,null,null,null,null," X",null,null,null,null,null,1718,null,"ERC/REC 12-07\nNational Legislation: S.I. 370 of 2009"," X","X","X",1.7,17,53," 29"," X"]
["Italy","ITA",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,4070,null,"ERC/REC 12-07","X","X","X",7,16,33,0.15,"yes"]
["Italy","ITA",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,1562,null,"national",null,"X",null,null,null,null,null,"yes"]
["Latvia","LVA",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,48,null,"ERC/REC 12-07",null,"X",null,3,25,37,20]
["Lithuania","LTU",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,262,null,"ERC/REC 12-07"]
["Luxembourg","LUX",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,"X",null,null,0,64,null,"ERC/REC 12-07",null,"X","X",1.4,"5-30",34.700000000000003,"N/A","NO","NO"]
["Netherlands","NLD",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,null,"X",null,null,116,null,"ERC/REC 12-07","x","x","x",7.71,14.7,34.9,20]
["Norway","NOR",0,"14500-14620 and 15230-15350"]
["Portugal","PRT",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,362,null,"ERC/REC 12-07","X","X",null,1,"15",37,5]
["Serbia","SRB",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,433,null,"ERC/REC 12-07","X","X","X",1.35,16.98,39.26,20]
["Slovak Republic","SVK",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,230,null,"ERC/REC 12-07","x","x",null,9.5,15,48,10]
["Slovenia","SVN",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07",null,null,null,null,null,null,null,null,null,"Defence systems:","Land military systems (FS, MS)"]
["Sweden","SWE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,2629,null,"Nat ch.plan(expdate 2016)",null,null,null,null,null,null,null,"Y"]
["Switzerland","CHE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,263,null,"ERC/REC 12-07",110,153,null,10,14.6,37.1,"unchanged"]
["UK","GBR",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,null,"X",null,2050,2050,null,"ERC/REC 12-07","X","X","X"]
["Russia","RUS",0,"14500-14620 and 15230-15350","X","X",null,null,null,null,"X",null,"X",null,null,12,13320,null,"ERC/REC 12-07 e ITU-R F.636","X","X","X",8,20,30]
["Slovenia","SVN",0,"14613-14725 and 15033-15145","X",null,null,null,"X",null,"X",null,null,null,null,null,82,null,"ITU-R F.636-3 (Ch. 5,6,7,8)",null,"x",null,7,25,45,-10,null,"x"]
["Slovenia","SVN",0,"14613-14725 and 15033-15145",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07",null,null,null,null,null,null,null,null,"x","Defence systems:","Land military systems (FS, MS)"]
["Czech Republic","CZE",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FS considered"]
["Greece","GRC",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Italy","ITA",0,"17300-17700","X",null,null,null,"X",null,null,null,null,null,null,null,33,null,"national",null,"X"]
["Latvia","LVA",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HDFSS"]
["Portugal","PRT",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,"FSS, HDFSS"]
["Russia","RUS",0,"17300-17700","No","No"]
["Serbia","SRB",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["Slovak Republic","SVK",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Iceland","ICE",0,"17700-19700","X",null,null,null,"X",null,null,null,null,null,null,null,60,null,"ERC/REC 12-03",40,10,10,10,15,20,25]
["Ireland","IRL",0,"17700-19700"," X",null,null,null,null,null," X",null,null,null,null,null,686,null,"ERC/REC 12-03\nNational Legislation: S.I. 370 of 2009",null," X","X",0.3,9,45," 28"," X"]
["Italy","ITA",0,"17700-19700","X","X",null,null,"X",null,"X",null,null,null,null,null,{"$f":"14300+1512","v":15812},null,"ERC/REC 12-03","X","X","X",0.3,6,12,0.25,"highly"]
["Italy","ITA",0,"17700-19700","X",null,null,null,null,null,"X",null,"X",null,null,71,35,null,null,null,"X","X",1.3,4,7.5,0.25]
["Lithuania","LTU",0,"17700-19700","X",null,null,null,"X",null,null,null,null,null,null,null,490,null,"ERC/REC 12-03"]
["Luxembourg","LUX",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,null,0,47,null,"ERC/REC 12-03",null,null,"X",4.8,"4-25",24.1,"N/A","NO","NO"]
["Luxembourg","LUX",0,"17700-19700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"17700-19700","X",null,null,null,"x",null,null,null,null,null,null,null,390,null,"ERC/REC 12-03",null,null,"X",1,20,43,20]
["Netherlands","NLD",0,"17700-19700","X",null,null,null,null,null,null,null,null,"X",null,null,1020,null,"ERC/REC 12-03",null,"x","x",7.7,5.27,34.9,20]
["Netherlands","NLD",0,"17700-19700","X",null,null,null,null,null,null,null,null,"X",null,null,43,null,"F-5958-8 Annex 8",null,"x","x",5.63,13.11,18.649999999999999,0]
["Norway","NOR",0,"17700-19700",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-03"]
["Norway","NOR",0,"17700-19700","X",null,null,null,null,null,null,null,null,"X",null,null,387,null,null,null,null,"x",0.5,10.199999999999999,44.8]
["Portugal","PRT",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,131,null,"ITU-R F.595","X",null,null,2,"10",29,10]
["Portugal","PRT",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,1087,null,"ERC/REC 12-03",null,"X","X",0,"7",35,20]
["Russia","RUS",0,"17700-19700","X","X",null,null,null,null,null,null,null,null,null,null,24277,null,"ERC/REC 12-03 and ITU-R F.595-9 ","X","X","X",5,12,20]
["Serbia","SRB",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,459,null,"ERC/REC 12-03 and ITU-R F.595-9 ","X","X","X",0.91,10.029999999999999,35.159999999999997,100]
["Slovak Republic","SVK",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,null,null,2170,null,"ERC/REC 12-03","x","x","x",1,10,38,20]
["Slovenia","SVN",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,null,null,361,null,"ERC/REC 12-03",null,null,"x",5,15,35,20,"x**",null,"congested in urban/sub urban regions"]
["Slovenia","SVN",0,"17700-19700",null,"X",null,null,"X",null,"X",null,null,null,null,null,300,null,"ERC/REC 12-03",null,"x","x",5,15,35,0,"x**",null,"congested in urban/sub urban regions"]
["Sweden","SWE",0,"17700-19700","X",null,null,null,"X",null,null,null,null,null,null,null,2242,null,"ERC/REC 12-03",null,null,null,null,null,null,"Y","N"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,3,null,"ERC/REC 12-03",null,null,3,9,null,11,null,"X",null,null,"NEC 900"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,23,null,null,null,null,23,3,null,14,0,null,null,null,"NERA Citylink"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,738,null,null,null,645,93,4,null,28,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,1,null,null,null,null,1,null,9,null,"++",null,null,null,"Ericsson TN"]
["Austria","AUT",0,"21200-22000","X",null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Bosnia and Herzegovina","BIH",0,"21200-22000","X",null,null,null,null,null,"X",null,null,null,null,null,256,null,null,"X","X","X","0.5",5,20,null,null,null,"21200-22000 MHz: Planned leaving of band and full harmonization according to T/R 13-02 Annexes A1, A2, A3"]
["Cyprus","CYP",0,"21200-22000","X",null,null,null,null,null,"X",null,null,null,null,null,97,null,null,"X","X"," ",0.2,null,18.27,null,"X"]
["Greece","GRC",0,"21200-22000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Use"]
["Hungary","HUN",0,"21200-22000","X",null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,40,null,null,"X"]
["Italy","ITA",0,"21200-22000","X",null,null,null,null,null,"X",null,null,null,null,26,7,null,null,null,"X",null,0.19,2.44,7.25]
["Lithuania","LTU",0,"21200-22000","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"local"]
["Latvia","LVA",0,"21200-22000","X",null,null,null,"x",null,null,null,null,null,null,2,null,null,"national plan","X",null,null,3,5,8,100]
["Portugal","PRT",0,"21200-22000",null,null,null,null,null,null,null,null,null,null,"SRR"]
["Serbia","SRB",0,"21200-22000","X",null,null,null,null,null,null,null,"X",null,null,3,null,null,"ITU-R F.637-3 annex 5 ","X",null,null,3.11,4.9800000000000004,7.15]
["Slovak Republic","SVK",0,"21200-22000","X",null,null,null,"X",null,null,null,"X",null,null,0,null,null,"ITU-R F.637",null,null,null,null,null,null,null,null,null,"currently no links"]
["Russia","RUS",0,"21200-23600","X","X",null,null,null,null,null,null,null,null,null,null,16816,null,"F.637 ITU-R","X","X","X",2,4,8]
["Austria","AUT",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,2885,null,"T/R 13-02 Annexes A1, A2, A3","x","x","x",1,10,20]
["Bosnia and Herzegovina","BIH",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,421,null,"T/R 13-02 Annexes A1, A2, A3","X","X","X","0.5",5,20,"+20"]
["switzerland","CHE",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,1900,null,"T/R 13-02 Annexes A1, A2, A3",787,1113,null,5,7.4,29.9,"unchanged","city areas congested, HIGH/LOW situation",null,"problem: SRR"]
["Cyprus","CYP",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,738,null,"T/R 13-02 Annexes A1, A2, A3","X","X"," ",0.25,null,15.16,null,"X"]
["Czech Republic","CZE",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,3707,null,"T/R 13-02 Annexes A1, A2, A3",null,null,null,null,null,null,5]
["Denmark","DNK",0,"22000-22600 and 23000-23600",null,"X",null,null,null,null,null,null,null,null,null,null,"No info",null,"T/R 13-02 Annexes A1, A2, A3"]
["Denmark","DNK",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,null,null,null,650]
["Estonia","EST",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,788,null,"T/R 13-02 Annexes A1, A2, A3",null,788,null,3,14,24,"+25"]
["Finland","FIN",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,2770,null,"T/R 13-02 Annexes A1, A2, A3",null,"X","X",0.1,4.5999999999999996,19,0.15,"x",null,"Local congestion"]
["France","FRA",0,"22000-22600 and 23000-23600","X","X",null,null,"X",null,"X",null,null,null,null,null,12195,null,"T/R 13-02 Annexes A1, A2, A3",4614,7498,83,0.1,"3<x>20",32,"+ 9 %"]
["France","FRA",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IUT-RF 637-3"]
["UK","GBR",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,"X",null,4750,null,null,"T/R 13-02 ","X","X","X"]
["Germany","GER",0,"22000-22600 and 23000-23600","x",null,null,null,"x",null,null,null,null,null,null,19401,null,null,"ERC/REC 13-02 ",null,"x",null,0.13,8,51.1]
["Croatia","HRV",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,1220,null,"T/R 13-02 Annexes A1, A2, A3",null,"x",null,0.18,5.5,21.1,10]
["Hungary","HUN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,"22442-22600 MHz Emergency Services Digital P-P links",null,40,null,"T/R 13-02 Annexes A1, A2, A3","X","X",null,null,null,null,null,"x"]
["Hungary","HUN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,"23450-23600 MHz Emergency services Digital P-P links",null,3512,null,"T/R 13-02 Annexes A1, A2, A3","X","X",null,null,null,null,null,"x"]
["Iceland","ICE",0,"22000-22600 and 23000-23600","X",null,null,null,"x",null,null,null,null,null,null,null,18,null,"T/R 13-02 Annexes A1, A2, A3",5,11,2,1,6,25,25]
["Ireland","IRL",0,"22000-22600 and 23000-23600"," X",null,null,null,null,null," X",null,null,null,null,null,2178,null,"T/R 13-02 Annexes A1, A2, A3"," X","X","X",0.2,6.7,24," 36"," X"]
["Ireland","IRL",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Italy","ITA",0,"22000-22600 and 23000-23600","X","X",null,null,"X",null,"X",null,null,null,null,2,{"$f":"10970+1101","v":12071},null,"T/R 13-02 Annexes A1, A2, A3","X","X","X",2.1800000000000002,2.95,3.17,0.25,"yes"]
["Lithuania","LTU",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,1362,null,"T/R 13-02 Annexes A1, A2, A3"]
["Luxembourg","LUX",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,"X",null,null,1,243,null,"T/R 13-02 Annexes A1, A2, A3",null,"X",null,0.3,"3-20",15,"N/A","NO","NO"]
["Luxembourg","LUX",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,592,null,"T/R 13-02 Annexes A1, A2, A3",null,null,"X",0.15,15,25,30]
["Netherlands","NLD",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,"X",null,null,1450,null,"T/R 13-02 Annexes A1, A2, A3","x","x","x",3,7.65,14.78,30]
["Norway","NOR",0,"22000-22600 and 23000-23600",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annexes A1, A2, A3"]
["Norway","NOR",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,"X",null,2,64,null,null,null,null,"x",0.3,5.7,25.4]
["Portugal","PRT",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,"SRR",null,10,null,"Report 936-2 Annex 6","X",null,null,1,"5",12,-100]
["Portugal","PRT",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,"SRR",null,908,null,"T/R 13-02 Annexes A1","X","X","X",null,"5",12,10]
["Serbia","SRB",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,1288,null,"T/R 13-02 Annexes A1","X","X","X",0.14000000000000001,4.74,24.41,100]
["Slovak Republic","SVK",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,1582,null,"T/R 13-02 Annex A1","x","x","x",0.5,5,13,10]
["Slovenia","SVN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,767,null,"T/R 13-02 Annex A1",null,"x",null,3,7,10,5,"x**",null,"congested in urban/sub urban regions"]
["Slovenia","SVN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,10,null,"T/R 13-02 Annex A1",null,null,"x",2,4,5,20,"x**",null,"congested in urban/sub urban regions"]
["Sweden","SWE",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,1322,null,"T/R 13-02 Annexes A1, A2, A3",null,null,null,null,null,null,null,"Y"]
["Telia","TELIASON",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,506,null,"T/R 13-02 Annexes A1, A2, A3",303,203,null,1,null,18,"-",null,null,null,"Eric sson ML"]
["Telia","TELIASON",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,338,null,null,null,316,22,3,null,17,"+",null,null,null,"NEC NEO"]
["Greece","GRC",0,"22000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,1724,null,"T/R 13-02 Annex A","X","X","X","0.04",4,16,0.4]
["Czech Republic","CZE",0,"22600-22700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENG/OB"]
["Cyprus","CYP",0,"22600-23000","X",null,null,null,null,null,"X",null,null,null,null,37,null,null,"National","X","X"," ",0.2,null,18.14,null,null,"X"]
["Denmark","DNK",0,"22600-23000","X",null,null,null,null,null,null,null,null,null,null,null,1]
["France","FRA",0,"22600-23000","X",null,null,null,"X",null,"X",null,null,null,null,null,124,null,null,124,null,null,0.1,10,32,"+ 1%"]
["Greece","GRC",0,"22600-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,"No current FS use.\nAllocation for analogue links. SAP/SAB, ENG/OB"]
["Hungary","HUN",0,"22600-23000","X",null,null,null,null,null,null,null,"X",null,null,1,null,null,null,null,null,null,null,40,null,null,"x"]
["Italy","ITA",0,"22600-23000","x",null,null,null,null,null,"X",null,null,null,null,1,null,null,null,null,"x",null,null,0.19]
["Lithuania","LTU",0,"22600-23000","X",null,null,null,"X",null,null,null,"X",null,null,1,null,null,"local"]
["Latvia","LVA",0,"22600-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAP/SAB "]
["Portugal","PRT",0,"22600-23000","X",null,null,null,"X",null,"?",null,null,null,"SRR",null,null,null,"T/R 13-02 Annexes A2, A3",null,null,null,null,null,null,"no use at the moment"]
["Serbia","SRB",0,"22600-23000","X",null,null,null,null,null,null,null,"X",null,null,94,null,null,"ITU-R F.637-3 annex 5 ","X",null,null,0.21,2.5,11.87]
["Slovak Republic","SVK",0,"22600-23000","x",null,null,null,"X",null,null,null,"X",null,null,0,null,null,"ITU-R F.637",null,null,null,null,null,null,null,null,null,"currently no links"]
["Slovenia","SVN",0,"22600-23000","x",null,null,null,"X",null,"X",null,null,null,null,null,"planned",null,"T/R 13-02 Annex A2","x","x"]
["Slovenia","SVN",0,"22600-23000",null,null,null,null,"X",null,null,null,"X","X",null,"planned",null,null,"T/R 13-02 Annex A3","x","x"]
["Czech Republic","CZE",0,"22700-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no utilisation"]
["Czech Republic","CZE",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAB"]
["Denmark","DNK",0,"24250-24500","X",null,null,null,null,null,null,null,null,null,null,null,1]
["Greece","GRC",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC REP 38",null,null,null,null,null,null,"-",null,null,"No current use.\nAllocation for analogue links. SAP/SAB, ENG/OB"]
["Hungary","HUN",0,"24250-24500","X","X",null,null,"X","X",null,null,null,null,null,null,41,31,null,"X","X","X",null,7,null,0.25,"x",null,"ù"]
["Lithuania","LTU",0,"24250-24500","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"local"]
["Luxembourg","LUX",0,"24250-24500",null,"X",null,null,null,"X","X",null,"X",null,null,null,null,4,"Nat. freq. plan",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"24250-24500","X",null,null,null,"X",null,"X",null,"X",null,null,0,10,null,"Nat. freq. plan",null,"X",null,null,"2-15",null,"N/A","NO","NO"]
["Latvia","LVA",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAB/SAP, SRR"]
["Portugal","PRT",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,"SRR, SRD"]
["Russia","RUS",0,"24250-24500","No","No",null,null,null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["Slovak Republic","SVK",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Czech Republic","CZE",0,"24500-24745/25500-25753",null,"X",null,null,null,"X",null,null,null,null,null,null,null,133,"T/R 13-02 Annex B",null,null,null,null,null,null,10]
["Austria","AUT",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,2365,null,"T/R 13-02 Annex B","x","x","x",1,6,24]
["Austria","AUT",0,"24500-26500"]
["Bosnia and Herzegovina","BIH",0,"24500-26500","X","X",null,null,null,null,"X",null,null,null,null,null,3,null,"T/R 13-02 Annex B","X","X","X",1,4,6,"+35",null,null,"24500-26500, 27500-29500 MHz: Shared band between P-P links and FWA. Actually, block assignments for P-P links in process. We still do not have active implemented FWA systems."]
["Bosnia and Herzegovina","BIH",0,"24500-26500",null,"X",null,null,"X","X"]
["switzerland","CHE",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,38,null,"T/R 13-02 Annex B",null,null,38,2,2.9,5.9,"growth",null,null,"problem: SRR"]
["switzerland","CHE",0,"24500-26500"]
["Cyprus","CYP",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Cyprus","CYP",0,"24500-26500"]
["Denmark","DNK",0,"24500-26500",null,"X",null,null,null,null,null,null,null,null,null,null,null,"No info","T/R 13-02 Annex B"]
["Denmark","DNK",0,"24500-26500","X",null,null,null,null,null,null,null,null,null,null,null,null,135]
["Estonia","EST",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Estonia","EST",0,"24500-26500"]
["Finland","FIN",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Finland","FIN",0,"24500-26500"]
["France","FRA",0,"24500-26500","X","X",null,null,"X","X","X",null,null,null,null,null,215,75,"T/R 13-02 Annex B",null,88,127,0.12,"3<x>20",15,"+ 3 %"]
["France","FRA",0,"24500-26500"]
["UK","GBR",0,"24500-26500","X",null,null,null,null,null,null,null,null,"X",null,3570,null,null,"T/R 13-02","X","X","X"]
["UK","GBR",0,"24500-26500"]
["Germany","GER",0,"24500-26500","x",null,null,null,"x","x",null,null,null,null,null,15880,null,null,"ERC/REC 13-02 ",null,"x",null,0.1,4,10.9]
["Germany","GER",0,"24500-26500",null,"x",null,null,null,null,null,null,null,null,null,null,null,836]
["Greece","GRC",0,"24500-26500",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC 13-02","-",null,null,null,null,null,"-",null,null,"5 issued licenses"]
["Croatia","HRV",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Croatia","HRV",0,"24500-26500"]
["Hungary","HUN",0,"24500-26500","X","X",null,null,"X","X",null,null,null,null,null,null,83,31,"T/R 13-02 Annex B","X","X","X",null,7,null,0.25,"x",null,"PMP systems"]
["Hungary","HUN",0,"24500-26500"]
["Iceland","ICE",0,"24500-26500","X",null,null,null,"x",null,null,null,null,null,null,null,2,null,"T/R 13-02 Annex B",null,null,2,12,15,18,10]
["Ireland","IRL",0,"24500-26500"," X",null,null,null,"X",null," X",null,null,null,null,null,636,null,"T/R 13-02 Annex B"," X","X","X",0.05,5,17," 43"," X"]
["Ireland","IRL",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Ireland","IRL",0,"24500-26500",null," X",null,null,null,null," X",null,null,null,null,null,null,null," National Legislation: S.I. 762 of 2007"]
["Ireland","IRL",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ireland","IRL",0,"24500-26500","X",null,null,null,null,"X",null,null,null,null,null,null,null,15,"National Legislation: S.I. 79 of 2003",null,null,null,null,null,null,55]
["Ireland","IRL",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 530 of 2003"]
["Italy","ITA",0,"24500-26500",null,"X",null,null,null,"X","X",null,null,null,null,null,null,"not known","T/R 13-02 Annex B",null,null,null,null,null,null,0.15,"not yet"]
["Italy","ITA",0,"24500-26500"]
["Lithuania","LTU",0,"24500-26500","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"T/R 13-02 Annex B"]
["Lithuania","LTU",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,84,"T/R 13-02 Annex B",null,null,null,null,null,null,30]
["Luxembourg","LUX",0,"24500-26500",null,"X",null,null,null,"X","X",null,"X",null,null,null,null,4,"T/R 13-02 Annex B",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"24500-26500","X",null,null,null,"X",null,"X",null,"X",null,null,0,10,null,"Nat. freq. plan",null,"X",null,null,"2-15",null,"N/A","NO","NO"]
["Latvia","LVA",0,"24500-26500","X",null,null,null,"x",null,null,null,null,null,null,null,6,null,"T/R 13-02 Annex B",null,null,"X",1.4,5,6]
["Latvia","LVA",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,52,null,null,"X",null,null,5,null,50]
["Netherlands","NLD",0,"24500-26500","x",null,null,null,null,null,null,null,null,"X",null,null,908,null,"T/R 13-02 Annex B","x","x","x",2.5499999999999998,6.42,14.52,30]
["Netherlands","NLD",0,"24500-26500",null,null,null,null,null,"x",null,null,null,"X",null,null,null,90,"T/R 13-02 Annex B",null,null,null,null,null,null,10]
["Norway","NOR",0,"24500-26500",null,"x",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annex B"]
["Norway","NOR",0,"24500-26500","x",null,null,null,null,null,null,null,null,"X",null,3,65,null,null,null,"x","x",0.5,4.8,21.1]
["Portugal","PRT",0,"24500-26500",null,"X",null,null,null,"X","X",null,null,null,"SRR, SRD, Military (25.25-25.492 GHz and 26.25-27.5 GHz)",null,null,125,"T/R 13-02 Annex B","X","X",null,null,"5",null,0]
["Portugal","PRT",0,"24500-26500"]
["Russia","RUS",0,"24500-26500","X","X",null,null,null,"X","X",null,null,null,null,null,447,null,"T/R 13-02 Annex B","X","X","X",2,4,8]
["Russia","RUS",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["Serbia","SRB",0,"24500-26500","X",null,null,null,null,null,"X",null,null,null,null,null,660,null,"T/R 13-02 Annex B","X","X","X",0.6,2.21,12.5,100]
["Serbia","SRB",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,4]
["Slovak Republic","SVK",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,1230,null,"T/R 13-02 Annex B","x","x","x",0.1,3.5,8,20]
["Slovak Republic","SVK",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,40,null,"x","x",null,null,null,null,10]
["Slovenia","SVN",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,109,null,"T/R 13-02 Annex B (25.165-25.557 GHz/>26.173 GHz)",null,"x",null,3,6,8,100,null,null,null,"used instead of the congested 23 GHz band"]
["Slovenia","SVN",0,"24500-26500","X",null,null,null,null,"X","X",null,null,null,null,null,null,22,"T/R13-02 AnnexB (25.053-25.165GHz/26.061-26.173GHz)",null,"x",null,null,null,null,-5]
["Slovenia","SVN",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,"BWA",null,null,"planned","T/R13-02 Annex B (24.549–25.053GHz/25.557–26.061GHz)",null,"x","x",1,3,5,null,null,null,"BWA"]
["Sweden","SWE",0,"24500-26500",null,"X",null,null,"X","X","X",null,null,null,null,null,5601,null,"T/R 13-02 Annex B",null,null,null,null,null,null,"Y"]
["Sweden","SWE",0,"24500-26500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null," ERC / REC / (00) 05",null,null,null,null,null,null,null,"N"]
["Telia","TELIASON",0,"24500-26500",null,"X",null,null,null,null,"X",null,null,null,null,null,161,null,"T/R 13-02 Annex B",99,18,44,2,null,10,"-",null,null,null,"Eric sson ML"]
["Telia","TELIASON",0,"24500-26500",null,"X",null,null,null,null,null,null,null,null,null,null,629,null,null,null,574,55,1,null,12,"+",null,null,null,"NEC NEO"]
["Czech Republic","CZE",0,"24745-25500/25753-26500","X",null,null,null,"X",null,null,null,null,null,null,null,4537,null,null,null,null,null,null,null,null,10]
["Czech Republic","CZE",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,"MD"]
["Czech Republic","CZE",0,"26500-27500"]
["Greece","GRC",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Hungary","HUN",0,"26500-27500",null,null,null,null,"X",null,null,null,null,null,"Land military systems. P-P links Harmonized NATO band type 2.(planned)",null,null,null,null,null,null,null,null,null,null,null,"X"]
["Latvia","LVA",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band"]
["Portugal","PRT",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,"SRR, SRD, Military (26.25-27.5 GHz)"]
["Russia","RUS",0,"26500-27500","X","X",null,null,null,"X","X",null,null,null,null,null,26,null,"F.748 ITU-R","X","X","X",2,4,8]
["Serbia","SRB",0,"26500-27500",null,null,null,null,null,null,null,null,null,"X"]
["Slovak Republic","SVK",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Austria","AUT",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,156,null,"T/R 13-02 Annex C",null,null,"x",1,2,4]
["Austria","AUT",0,"27500-29500"]
["Bosnia and Herzegovina","BIH",0,"27500-29500","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,"+5",null,null,"24500-26500, 27500-29500 MHz: Shared band between P-P links and FWA. Actually, block assignments for P-P links in process. We still do not have active implemented FWA "]
["Bosnia and Herzegovina","BIH",0,"27500-29500",null,"X",null,null,"X","X"]
["switzerland","CHE",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,"starts now",null,"T/R 13-02 Annex C",null,null,null,null,null,null,"growth"]
["switzerland","CHE",0,"27500-29500"]
["Cyprus","CYP",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Cyprus","CYP",0,"27500-29500"]
["Czech Republic","CZE",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,41,"T/R 13-02 Annex C"]
["Czech Republic","CZE",0,"27500-29500","X","X",null,null,"X","X",null,null,null,null,null,null,189]
["Denmark","DNK",0,"27500-29500","X",null,null,null,null,null,null,null,null,null,null,null,null,18,"T/R 13-02 Annex C"]
["Denmark","DNK",0,"27500-29500"]
["Estonia","EST",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Estonia","EST",0,"27500-29500"]
["Finland","FIN",0,"27500-29500","X",null,null,null,null,null,"X",null,null,null,null,null,380,null,"T/R 13-02 Annex C",null,"X","X",0.1,1.1000000000000001,7.2,0.9,"x",null,"Local congestion"]
["Finland","FIN",0,"27500-29500"]
["France","FRA",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["France","FRA",0,"27500-29500"]
["UK","GBR",0,"27500-29500"]
["UK","GBR",0,"27500-29500"]
["Germany","GER",0,"27500-29500",null,"x",null,null,"x","x",null,null,null,null,null,1424,null,29,"ERC/REC 13-02 ",null,null,null,0.18,3,13.3]
["Greece","GRC",0,"27500-29500",null,null,null,null,"X","X",null,null,null,null,null,null,null,null,"ECC/DEC/(05)01","no current use",null,null,null,null,null,"-",null,null,"27828,5-27940,5 and 27940,5-28444,5 MHz paired with 28948,5-29452,5 new row by EETT allocated to digital P-P and P-MP links"]
["Croatia","HRV",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Croatia","HRV",0,"27500-29500"]
["Hungary","HUN",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Hungary","HUN",0,"27500-29500"]
["Iceland","ICE",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Ireland","IRL",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Ireland","IRL",0,"27500-29500"]
["Italy","ITA",0,"27500-29500",null,"X",null,null,null,"X","X",null,null,null,null,null,null,"not known","T/R 13-02 Annex C",null,null,null,null,null,null,0.15,"not yet"]
["Italy","ITA",0,"27500-29500"]
["Lithuania","LTU",0,"27500-29500","X",null,null,null,"X",null,null,null,null,null,null,null,20,null,"T/R 13-02 Annex C",null,20]
["Lithuania","LTU",0,"27500-29500",null,"X",null,null,null,"X",null,null,"X",null,null,null,null,8,"54MHz/3,2MHz",null,null,null,null,null,null,0,null,null,"LMDS (do not comply T/R 13-02)"]
["Luxembourg","LUX",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Luxembourg","LUX",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Latvia","LVA",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,51,null,null,null,"X",null,null,null,50]
["Netherlands","NLD",0,"27500-29500","X",null,null,null,null,null,null,null,null,"X",null,null,185,null,"T/R 13-02 Annex C",null,null,"x",2.52,4.21,6.8730000000000002,30]
["Netherlands","NLD",0,"27500-29500"]
["Norway","NOR",0,"27500-29500",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annex C"]
["Norway","NOR",0,"27500-29500","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Portugal","PRT",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,"FSS, HDFSS",null,null,21,"T/R 13-02 Annex C",null,"X",null,null,"5",null,0]
["Portugal","PRT",0,"27500-29500"]
["Russia","RUS",0,"27500-29500","X","X",null,null,null,"X","X",null,null,null,null,null,1,null,"T/R 13-02 Annex C","X","X","X",2,4,8]
["Russia","RUS",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["Serbia","SRB",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["Serbia","SRB",0,"27500-29500"]
["Slovak Republic","SVK",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,110,null,"T/R 13-02 Annex C","x","x","x",0.2,2.5,4.5,10]
["Slovak Republic","SVK",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,15,null,"x","x",null,null,null,null,10]
["Slovenia","SVN",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,"planned",null,"T/R 13-02 Annex C (27.8285 – 27.9405 GHz/28.8365 – 28.9485 GHz)",null,"x",null,0.5,3,5]
["Slovenia","SVN",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,"planned","T/R13-02 Annex C (27.9405 – 28.4445 GHz/28.9485 – 29.4525 GHz)",null,"x","x",0.3,2,4]
["Sweden","SWE",0,"27500-29500",null,"X",null,null,"X","X","X",null,null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,"Y"]
["Telia","TELIASON",0,"27500-29500",null,"X",null,null,null,null,"X",null,null,null,null,null,6,null,"T/R 13-02 Annex C",null,null,6,1,null,4,"++",null,null,null,"Ericsson TN"]
["Telia","TELIASON",0,"27500-29500"]
["Czech Republic","CZE",0,"31000-31300","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,5]
["UK","GBR",0,"31000-31300","X",null,null,null,null,null,null,null,null,null,"X",null,null,null,"national arrangement"]
["Germany","GER",0,"31000-31300",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,"x",null,null,null,null,null,null,null,"not open"]
["Hungary","HUN",0,"31000-31300","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02","X","X","X",null,5,null,null,"x",null,"FDD mode PP systems"]
["Lithuania","LTU",0,"31000-31300","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ECC/REC/(02)02"]
["Luxembourg","LUX",0,"31000-31300","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ECC/REC/(02)02",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"31000-31300",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"31000-31300","?",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,null,null,null,"Fixed links, FWA"]
["Portugal","PRT",0,"31000-31300",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,"Planned"]
["Russia","RUS",0,"31000-31300","No","No",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02"]
["Austria","AUT",0,"31800-33400"]
["Bosnia and Herzegovina","BIH",0,"31800-33400"]
["switzerland","CHE",0,"31800-33400","X",null,null,null,"X",null,"X",null,null,null,null,null,102,null,"ERC/REC/(01)02",null,69,33,0.5,2.2999999999999998,4.5999999999999996,"growth"]
["Cyprus","CYP",0,"31800-33400"]
["Czech Republic","CZE",0,"31800-33400","X",null,null,null,"X",null,null,null,null,null,null,null,50,null,"ERC/REC/(01)02",null,null,null,null,null,null,50]
["Denmark","DNK",0,"31800-33400",null,"X",null,null,null,null,null,null,null,null,null,null,"No info",null,"ERC/REC/(01)02"]
["Estonia","EST",0,"31800-33400"]
["Finland","FIN",0,"31800-33400","X",null,null,null,null,null,"X",null,null,null,null,null,1,null,"ERC/REC/(01)02",null,"X","X",null,null,null,100]
["France","FRA",0,"31800-33400","X","X",null,null,"X",null,"X",null,null,null,null,null,null,null,"ERC/REC/(01)02"]
["UK","GBR",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it have not been used yet"]
["Germany","GER",0,"31800-33400","x",null,null,null,"x",null,null,null,null,null,null,1466,null,null,"ERC/REC/(01)02",null,"x",null,0.1,2.2999999999999998,6.8,20]
["Greece","GRC",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Croatia","HRV",0,"31800-33400"]
["Hungary","HUN",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,"x"]
["Hungary","HUN",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(04)06",null,null,null,null,null,null,null,"x"]
["Iceland","ICE",0,"31800-33400"]
["Ireland","IRL",0,"31800-33400"]
["Italy","ITA",0,"31800-33400"]
["Lithuania","LTU",0,"31800-33400","X",null,null,null,"X",null,null,null,null,null,null,null,28,null,"ERC/REC/(01)02"]
["Luxembourg","LUX",0,"31800-33400","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC/(01)02",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan "]
["Latvia","LVA",0,"31800-33400",null,"X",null,null,"X",null,null,null,null,null,null,null,43,null,"ERC/REC/(01)02",null,null,"X",0.2,3,4.5999999999999996,100]
["Netherlands","NLD",0,"31800-33400","X",null,null,null,null,null,null,null,null,"X",null,null,515,null,"ERC/REC/(01)02","x","x","x",0.253,3.57,6.27,30]
["Norway","NOR",0,"31800-33400",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC/(01)02"]
["Norway","NOR",0,"31800-33400","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Portugal","PRT",0,"31800-33400","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,null,null,"Not used at the moment."]
["Russia","RUS",0,"31800-33400","No","No",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02"]
["Russia","RUS",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(04)06"]
["Serbia","SRB",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,null,null,"it have not been used yet"]
["Slovak Republic","SVK",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,100,null,null,"operation expected"]
["Slovenia","SVN",0,"31800-33400","x",null,null,null,"X",null,"X",null,null,null,null,null,"planned Upper part",null,"ERC/REC/(01)02",null,"x","x",0.2,2,4]
["Slovenia","SVN",0,"31800-33400",null,"x",null,null,null,"X",null,null,null,null,"BWA",null,"planned Lower part",null,"ERC/REC/(01)02/ ECC/REC/(04)06",null,"x","x",0.2,1,3,null,null,null,"BWA"]
["Sweden","SWE",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,1887,null,"ERC/REC/(01)02"]
["Sweden","SWE",0,"31800-33400","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(04)06",null,null,null,null,null,null,"Y","N"]
["Telia","TELIASON",0,"31800-33400","X",null,null,null,null,null,"X",null,null,null,null,null,1085,null,"ERC/REC/(01)02",null,996,89,0.2,null,8.6999999999999993,"+",null,null,null,"NEC NEO"]
["Russia","RUS",0,"36000-37000","X","X",null,null,null,null,"X",null,null,null,null,null,132,null,"F.749 ITU-R","X","X","X",0.1,3,5]
["Austria","AUT",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,5273,null,"T/R 12-01","x","x","x",1,5,17]
["Bosnia and Herzegovina","BIH",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,1,23,null,"T/R 12-01","X",null,null,"0.1",1,5,"+5"]
["switzerland","CHE",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,3134,null,"T/R 12-01",1248,1886,null,1,2.6,7.9,"unchanged","city areas congested, HIGH/LOW situation"]
["Cyprus","CYP",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 12-01"]
["Czech Republic","CZE",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,5603,null,"T/R 12-01",null,null,null,null,null,null,5]
["Denmark","DNK",0,"37000-39500","X",null,null,null,null,null,null,null,null,null,null,null,158,null,"T/R 12-01"]
["Denmark","DNK",0,"37000-39500",null,"X",null,null,null,null,null,null,null,null,null,null,"No info"]
["Estonia","EST",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,232,null,"T/R 12-01",169,63,null,0.7,5,10,"+10"]
["Finland","FIN",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,45,null,"T/R 12-01",null,"X","X",0.2,1.7,6.1,0.1]
["France","FRA",0,"37000-39500","X","X",null,null,"X",null,"X",null,null,null,null,null,8304,null,"T/R 12-01",2223,6057,24,0.1,"0<x>6",15,"+8%"]
["UK","GBR",0,"37000-39500","X",null,null,null,null,null,null,null,null,"X",null,12050,null,null,"T/R 12-01","X","X","X"]
["Germany","GER",0,"37000-39500","x",null,null,null,"x",null,null,null,null,null,null,30594,null,null,"ERC/REC 12-01 ",null,"x",null,0.02,2.2999999999999998,13.2]
["Greece","GRC",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,984,null,"T/R 12-01",null,"X","X","0.05","1.5","6.8",0.2]
["Croatia","HRV",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,335,null,"T/R 12-01",null,"x",null,7.0000000000000007E-2,0.42,4.9000000000000004,20]
["Hungary","HUN",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,6454,null,"T/R 12-01","X","X","X",null,4]
["Hungary","HUN",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,"37926-38178 and 39186-39500 MHz Non-Civil P-P links.   39186-39500 MHz Emergency services. 37-39.5 GHz NJFA military requirement for existing and future fixed systems.",null,100,null,"ERC/DEC/(00)02","X","X","X"]
["Iceland","ICE",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,1,null,"T/R 12-01",1,null,null,null,5]
["Ireland","IRL",0,"37000-39500"," X",null,null,null,null,null,"X",null,null,null,null,null,2924,null,"T/R 12-01"," X","X","X",1.6E-2,1.9,10.7," 31"," X"]
["Ireland","IRL",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Italy","ITA",0,"37000-39500","X","X",null,null,"X",null,"X",null,null,null,null,null,10412,null,"T/R 12-01","X","X","X",null,"0,8/10",null,0.25,"yes"]
["Lithuania","LTU",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,268,null,"T/R 12-01",null,268]
["Luxembourg","LUX",0,"37000-39500","X",null,null,null,"X",null,"X",null,"X",null,null,1,110,null,"T/R 12-01",null,"X",null,0.13,"1-6",5.4,"N/A","NO","NO"]
["Luxembourg","LUX",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,27,null,"T/R 12-01",null,null,"X",0.2,3,4.7,20]
["Netherlands","NLD",0,"37000-39500","X",null,null,null,null,null,null,null,null,"X",null,null,6377,null,"T/R 12-01","x","x","x",0.05,2.15,10.266,30]
["Norway","NOR",0,"37000-39500",null,"x",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 12-01 Annex A"]
["Norway","NOR",0,"37000-39500","X",null,null,null,null,null,null,null,null,"X",null,null,64,null,null,null,null,"x",0.1,3.6,16.399999999999999]
["Norway","NOR",0,"37000-39500"]
["Portugal","PRT",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,"FS",null,617,null,"T/R 12-01","X","X","X",0,"2",6,5]
["Russia","RUS",0,"37000-39500","X","X",null,null,null,null,"X",null,null,null,null,null,16865,null,"T/R 12-01","X","X","X",0.1,3,5]
["Russia","RUS",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.749 ITU-R"]
["Serbia","SRB",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,426,null,"T/R 12-01","X","X","X",0.16,1.4,4.8600000000000003,300]
["Slovak Republic","SVK",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,1600,null,"T/R 12-01","x","x","x",0.1,2,9,20]
["Slovenia","SVN",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,580,null,"T/R 12-01",null,"x",null,0.1,2,4,30,"x***",null,null,"HI/LO problem"]
["Slovenia","SVN",0,"37000-39500","X",null,null,null,"X",null,"X"]
["Sweden","SWE",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,6188,null,"T/R 12-01"]
["Sweden","SWE",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"T/R 12-01",null,null,null,null,null,null,"Y","N"]
["Telia","TELIASON",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,173,null,"T/R 12-01",95,78,null,0.1,null,5.4,0,null,null,null,"Ericsson ML"]
["Austria","AUT",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Bosnia and Herzegovina","BIH",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["switzerland","CHE",0,"40500-43500","X",null,null,null,"X",null,"X",null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"growth. Starts now"]
["Cyprus","CYP",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Czech Republic","CZE",0,"40500-43500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"yes",null,null,"P-P and P-MP planned"]
["Denmark","DNK",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Estonia","EST",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Finland","FIN",0,"40500-43500","X",null,null,null,null,null,"X",null,null,null,null,null,null,null,"ECC/REC/(01)04",null,"X","X",null,null,null,null,null,null,"Opens 2011"]
["France","FRA",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Germany","GER",0,"40500-43500","x",null,null,null,"x",null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,"x",null,null,null,null,null,null,"will be opened 2011"]
["Greece","GRC",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Use"]
["Croatia","HRV",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Hungary","HUN",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Iceland","ICE",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Ireland","IRL",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Italy","ITA",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Lithuania","LTU",0,"40500-43500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,0,"ECC/REC/(01)04"]
["Luxembourg","LUX",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Latvia","LVA",0,"40500-43500",null,"X",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,null,null,null,"MWS (MVDS)"]
["Netherlands","NLD",0,"40500-43500","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,100]
["Norway","NOR",0,"40500-43500",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ECC/REC/(01)04 Annex A"]
["Norway","NOR",0,"40500-43500","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Portugal","PRT",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,"MWS, MVDS",null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"Planned "]
["Russia","RUS",0,"40500-43500","X","X",null,null,null,"X","X",null,null,null,null,null,73,null,"ECC/REC/(01)04","X","X","X",0.1,3,5]
["Serbia","SRB",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["Slovak Republic","SVK",0,"40500-43500",null,"X",null,null,null,"X",null,null,"X",null,null,null,null,3,"ECC/REC/(01)04",null,"x"]
["Slovenia","SVN",0,"40500-43500",null,"X",null,null,null,"X",null,null,null,null,"MWS",null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"planned Upper part",null,null,"MWS"]
["Slovenia","SVN",0,"40500-43500","X",null,null,null,"X",null,"X",null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"planned Lower part (only small part)"]
["Sweden","SWE",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04\n(New ITU-R Rec under dev.)",null,null,null,null,null,null,"Y","N",null,"Blockassignments?"]
["Telia","TELIASON",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Czech Republic","CZE",0,"47200-48500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["Latvia","LVA",0,"47200-48500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAP/SAB, HAPS "]
["Portugal","POR",0,"47200-48500",null,null,null,null,null,null,null,null,null,null,"HDFSS (47.5-47.9 GHz)"]
["Russia","RUS",0,"47200-48500"]
["Czech Republic","CZE",0,"48500-50200","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["Hungary","HUN",0,"48500-50200",null,null,null,null,"X",null,null,null,null,null,"Non-Civil Digital P-P links",null,null,null,"ERC/REC 12-10"]
["Lithuania","LTU",0,"48500-50200","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 12-10"]
["Luxembourg","LUX",0,"48500-50200","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-10",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"48500-50200","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"Fixed links"]
["Norway","NOR",0,"48500-50200","X","X",null,null,null,null,null,null,null,"X",null,null,0,null,"ERC/REC 12-10"]
["Portugal","POR",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,"HDFSS (48.2-48.54 GHz and 49.44-50.2 GHz)",null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,"Planned"]
["Russia","RUS",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10"]
["Serbia","SRB",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Slovenia","SVN",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,null,null,"planned",null,"ERC/REC 12-10"]
["Czech Republic","CZE",0,"50400-51400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["Denmark","DNK",0,"50400-51400","X",null,null,null,null,null,null,null,null,null,null,null,1]
["Latvia","LVA",0,"50400-51400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Future satellite and terrestrial applications"]
["Portugal","POR",0,"50400-51400",null,null,null,null,null,null,null,null,null,"X"]
["Russia","RUS",0,"50400-51400"]
["switzerland","CHE",0,"51400-52600",null,"X",null,null,"X",null,"X",null,null,null,null,null,837,null,"ERC/REC 12-11",193,644,null,0.15,0.8,2.8,"growth"]
["Czech Republic","CZE",0,"51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["UK","GBR",0,"51400-52600","X",null,null,null,null,null,null,null,null,null,null,0,null,null,"ERC/REC 12-11"]
["Germany","GER",0,"51400-52600","x",null,null,null,"x",null,null,null,null,null,null,null,null,0,"ERC/REC 12-11",null,"x"]
["Hungary","HUN",0,"51400-52600","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,null,null,"30 original value"]
["Lithuania","LTU",0,"51400-52600","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 12-11"]
["Luxembourg","LUX",0,"51400-52600","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-11",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"51400-52600","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"Fixed links"]
["Portugal","POR",0,"51400-52600",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,"Planned"]
["Russia","RUS",0,"51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11"]
["Serbia","SRB",0,"51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Slovenia","SVN",0,"51400-52600","X",null,null,null,"X",null,"X",null,null,null,null,null,"planned",null,"ERC/REC 12-11",null,"x","x",0.1,2,4]
["switzerland","CHE",0,"55780-57000",null,"X",null,null,"X",null,"X",null,null,null,null,null,0,null,"ERC/REC 12-12",null,null,null,null,null,null,"no equipment available"]
["Czech Republic","CZE",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["UK","GBR",0,"55780-57000","X",null,null,null,null,null,null,null,null,null,null,0,null,null,"ERC/REC 12-12"]
["Germany","GER",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,0,"ERC/REC 12-12",null,"x",null,null,null,null,null,null,null,"not open"]
["Greece","GRC",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12 Annex 3",null,null,null,null,null,null,"Maximum PFD=-26dBW/MHz",null,null,"No current use. Allocation for digital P-P links"]
["Hungary","HUN",0,"55780-57000","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,30]
["Luxembourg","LUX",0,"55780-57000","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-12",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"55780-57000","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"Fixed links"]
["Norway","NOR",0,"55780-57000","X","X",null,null,null,null,null,null,null,"X",null,null,0,null,"ERC/REC 12-09"]
["Portugal","POR",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,"EESS",null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,"Planned"]
["Russia","RUS",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12"]
["Serbia","SRB",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Slovenia","SVN",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,"planned",null,"ERC/REC 12-12"]
["Sweden","SWE",0,"55780-57000",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,"N"]
["switzerland","CHE",0,"57000-58000",null,"X",null,null,"X",null,"X",null,null,null,null,null,292,null,"ECC/REC/(09)01",292,null,null,0.1,0.3,2.2000000000000002,"reduction"]
["Czech Republic","CZE",0,"57000-59000","X",null,null,null,"X",null,null,null,null,null,null,null,3,null,"ECC/REC/(09)01",null,null,null,null,null,null,"yes"]
["UK","GBR",0,"57000-59000",null,null,null,"X",null,null,null,null,null,"X",null,null,null,null,"no channel plan"]
["Greece","GRC",0,"57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-09 Annex A",null,null,null,null,null,null,"Radio Frequency Rights of Use not required. Maximum EIRP=15dBW",null,null,"No current use. Allocation for digital P-P links"]
["Hungary","HUN",0,"57000-59000","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,null,null,"25 original"]
["Ireland","IRL",0,"57000-59000","X",null,null,null,null,null," X",null,null,null,null,null,1,null,"ECC/REC/(09)01\nNational Legislation: S.I. 370 of 2009"," X",null,null,1.4,1.4,1.4," 0"]
["Luxembourg","LUX",0,"57000-59000","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"57000-59000",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"SRD, Fixed links, FWA"]
["Portugal","POR",0,"57000-59000","?","?",null,null,"X","X","X",null,null,null,"EESS, SRD",null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"No use at the moment."]
["Russia","RUS",0,"57000-59000","X","X",null,null,null,null,"X",null,null,null,null,null,420,null,"ECC/REC/(09)01","X","X",null,0.1,1,2]
["Russia","RUS",0,"57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.1497 ITU-R"]
["Serbia","SRB",0,"57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Slovenia","SVN",0,"57000-59000",null,null,null,"X","X",null,null,null,null,null,null,null,"N/A",null,"ECC/REC/(09)01",null,null,"x",null,1,null,"N/A"]
["Sweden","SWE",0,"57000-59000",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Y","N",null,"Exemption"]
["Norway","NOR",0,"57000-64000","X","X",null,null,null,null,null,null,null,"X",null,null,1,null,"ECC/REC/(09)01",null,null,1,null,0.4]
["Germany","GER",0,"57100-58900",null,null,null,"x","x",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01","x"]
["switzerland","CHE",0,"58000-63000",null,null,null,"X",null,null,null,null,null,null,null,null,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"no equipment available"]
["Germany","GER",0,"59000-63000",null,null,null,"x","x",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,"x"]
["Czech Republic","CZE",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,"MD shared",null,null,null,"ECC/REC/(09)01"]
["UK","GBR",0,"59000-64000",null,null,null,"X",null,null,null,null,null,"X",null,null,null,null,"no channel plan"]
["Hungary","HUN",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,"59000-61000 MHz Harmonized NATO band type 2. (planned for P-P)",null,null,null,"ECC/REC/(09)01"]
["Luxembourg","LUX",0,"59000-64000","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"SRD,  Military band 59-61 GHz"]
["Portugal","POR",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,"SRD, ISM, Military (59-61 GHz)",null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Planned"]
["Russia","RUS",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01"]
["Serbia","SRB",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Sweden","SWE",0,"59000-64000",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Y","N",null,"Exemption"]
["Russia","RUS",0,"71000-76000 and  81000-86000",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07"]
["switzerland","CHE",0,"71000-76000 and  81000-86000","X",null,null,null,"X",null,"X",null,null,null,null,null,"starts now",null,"ECC/REC/(05)07",null,null,null,null,null,null,"equipment not clear defined"]
["Czech Republic","CZE",0,"71000-76000 and  81000-86000",null,null,null,"X","X",null,null,null,null,null,null,null,57,null,"ECC/REC/(05)07",null,null,null,null,null,null,100]
["France","FRA",0,"71000-76000 and  81000-86000","X",null,null,null,"X",null,"X",null,null,null,null,null,0,null,"ECC/REC/(05)07"]
["UK","GBR",0,"71000-76000 and  81000-86000","X",null,null,null,null,null,null,null,null,"X",null,null,30,null,"no channel plan",null,null,"X"]
["Germany","GER",0,"71000-76000 and  81000-86000","x",null,null,null,"x",null,null,null,null,null,null,null,null,0,"ECC/REC/(05)07",null,null,"x"]
["Greece","GRC",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"No current use. Allocation for digital P-P links"]
["Hungary","HUN",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,"71000-74000 and 81000-84000 MHz Common Civil and Non-Civil band for P-P links",null,null,null,"ECC/REC/(05)07"]
["Ireland","IRL",0,"71000-76000 and  81000-86000","X",null,null,null,null,null," X",null,null,null,null,null,5,null,"ECC/REC/(05)07\nNational Legislation: S.I. 370 of 2009",null,null," X",0.1,1,2.9," 0"]
["Lithuania","LTU",0,"71000-76000 and  81000-86000",null,null,null,"X","X",null,null,null,null,null,null,0,0,null,"ECC/REC/(05)07"]
["Latvia","LVA",0,"71000-76000 and  81000-86000","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"Military band 71-74 GHz, 81-84 GHz. Fixed links 74-76GHz, 84-86 GHz"]
["Norway","NOR",0,"71000-76000 and  81000-86000","X","X",null,null,null,null,null,null,null,"X",null,null,4,null,"ECC/REC/(05)07",null,null,"x",1,1.8,3.4]
["Portugal","POR",0,"71000-76000 and  81000-86000","?","?",null,null,"X","X","X",null,null,null,"SRD, AM (75.5-76 GHz), Military (71-74 GHz and 81-84 GHz)",null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,"No use at the moment."]
["Serbia","SRB",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Sweden","SWE",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,"Y","N",null,"Light Lic?"]
["Slovenia","SVN",0,"74000-76000 and 84000-86000","X",null,null,null,"X",null,null,null,null,"X",null,null,"planned",null,"ECC/REC/(05)07",null,null,"x"]
["Czech Republic","CZE",0,"92000-95000","X",null,null,null,"X",null,null,null,null,null,null,null,3]
["Hungary","HUN",0,"92000-95000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5.149"]
["Latvia","LVA",0,"92000-95000"]
["Portugal","POR",0,"92000-95000",null,null,null,null,null,null,null,null,null,"X"]
["Russia","RUS",0,"92000-95000",null,null,null,"X"]
["Sweden","SWE",0,"92000-95000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N",null,"Light Lic?"]

{"sheet":"Country names","index":2,"n_rows":55,"n_cols":10,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,0,3,0],[0,1,3,1],[51,0,52,0],[51,1,52,1],[51,2,52,2]]}
["Member",null,"CEPT",null,null,6]
[null,null,"Country"]
[null,null,"Code"]
[]
["Albania",null,"ALB"]
["Andorra",null,"AND",null,null,null,"respondent to 2016 Quest"]
["Austria",null,"AUT",null,null,null,"respondent to 2010 Quest"]
["Azerbaijan",null,"AZE"]
["Belarus",null,"BLR"]
["Belgium",null,"BEL",null,null,null,null,null,null,"E"]
["Bosnia and Herzegovina",null,"BIH"]
["Bulgaria",null,"BUL",null,null,null,null,null,null,"E"]
["Croatia",null,"HRV"]
["Cyprus",null,"CYP",null,null,null,null,null,null,"E"]
["Czech Republic",null,"CZE"]
["Denmark",null,"DNK",null,null,null,null,null,null,"E"]
["Estonia",null,"EST"]
["Finland",null,"FIN"]
["France",null,"FRA"]
["Georgia",null,"GEO"]
["Germany",null,"GER"]
["Greece",null,"GRC"]
["Hungary",null,"HUN"]
["Iceland",null,"ICE",null,null,null,null,null,null,"E"]
["Ireland",null,"IRL"]
["Italy",null,"ITA"]
["Latvia",null,"LVA"]
["Liechtenstein",null,"LIE"]
["Lithuania",null,"LTU",null,null,null,null,null,null,"E"]
["Luxembourg",null,"LUX",null,null,null,null,null,null,"E"]
["The Former Yugoslav Republic of Macedonia (FYROM) ",null,"MKD"]
["Malta",null,"MLT",null,null,null,null,null,null,"E"]
["Moldova",null,"MDA"]
["Monaco",null,"MCO"]
["Montenegro",null,"MNE"]
["Netherlands",null,"NLD"]
["Norway",null,"NOR"]
["Poland",null,"POL",null,null,null,null,null,null,"E"]
["Portugal",null,"PRT"]
["Romania",null,"ROU"]
["Russia",null,"RUS"]
["San Marino",null,"SMR"]
["Serbia",null,"SRB",null,null,null,null,null,null,"E"]
["Slovak Republic",null,"SVK"]
["Slovenia",null,"SVN"]
["Spain",null,"E",null,null,null,null,null,null,"E"]
["Sweden",null,"SWE"]
["Switzerland",null,"CHE"]
["Turkey",null,"TUR",null,null,null,null,null,null,"E"]
["Ukraine",null,"UKR"]
["UK",null,"GBR"]
["Vatican",null,"CVA"]
[]
["Telia",null,"TELIASON",null,null,null,null,null,null,"E"]
["Portugal",null,"POR"]

{"sheet":"Admins analyzes","index":3,"n_rows":1106,"n_cols":55,"rows_kept":1106,"cut":false,"hidden":false,"merged":[[543,27,544,27],[543,28,544,28],[543,19,544,19],[543,20,544,20],[543,21,544,21],[543,25,544,25],[543,26,544,26],[1,4,1,7],[1,8,1,9],[1,10,1,14],[1,15,1,16],[543,4,544,4],[543,12,544,12],[543,13,544,13],[543,14,544,14],[1,18,3,18],[1,19,1,24],[1,25,1,28],[2,8,2,9],[2,10,2,11],[2,19,2,21],[2,22,2,24]]}
[1,{"$f":"A1+1","v":2},{"$f":"B1+1","v":3},4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,{"$f":"AO1+1","v":42},43,44,45,46,47,48,49,50,51,52,53,54,55]
["Respondent","Country code","Band index","Frequency band (MHz)","Licensing regime",null,null,null," Topo-logy",null,"Application",null,null,null,null,"Number of P-P links",null,"Number of CS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends (e.g. in the next 5 years)"]
[null,null,null,null,null,null,null,null,"FWA",null,"Network Infrastruc-ture",null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop length (km)"]
[null,null,null,null,"Link by link","Block","Light licensed","Licence exempt","P-P","P-MP","Mobile backhaul","Others","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","Currently congested","Planned reallocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["Bosnia and Herzegovina","BIH",0,"370-400","X",null,null,null,null,null,null,null,"X",null,null,129,null,null,null,"X",null,null,1,30,100,null,null,null,"370-400 MHz: Planned migration of P-P links to 1350-1375/1492-1517 and 1375-1400/1427-1452 MHz"]
[]
["Bosnia and Herzegovina","BIH",0,"1350-1375 and 1492-1517","X",null,null,null,null,null,null,null,"X",null,null,48,null,null,"T/R 13-01 Annex A","X",null,null,"0.5",7,70,"+15"]
["switzerland","CHE",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,"X",null,null,15,null,"T/R 13-01 Annex A",15,null,null,20,null,30.5,"reduction"]
["Cyprus","CYP",0,"1350-1375 and 1492-1517","X",null,null,null," ",null,null,null,"X",null,null,13,null,null,"T/R 13-01 Annex A","X",null,null,0.9,null,58.65]
["Cyprus","CYP",0,"1350-1375 and 1492-1517","X",null,null,null," ",null,null,null,"X",null,null,17,null,null,null,"X",null,null,0.9,null,73.55]
["Czech Republic","CZE",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"T/R 13-01 Annex A"]
["Denmark","DNK",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Estonia","EST",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Finland","FIN",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A",null,null,null,null,null,null,null,null,null,"Planned opening 2011-2012"]
["France","FRA",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["UK","GBR",0,"1350-1375 and 1492-1517","X",null,null,null,null,null,null,null,null,"X",null,860,null,null,"T/R 13-01 Annex A","X"]
["Croatia","HRV",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Hungary","HUN",0,"1350-1375 and 1492-1517","X",null,null,null,"X","X","X",null,null,null,"Non-Civil P-P, P-MP systems",null,null,null,"T/R 13-01 Annex A",null,null,null,null,null,null,0.1]
["Iceland","ICE",0,"1350-1375 and 1492-1517","x",null,null,null,"X",null,null,null,null,null,null,null,0,null,"T/R 13-01 Annex A",null,null,null,null,null,null,0]
["Ireland","IRL",0,"1350-1375 and 1492-1517"," X",null,null,null,null,null," X",null,null,null,null,0,69,null,"T/R 13-01 Annex A"," X","X","X",0.02,23,83,48,null," X"]
["Ireland","IRL",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009 "]
["Italy","ITA",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Lithuania","LTU",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"T/R 13-01 Annex A"]
["Lithuania","LTU",0,"1350-1375 and 1492-1517",null,"X",null,null,null,"X","X",null,null,null,null,null,null,8,"local",null,null,null,null,null,null,-100]
["Luxembourg","LUX",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"T/R 13-01 Annex A","X",null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Latvia","LVA",0,"1350-1375 and 1492-1517",null,"X",null,null,null,"X",null,null,null,null,null,null,null,30,"national plan","X",null,null,null,null,null,-50]
["Netherlands","NLD",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Norway","NOR",0,"1350-1375 and 1492-1517","X",null,null,null,null,null,null,null,null,"X",null,8,46,null,"T/R 13-01 Annex A","x",null,null,1,12,42]
["Portugal","PRT",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,null,null,null,55,null,"T/R 13-01 Annex A","X",null,null,12,"40",57,5]
["Portugal","PRT",0,"1350-1375 and 1492-1517","X",null,null,null,null,"X",null,null,null,null,null,null,null,9,"T/R 13-01 Annex A","X",null,null,2,"10",18,0]
["Russia","RUS",0,"1350-1375 and 1492-1517","X","X",null,null,null,null,"X",null,null,null,null,null,25,49,"T/R 13-01 Annex A","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Serbia","SRB",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,"X",null,null,52,null,null,"T/R 13-01 Annex A","x",null,null,2,15,52,100,null,null,"From band 1517.5 - 1530 MHz"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517",null,"X",null,null,null,null,null,null,null,"X",null,null,"N/A",null,"T/R 13-01 Annex A","x",null,null,5,20,90,0,"x",null,null,"assigned all SVN (2MHz Ch.1)"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517","X",null,null,null,null,"X","X",null,null,null,null,null,null,17,"T/R 13-01 Annex A","x",null,null,5,15,50,2,"x"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,"X",null,null,null,null,null,20,null,"T/R 13-01 Annex A","x",null,null,5,20,90,10,"x"]
["Telia","TELIASON",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
[]
["Austria","AUT",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,null,8,null,"T/R 13-01 Annex B","x",null,null,3,20,60]
["Bosnia and Herzegovina","BIH",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,null,null,"X",null,null,5,null,null,"T/R 13-01 Annex B","X",null,null,5,20,90,"+15"]
["switzerland","CHE",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,"X",null,null,152,null,"T/R 13-01 Annex B",152,null,null,20,null,61.9,"reduction"]
["Cyprus","CYP",0,"1375-1400 and 1427-1452","X",null,null,null," ",null,null,null,"X",null,null,6,null,null,"T/R 13-01 Annex B","X",null,null,3.52,null,35.47]
["Cyprus","CYP",0,"1375-1400 and 1427-1452","X",null,null,null," ",null,null,null,"X",null,null,8,null,null,null,"X",null,null,22.62,null,74.209999999999994]
["Czech Republic","CZE",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"T/R 13-01 Annex B"]
["Denmark","DNK",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Estonia","EST",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Finland","FIN",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,"X",null,null,null,null,null,4,null,"T/R 13-01 Annex B","X","X",null,null,null,null,null,null,null,"Planned closing 2011-2012"]
["France","FRA",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,null,1259,null,"T/R 13-01 Annex B",1259,null,null,0.1,null,95,"+ 10 %"]
["Croatia","HRV",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Hungary","HUN",0,"1375-1400 and 1427-1452","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"T/R 13-01 Annex B","X",null,null,null,20,null,0.1]
["Hungary","HUN",0,"1375-1400 and 1427-1452","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"X",null,null,null,20]
["Iceland","ICE",0,"1375-1400 and 1427-1452","x",null,null,null,"X",null,null,null,null,null,null,null,2,null,"T/R 13-01 Annex B",null,null,null,null,25,null,0]
["Ireland","IRL",0,"1375-1400 and 1427-1452"," X",null,null,null,null,null," X",null,null,null,null,37,18,null,"T/R 13-01 Annex B"," X",null,null,0.45,23,69," 0",null," X"]
["Ireland","IRL",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009 "]
["Italy","ITA",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Lithuania","LTU",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"T/R 13-01 Annex B"]
["Lithuania","LTU",0,"1375-1400 and 1427-1452",null,"X",null,null,null,"X","X",null,null,null,null,null,null,8,"local",null,null,null,null,null,null,-100]
["Luxembourg","LUX",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"T/R 13-01 Annex B","X",null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Netherlands","NLD",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Netherlands","NLD",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,null,null,null,"X",null,2,7,null,"nat. plan 1427 - 1517","x",null,null,39.299999999999997,58.9,71.400000000000006,10]
["Norway","NOR",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,null,null,null,"X",null,1,26,null,"T/R 13-01 Annex B","x",null,null,1,18,42.5]
["Portugal","PRT",0,"1375-1400 and 1427-1452","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"T/R 13-01 Annex B","X",null,null,null,"40",null,"No use at the moment."]
["Russia","RUS",0,"1375-1400 and 1427-1452","X","X",null,null,null,null,"X",null,null,null,null,null,30,49,"T/R 13-01 Annex B","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Serbia","SRB",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["Slovak Republic","SVK",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovenia","SVN",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,"X",null,null,12,null,null,"T/R 13-01 Annex B","x",null,null,2,15,52,200,null,null,"From band 1517.5 - 1530 MHz"]
["Slovenia","SVN",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,null,1,null,"T/R 13-01 Annex B",null,null,null,5,10,30,200]
["Sweden","SWE",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,null,null,59,99,null,"T/R 13-01 Annex B",null,null,null,null,null,null,null,"N"]
["Telia","TELIASON",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,"X",null,null,null,null,null,17,null,"T/R 13-01 Annex B","X",null,null,4,null,19,0,null,null,null,"IDR140"]
[]
["Italy","ITA",0,"1400-1525","X",null,null,null,null,null,"X",null,null,null,null,null,530,null,"national","X"]
[]
["Slovak Republic","SVK",0,"1427-1530","X",null,null,null,null,"X",null,null,null,null,null,null,null,null,"Rep.CCIR 379-5, DS 65,5MHz","x",null,null,null,null,null,-100,null,"x","no new links"]
["Slovak Republic","SVK",0,"1427-1530",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"relocation to other band"]
[]
["Slovenia","SVN",0,"1517-1525","X",null,null,null,"X",null,null,null,"X",null,null,92,null,null,"national (500kHz)","x",null,null,2,15,52,-50,null,"x","realocated into 1.4 GHz bands"]
["Portugal","PRT",0,"1517-1525","X",null,null,null,null,null,null,null,"X",null,null,365,null,null,"National plan (STL)","X",null,null,null,"15",null,5]
[]
["Slovenia","SVN",0,"1525-1530","X",null,null,null,"X",null,null,null,"X",null,null,6,null,null,"national (500kHz)","x",null,null,2,15,52,-100,null,"x","realocated into 1.4 GHz bands"]
[]
["Greece","GRC",0,"1700-1710 and 1785-1800","X",null,null,null,null,null,null,null,"X",null,null,615,null,null,"national plan","X","X",null,0.4,14,90,null,"congested in urban areas"]
[]
["Austria","AUT",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"T/R 13-01 Annex C"]
["Austria","AUT",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Bosnia and Herzegovina","BIH",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,"X",null,null,27,null,null,"T/R 13-01 Annex C","X",null,null,"1",55,99,"+10"]
["switzerland","CHE",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,"No civil FS use",null,null,null,"T/R 13-01 Annex C"]
["Cyprus","CYP",0,"2025-2110 and 2200-2290",null,null,null," ",null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,"X"]
["Czech Republic","CZE",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X",null,null,null,null,"MD shared",null,null,110,"T/R 13-01 Annex C",null,null,null,null,null,null,0]
["Denmark","DNK",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Estonia","EST",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Finland","FIN",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,"X",null,null,null,null,null,12,null,"T/R 13-01 Annex C","X","X"]
["France","FRA",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["UK","GBR",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,null,"row missing in the questionnaire"]
["Greece","GRC",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,"X",null,null,null,null,null,206,null,"T/R 13-01 Annex C","X","X",null,0.6,21,60,"reduction"]
["Croatia","HRV",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,"X",null,null,182,null,null,"National plan","X",null,null,0.09,8.9,55.6]
["Hungary","HUN",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,"2070-2110 and 2245-2290 MHz Non-Civil digital P-P links",null,3,null,"T/R 13-01 Annex C","X","X",null,null,20]
["Iceland","ICE",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,null,null,90,null,"T/R 13-01 Annex C",45,45,null,20,40,70,0]
["Ireland","IRL",0,"2025-2110 and 2200-2290","X",null,null,null,null,null," X",null,null,null,null,null,47,null,"T/R 13-01 Annex C"," X","X",null,1.5,24,66," 0"]
["Ireland","IRL",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X","X",null,null,null,null,12,21,null,"T/R 13-01 Annex C","x",null,null,6.71,30.92,64.77,0.15]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X","X",null,null,null,null,95,3,null,"T/R 13-01 Annex C",null,"x",null,3.28,52.12,238.26,0.15]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X","X",null,null,null,null,null,122,null,"T/R 13-01 Annex C",null,null,"x",0.49,67.06,238.26,0.15]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X",null,null,null,null,null,null,null,10,"T/R 13-01 Annex C","X",null,null,null,null,null,0.05,"stable"]
["Lithuania","LTU",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,"X",null,null,5,null,"T/R 13-01 Annex C",5]
["Luxembourg","LUX",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Latvia","LVA",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,null,null,3,null,"T/R 13-01 Annex C","X",null,null,5,null,41]
["Netherlands","NLD",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Norway","NOR",0,"2025-2110 and 2200-2290","X","X",null,null,null,null,null,null,null,null,"X",null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,null,"SAP/SAB"]
["Norway","NOR",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,null,"X",null,null,2,null,null,null,"x",null,17,19.7,22,null,null,null,"Offshore"]
["Portugal","PRT",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,"TCR, SAP/SAB",null,11,null,"T/R 13-01 Annex C","X",null,null,2,"40",193,0]
["Portugal","PRT",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,"TCR, SAP/SAB",null,2,null,"National plan",null,"X",null,20,"40",64,0]
["Russia","RUS",0,"2025-2110 and 2200-2290","X","X",null,null,null,null,"X",null,null,null,null,null,73,1,"T/R 13-01 Annex C","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Serbia","SRB",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defense systems"]
["Slovak Republic","SVK",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovenia","SVN",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Sweden","SWE",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Telia","TELIASON",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
[]
["Italy","ITA",0,"2300-2400","X",null,null,null,"X",null,null,null,null,null,null,null,275,null,"national","X"]
[]
["Austria","AUT",0,"3400-3600","X",null,null,null,null,"X","X",null,null,null,null,null,null,240,"ERC/REC 14-03","X",null,null,3,15,30]
["Bosnia and Herzegovina","BIH",0,"3400-3600","X",null,null,null,null,null,"X",null,"X",null,null,9,1,null,"ERC/REC 14-03 Annex B","X","X",null,null,2,null,null,null,null,"3400-3600 MHz: Only two channels are available for P-P links out of FWA systems. We still do not have active implemented FWA systems.\n3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Bosnia and Herzegovina","BIH",0,"3400-3600",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,null,null,"X","X",null,null,null,"+25",null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["switzerland","CHE",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ERC/REC 14-03"]
["Cyprus","CYP",0,"3400-3600","P.C.",null,null,null,null,null,null,null,null,null,null,null,null,null,"2008/411/EC"]
["Czech Republic","CZE",0,"3400-3600","X","X",null,null,"X","X",null,null,null,null,null,null,null,667,"ERC/REC 14-03",null,null,null,null,null,null,100,null,null,"P-MP, FWA planned"]
["Denmark","DNK",0,"3400-3600","X",null,null,null,null,null,null,null,null,null,null,null,null,29,"ERC/REC 14-03"]
["Denmark","DNK",0,"3400-3600",null,"X",null,null,null,null,null,null,null,null,null,null,null,null," ",null,null,null,null,null,null,null,null,null,"No info"]
["Estonia","EST",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,null,null,null,"No info"]
["Finland","FIN",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,540,"ERC/REC 14-03"]
["France","FRA",0,"3400-3600","X","X",null,null,"X","X","X",null,null,null,null,null,236,1135,"ERC/REC 14-03",236,null,null,2,"20<x>80",135,"-30"]
["Germany","GER",0,"3400-3600",null,"x",null,null,null,"x",null,null,null,null,null,null,null,392,"ERC/REC 14-03",null,"x"]
["Greece","GRC",0,"3400-3600",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC 14-03","-",null,null,null,null,null,"4 issued licenses"]
["Croatia","HRV",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,67,"ERC/REC 14-03",null,null,null,null,null,null,-30]
["Hungary","HUN",0,"3400-3600",null," ",null," ",null," ",null,null,null,null,null,null,null,null,"ERC/REC 14-03"]
["Hungary","HUN",0,"3400-3600",null,"X",null,"X",null,"X",null,null,null,null,null,null,null,383,"ECC/DEC/(07)02",null,null,null,null,null,null,"20"]
["Iceland","ICE",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,20,"ERC/REC 14-03",null,null,null,null,10]
["Ireland","IRL",0,"3400-3600"," X",null,null,null,null," X",null,null,null,null,null,null,null,120,"ERC/REC 14-03",null,null,null,null,null,null," 66"]
["Italy","ITA",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,null,null,null,"No info"]
["Lithuania","LTU",0,"3400-3600","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 14-03"]
["Lithuania","LTU",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,402,"ERC/REC 14-03",null,null,null,null,null,null,50,null,null,"Fixed and mobile P-MP (BWA)"]
["Luxembourg","LUX",0,"3400-3600",null,"X",null,null,null,"X","X",null,null,null,null,null,null,3,"Nat. freq. Plan",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,69,"ERC/REC 14-03",null,"X",null,null,10,null,50]
["Netherlands","NLD",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03"]
["Portugal","PRT",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,64,"ERC/REC 14-03","X",null,null,null,"20",null," BWA"]
["Russia","RUS",0,"3400-3600","X","X",null,null,null,"X","X",null,"X",null,null,null,2190,8033,"ERC/REC 14-03","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Serbia","SRB",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,51,"ERC/REC 14-03",null,null,null,null,null,null,50]
["Slovak Republic","SVK",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,198,"ERC/REC 14-03","X",null,null,null,null,null,10]
["Slovenia","SVN",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,"BWA",null,null,10,"ERC/REC 14-03",null,"X",null,5,30,70,400]
["Sweden","SWE",0,"3400-3600",null,"X",null,null,"X","X","X",null,"X",null,"X",null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,"Y","N",null,"IMT-?"]
["Telia","TELIASON",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03"]
[]
["Norway","NOR",0,"3410-3600",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 14-03 Annex A"]
["Norway","NOR",0,"3410-3600","X",null,null,null,null,null,null,null,null,"X",null,null,0]
[]
["Bosnia and Herzegovina","BIH",0,"3600-3800","X",null,null,null,null,null,null,null,"X",null,null,9,null,null,"ERC/REC 12-08",null,"X","X",null,null,null,null,null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Bosnia and Herzegovina","BIH",0,"3600-3800",null,"X",null,null,"X","X",null,null,null,null,null,null,null,65,null,null,null,"X",null,null,null,"+25"]
["Czech Republic","CZE",0,"3600-3800","X",null,null,null,"X",null,null,null,null,null,null,null,150,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,"X","DEC EC/411/EC"]
["Germany","GER",0,"3600-3800",null,"x",null,null,null,"x",null,null,null,null,null,null,null,0,"ERC/REC 14-03",null,"x"]
["Norway","NOR",0,"3600-3800",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-08"]
["Norway","NOR",0,"3600-3800","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Serbia","SRB",0,"3600-3800",null,"X",null,null,null,"X",null,null,null,null,null,null,null,1,"ERC/REC 12-08"]
["Slovenia","SVN",0,"3600-3800","X",null,null,null,"X",null,null,null,"X",null,null,null,2,null,"ERC/REC 12-08",null,null,"X",null,null,null,-100,null,"x","BWA"]
["Slovenia","SVN",0,"3600-3800","X",null,null,null,"X",null,null,null,"X",null,null,1,null,null,"ERC/REC 12-08",null,null,"X",10,45,90,-100,null,"x","BWA"]
["Slovenia","SVN",0,"3600-3800",null,"X",null,null,null,"X",null,null,null,null,"BWA",null,null,"planned","ERC/REC 12-08",null,"X",null,null,null,null,">400",null,null,"BWA"]
[]
["Austria","AUT",0,"3600-4200","X",null,null,null,"X",null,"X",null,null,null,null,null,90,null,"ERC/REC 12-08",null,"X",null,13,50,100]
["switzerland","CHE",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ERC/REC 12-08"]
["Cyprus","CYP",0,"3600-4200","P.C. (3.6-3.8 GHz)",null,null,null,null,null,null,null,null,null,null,null,null,null,"2008/411/EC"]
["Denmark","DNK",0,"3600-4200","X",null,null,null,null,null,null,null,null,null,null,null,null,21,"ERC/REC 12-08"]
["Denmark","DNK",0,"3600-4200",null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No info"]
["Estonia","EST",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"No info"]
["Finland","FIN",0,"3600-4200","X",null,null,null,null,null,"X",null,"X",null,null,null,160,null,"ERC/REC 12-08",null,null,"X"]
["Finland","FIN",0,"3600-4200",null,null,null,null,null,null,null,null,"X",null,null,40,null,null,"National","Analog","Analog",null,null,null,null,null,null,null,"Will be phased out"]
["Finland","FIN",0,"3600-4200","X",null,null,null,null,null,null,null,"X",null,null,120,null,null,"ITU-R F.382","Analog","Analog",null,null,null,null,null,null,null,"Will be phased out"]
["France","FRA",0,"3600-4200","X",null,null,null,"X",null,"X",null,null,null,null,null,11,null,"ERC/REC 12-08",null,null,11,2,"20<x>80",135,"-20"]
["UK","GBR",0,"3600-4200","X",null,null,null,null,null,null,null,null,"X",null,40,null,null,"ERC/REC 12-08",null,"X","X"]
["Croatia","HRV",0,"3600-4200","X",null,null,null,null,null,null,null,"X",null,null,null,9,null,"ERC/REC 12-08",null,"X"]
["Croatia","HRV",0,"3600-4200","X",null,null,null,null,null,"X",null,null,null,null,1,70,null,null,null,null,"X",20.2,44.2,91.4,10]
["Hungary","HUN",0,"3600-4200","X"," ",null," ","X",null,null,null,null,null,null,null,20,null,"ERC/REC 12-08",null,null,"X",null,30,null,"25"]
["Hungary","HUN",0,"3600-4200"]
["Iceland","ICE",0,"3600-4200","X",null,null,null,"X",null,null,null,null,null,null,null,7,null,"ERC/REC 12-08",null,null,7,20,30,40,0]
["Ireland","IRL",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
["Italy","ITA",0,"3600-4200","X",null,null,null,"X",null,"X",null,null,null,null,null,77,null,"ERC/REC 12-08",null,null,"X",13.6,60,238,-5]
["Italy","ITA",0,"3600-4200","X",null,null,null,null,null,"X",null,"X",null,null,105,9,null,"ERC/REC 12-08",null,"X","X",17.46,88.5,238.26,-5]
["Italy","ITA",0,"3600-4200",null,"X",null,null,null,null,"X",null,"X",null,null,null,210,null,"ERC/REC 12-08",null,null,"X",13.6,67.34,238.26,-5]
["Lithuania","LTU",0,"3600-4200","X",null,null,null,"X",null,null,null,null,"X",null,null,30,null,"ERC/REC 12-08",null,null,30]
["Lithuania","LTU",0,"3600-4200",null,"X",null,null,null,"X",null,null,null,"X",null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"3600-3800 future for BWA"]
["Luxembourg","LUX",0,"3600-4200","X",null,null,null,"X",null,"X",null,"X",null,null,1,0,null,"Nat. freq. Plan",null,"X","X",null,"20-80",null,"N/A","NO","NO"]
["Latvia","LVA",0,"3600-4200",null,"X",null,null,null,"X",null,null,null,null,null,null,null,154,"ERC/REC 12-08",null,"X",null,null,10,null,50]
["Netherlands","NLD",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
["Portugal","PRT",0,"3600-4200",null,"X",null,null,null,"X",null,null,null,null,"VSAT (3.8-4.2 GHz)",null,null,null,"ERC/REC 12-08","X","X",null,null,"20",null,null,null,null,"BWA in 3.3 -3.6GHz and FSS in 3.8-4.2GHz"]
["Russia","RUS",0,"3600-4200","X","X",null,null,null,null,"X",null,"X",null,null,null,688,null,"ERC/REC 12-08","X","X","X",40,80,90]
["Russia","RUS",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.635 ITU-R"]
["Slovak Republic","SVK",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"N.A. FWA planned"]
["Sweden","SWE",0,"3600-4200",null,"X",null,null,"X","X","X",null,"X",null,"X",null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,"Y","N",null,"IMT-?"]
["Telia","TELIASON",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
[]
["Bosnia and Herzegovina","BIH",0,"3800-4200","X",null,null,null,null,null,null,null,"X",null,null,11,3,null,"ERC/REC 12-08 Annex B",null,null,null,27,35,85,"+40"]
["Czech Republic","CZE",0,"3800-4200","X",null,null,null,"X",null,null,null,null,null,null,null,479,null,"ERC/REC 12-08"]
["Germany","GER",0,"3800-4200","x",null,null,null,"x",null,null,null,null,null,null,269,null,null,"ERC/REC 12-08",null,null,"x",14.4,42,64.8]
["Greece","GRC",0,"3800-4200","X",null,null,null,null,null,"X",null,null,null,null,null,163,null,"ERC/REC 12-08 Annex B",null,"X","X",5,55,101,"reduction"]
["Norway","NOR",0,"3800-4200",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-08"]
["Norway","NOR",0,"3800-4200","X",null,null,null,null,null,null,null,null,"X",null,null,2,null,null,null,"X",null,2.5,2.7,2.9,null,null,null,null,null,"Offshore"]
["Serbia","SRB",0,"3800-4200","X",null,null,null,null,null,"X",null,null,null,null,null,3,null,"ITU-R F.382-8",null,null,"X",72.09,74.02,77.89]
["Slovenia","SVN",0,"3800-4200","X",null,null,null,"X",null,null,null,"X",null,null,null,18,null,"ERC/REC 12-08",null,null,"X",30,60,90,null,"X*",null,"congested in backbone directions"]
["Slovenia","SVN",0,"3800-4200","X",null,null,null,"X",null,null,null,"X",null,null,18,null,null,"ERC/REC 12-08",null,null,"X",10,30,90,null,"X*",null,"congested in backbone directions"]
[]
["Austria","AUT",0,"4400-5000","X",null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Austria","AUT",0,"4400-5000"]
["switzerland","CHE",0,"4400-5000",null,null,null,null,null,null,null,null,null,null,"No civil FS use"]
["switzerland","CHE",0,"4400-5000"]
["Cyprus","CYP",0,"4400-5000",null,null,null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X"]
["Cyprus","CYP",0,"4400-5000"]
["Czech Republic","CZE",0,"4400-5000",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,null,null,null,null,null,null,null,null,null,null,"civil/MD sharing"]
["Czech Republic","CZE",0,"4400-5000"]
["Hungary","HUN",0,"4400-5000","X",null,null,null,"X","X",null,null,null,null,"Harmonized NATO band type 1. Land military systems, Tactical Radio Relay",null,140,null,null,"X","X","X",null,null,null,null,null,null,"non-civil usage"]
["Hungary","HUN",0,"4400-5000"]
["Latvia","LVA",0,"4400-5000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band"]
["Portugal","PRT",0,"4400-5000",null,null,null,null,null,null,null,null,null,"X","Military"]
["Portugal","PRT",0,"4400-5000"]
["Russia","RUS",0,"4400-5000","X","X",null,null,null,null,"X",null,"X",null,null,null,344,null,"F.382 ITU-R","X","X","X",40,80,90]
["Serbia","SRB",0,"4400-5000",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["Serbia","SRB",0,"4400-5000"]
[]
["Norway","NOR",0,"5725-5795 and 5815-5850",null,null,null,"X",null,null,null,null,null,"X",null,null,null,null,"National plan"]
[]
["Bosnia and Herzegovina","BIH",0,"5850-5925"]
["switzerland","CHE",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast"]
["Cyprus","CYP",0,"5850-5925","X",null,null,null,null,null,null,null,"X",null,null,2,null,null,null,null,"X"," ","PORTABLE"]
["Czech Republic","CZE",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,null,null,null,null,null,null,null,null,null,null,"civil/MD sharing"]
["Denmark","DNK",0,"5850-5925"]
["Estonia","EST",0,"5850-5925"]
["Finland","FIN",0,"5850-5925"]
["France","FRA",0,"5850-5925"]
["Greece","GRC",0,"5850-5925"]
["Croatia","HRV",0,"5850-5925"]
["Hungary","HUN",0,"5850-5925","X",null,null,null,"X","X","X",null,null,null,"Non-Civil BFWA systems",null,null,null,"ECC/DEC/(06)04"]
["Hungary","HUN",0,"5850-5925","X",null,null,null,"X"]
["Iceland","ICE",0,"5850-5925"]
["Ireland","IRL",0,"5850-5925"]
["Italy","ITA",0,"5850-5925","X",null,null,null,"X",null,null,null,"X",null,null,71,null,null,"national",null,null,"x",20,50,238,1,"yes"]
["Italy","ITA",0,"5850-5925",null,"X",null,null,null,null,"X",null,"X",null,null,116,null,null,"national",null,"x",null,9.4700000000000006,61.58,121.23,1,"yes"]
["Lithuania","LTU",0,"5850-5925","X",null,null,null,"X",null,"X",null,null,null,null,null,29,null,null,29]
["Lithuania","LTU",0,"5850-5925",null,null,null,null,null,"X",null,null,null,"X",null,null,null,null,"5/10/20MHz",null,null,null,null,null,null,null,null,null,"5850-5875, 5905-5925 future P-MP"]
["Luxembourg","LUX",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Latvia","LVA",0,"5850-5925",null,"X",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Planning BFWA  within 5725-5875 MHz band. BFWA  5905-5925 MHz"]
["Netherlands","NLD",0,"5850-5925"]
["Netherlands","NLD",0,"5850-5925"]
["Portugal","PRT",0,"5850-5925",null,null,null,"X",null,null,null,null,null,null,"ISM, SRD"]
["Russia","RUS",0,"5850-5925","X","X",null,null,null,"X","X",null,"X",null,null,null,1350,623,null,"X","X","X",30,70,90]
["Serbia","SRB",0,"5850-5925",null,null,null,"X",null,null,null,null,null,null,"X",null,null,null,"ERC/REC 70-03",null,null,null,null,null,null,null,null,null,"SRD"]
["Slovak Republic","SVK",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovenia","SVN",0,"5850-5925"]
["Sweden","SWE",0,"5850-5925"]
["Telia","TELIASON",0,"5850-5925"]
[]
["Latvia","LVA",0,"5925-6245 and  6425-7125","X",null,null,null,"X",null,null,null,null,null,null,null,39,null,"ERC/REC 14-01 ",null,null,"X",22,30,36,100]
["Latvia","LVA",0,"5925-6245 and  6425-7125","X",null,null,null,"X",null,null,null,null,null,null,null,17,null,"ERC/REC 14-02",null,null,"X",28,35,52,100]
[]
["UK","GBR",0,"5925-6425","X",null,null,null,null,null,null,null,null,"X",null,220,null,null,"ERC/REC 14-01 ",null,null,"X"]
["Germany","GER",0,"5925-6425","x",null,null,null,"x",null,null,null,null,null,null,994,null,null,"ERC/REC 14-01",null,null,"x",11.1,40,67.3]
["Slovak Republic","SVK",0,"5925-6425","X",null,null,null,"X",null,"X",null,null,null,null,null,81,null,"ERC/REC 14-01 ",null,null,"X",8.5,20,54,25]
[]
["Slovenia","SVN",0,"5925–6425 ","X",null,null,null,"X",null,"X",null,null,null,null,null,6,null,"ERC/REC 14-01 ",null,null,"X",12,50,75,30]
["Slovenia","SVN",0,"5925–6425 ","X",null,null,null,"X",null,null,null,"X",null,null,null,2,null,"ERC/REC 14-01 ",null,null,null,20,55,65,50]
["Slovenia","SVN",0,"5925–6425 ",null,"X",null,null,"X",null,null,null,"X",null,null,null,4,null,"ERC/REC 14-01 ",null,null,null,5,25,65,0,"x"]
[]
["Austria","AUT",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,336,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",5,45,70]
["Bosnia and Herzegovina","BIH",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,5,302,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",8,60,134,null,"X"]
["Switzerland","CHE",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,60,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,60,30,39.700000000000003,81.7,"growth"]
["Cyprus","CYP",0,"5925-7125","X",null,null,null,null,null,"X",null,"X",null,null,17,27,null,"ERC/REC 14-01 and ERC/REC 14-02","X","X"," ",7.19,null,53]
["Czech Republic","CZE",0,"5925-7125","X",null,null,null,"X",null,null,null,null,null,null,null,1642,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Denmark","DNK",0,"5925-7125","X",null,null,null,null,null,null,null,null,null,null,null,22,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Estonia","EST",0,"5925-7125",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Finland","FIN",0,"5925-7125","X",null,null,null,null,null,"X",null,"X",null,null,null,160,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",10,30,63,0.8]
["France","FRA",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,3491,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,3491,0.5,"20-80",105,"+ 5 % ","X"]
["Greece","GRC",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,638,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",8,45,102,"stable"]
["Croatia","HRV",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,98,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",10.7,34.1,70.8,20,"x"]
["Hungary","HUN",0,"5925-7125","X",null,null,null,"X",null,null,null,null,null,null,null,299,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,null,null,null,null,0.1]
["Iceland","ICE",0,"5925-7125","X",null,null,null,"X",null,null,null,"X",null,null,6,16,null,"ERC/REC 14-01 and ERC/REC 14-02",3,null,15,10,30,50,0]
["Ireland","IRL",0,"5925-7125"," X",null,null,null,null,null," X",null,null,null,null,2,356,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null," X",8,40,90," 28"]
["Italy","ITA",0,"5925-7125","X",null,null,null,"X",null,"X",null,"X",null,null,102,808,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",6.32,44,83,0.15,"almost"]
["Lithuania","LTU",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,137,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Lithuania","LTU",0,"5925-7125",null,null,null,null,null,"X",null,null,null,"X",null,null,null,null,"5/10/20MHz",null,null,null,null,null,null,null,null,null,"5925-6425 future for P-MP"]
["Luxembourg","LUX",0,"5925-7125","X",null,null,null,"X",null,"X",null,"X",null,null,10,2,null,"ERC/REC 14-01 and ERC/REC 14-02 and national plan",null,"X","X",3.4,"20-80",63,"N/A","NO","NO"]
["Netherlands","NLD",0,"5925-7125","X",null,null,null,null,null,null,null,null,"X",null,null,51,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",21.41,31.11,49.3,20]
["Norway","NOR",0,"5925-7125","X","X",null,null,null,null,null,null,null,"X",null,null,146,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",2.8,37.5,123]
["Portugal","PRT",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,"VSAT, SRD",2,8,null,"ERC/REC 14-01 ",null,"X","X",40,40,88,50]
["Portugal","PRT",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,"VSAT, SRD",null,59,null,"ERC/REC 14-02",null,"X","X",15,40,84,10]
["Russia","RUS",0,"5925-7125","X","X",null,null,"X","X","X",null,"X",null,null,null,3411,1942,"ERC/REC 14-01 and ERC/REC 14-02","X","X","X",30,55,65]
["Russia","RUS",0,"5925-7125",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.383 ITU-R"]
["Serbia","SRB",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,205,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",17,45,79,30]
["Sweden","SWE",0,"5925-7125","X",null,null,null,"X",null,null,null,null,null,null,null,952,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,null,null,null,null,null,"Y"]
["Telia","TELIASON",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,19,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,19,6,null,40,null,"X"]
[]
["UK","GBR",0,"6425-7125","X",null,null,null,null,null,null,null,null,"X",null,330,null,null,"ERC/REC 14-02",null,"X","X"]
["Germany","GER",0,"6425-7125","x",null,null,null,"x",null,null,null,null,null,null,2565,null,null,"ERC/REC 14-02",null,null,"x",4.3,30,103.9]
["Slovenia","SVN",0,"6425-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,14,null,"ERC/REC 14-02",null,null,"X",20,40,50,50]
[]
["Slovak Republic","SVK",0,"6430-7110","X",null,null,null,"X",null,"X",null,null,null,null,null,2,null,"ERC/REC 14-02",null,null,"X",44,49,54,"0-100 ",null,null,"expected growth"]
[]
["Germany","GER",0,"7125-7425","x",null,null,null,"x",null,null,null,null,null,null,917,null,null,"ECC REC (02)06",null,"x",null,4.2,28,89.9]
["Norway","NOR",0,"7125-7425","X",null,null,null,null,null,null,null,null,"X",null,null,135,null,null,null,null,"X",4.2,35.5,96]
["Slovak Republic","SVK",0,"7125-7425","X",null,null,null,"X",null,"X",null,null,null,null,null,30,null,"ECC REC (02)06",null,null,"X",17,25,44.5,50]
["Slovak Republic","SVK",0,"7125-7425","X",null,null,null,"X",null,"X",null,null,null,null,null,14,null,"ITU-R F.385, DS 161MHz","X","X",null,7,25,58,-100,null,"x","no new links"]
["Slovenia","SVN",0,"7125-7425","X",null,null,null,"X",null,"X",null,null,null,null,null,23,null,"ECC REC (02)06",null,null,"X",10,25,45,10,"x"]
["Slovenia","SVN",0,"7125-7425","X",null,null,null,"X",null,null,null,"X",null,null,null,43,null,"ECC REC (02)06",null,null,"X",5,25,65,5,"x"]
[]
["Serbia","SRB",0,"7125-7725","X",null,null,null,null,null,"X",null,null,null,null,null,138,null,"ITU-R F.385-9 base","X","X","X",11.67,37.979999999999997,104.2,150]
[]
["Telia","TELIASON",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,22,null,"ECC REC (02)06",null,22,null,15,null,42,null,"X",null,null,"NEC 770"]
["Telia","TELIASON",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,128,null,null,74,54,null,7,null,80,null,"X",null,null,"Eric sson ML"]
["Austria","AUT",0,"7125-7750","X",null,null,null,"X",null,null,null,null,null,null,null,570,null,"ECC REC (02)06",null,"X","X",1,40,78]
["Bosnia and Herzegovina","BIH",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,113,null,"ECC REC (02)06",null,"X","X",4,40,90,null,"X"]
["Bosnia and Herzegovina","BIH",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,10,62,null,"ITU-R F.385",null,"X","X"]
["Croatia","HRV",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,171,null,"Bands 7125 - 7425 and 7425 - 7725 with diff. ch. arrangements",null,"X","X",3.8,37.700000000000003,91.4,30,"x"]
["Czech Republic","CZE",0,"7125-7750","X",null,null,null,"X",null,null,null,null,null,null,null,1050,null,"ECC REC (02)06",null,null,null,null,null,null,null,null,"x","civil/MD sharing"]
["Cyprus","CYP",0,"7125-7750","X",null,null,null,null,null,"X",null,"x",null,null,8,48,null,"ECC REC (02)06","X","X"," ",0.49,null,63.77]
["Denmark","DNK",0,"7125-7750","X",null,null,null,null,null,null,null,null,null,null,null,225,null,"ECC REC (02)06",null,null,null,20]
["Estonia","EST",0,"7125-7750",null,null,null,null,null,null,null,null,null,null,null,null,62,null,"ECC REC (02)06",null,62,null,17,35,81]
["Finland","FIN",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,130,null,"ITU-R F.385",null,"X","X",13,36,65,0.05]
["Finland","FIN",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,330,null,"National (ITU-R F.385 mod.)",null,"X","X",2,27,70,0.1]
["France","FRA",0,"7125-7750",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["Hungary","HUN",0,"7125-7750","X",null,null,null,"X",null,null,null,"X",null,"7125-7250 MHz Non-Civil P-P links;  7125-7425 MHz Emergency Services\n7425-7725 MHz Civil P-P links 7725-7750 MHz Civil broadcasting infrastructure",null,171,null,"ECC REC (02)06","X","X","X",null,20]
["Hungary","HUN",0,"7125-7750",null,null,null,null,null,null,null,null,null,null,"7250-7750 MHz Satellite Systems downlink (military); Harmonized NATO band type 1."]
["Iceland","ICE",0,"7125-7750","X",null,null,null,"X",null,null,null,"X",null,null,23,65,null,"ECC REC (02)06",32,28,28,10,30,60,0]
["Ireland","IRL",0,"7125-7750"," X",null,null,null,null,null," X",null,null,null,null,1,279,null,"ECC REC (02)06"," X","X","X",7,36,76," 57"]
["Lithuania","LTU",0,"7125-7750","X",null,null,null,"X",null,null,null,null,null,null,null,197,null,"ECC REC (02)06"]
["Luxembourg","LUX",0,"7125-7750","X",null,null,null,"X",null,"X",null,"X",null,null,0,26,null,"ECC REC (02)06",null,"X","X",7.9,"20-80",55.9,"N/A","NO","NO"]
["Netherlands","NLD",0,"7125-7750","X",null,null,null,null,null,null,null,null,"X",null,null,113,null,"ECC REC (02)06","X","X","X",10.4,27.7,55.6,20]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS, Military (7.25-7.3 GHz)",null,7,null,"7 LOW: ITU-R F.385","X",null,null,15,"30",53,0]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS, Military (7.25-7.3 GHz)",null,287,null,"7 LOW: ECC REC (02)06","X","X","X",6,"30",63,10]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,40,null,"7 HIGH: ITU-R F.385","X","X",null,3,"22",71,-50]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,30,null,"7 HIGH: ECC REC (02)06","X","X","X",15,"30",78,50]
["Russia","RUS",0,"7125-7750","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",10495,null,"F.385 ITU-R","X","X","X",30,55,65]
["Switzerland","CHE",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,null,null,171,null,"ECC REC (02)06",70,81,20,20,30.2,99.5,"growth"]
[]
["Latvia","LVA",0,"7125-7800","X",null,null,null,"X",null,null,null,null,null,null,null,104,null,"ITU-R F.385",null,null,"X",14,35,54,50,null,null,"Military band 7250-7331 MHz"]
[]
["Slovenia","SVN",0,"7425–7725","X",null,null,null,"X",null,"X",null,null,null,null,null,26,null,"ECC REC (02)06",null,null,"X",10,25,45,20]
["Slovenia","SVN",0,"7425–7725","X",null,null,null,"X",null,null,null,"X",null,null,null,5,null,"ECC REC (02)06",null,null,"X",3,25,60,30]
[]
["Germany","GER",0,"7425-7725","x",null,null,null,"x",null,null,null,null,null,null,3157,null,null,"ECC REC (02)06",null,null,"x",5.5,26,71.099999999999994,null,"x"]
["Norway","NOR",0,"7425-7725","X",null,null,null,null,null,null,null,null,"X",null,null,446,null,null,null,null,"X",1.2,32.299999999999997,113]
["Slovak Republic","SVK",0,"7425-7725","X",null,null,null,"X",null,"X",null,null,null,null,null,70,null,"ITU-R F.385-9, DS 161MHz","X","X",null,5,25,55,10]
["Sweden","SWE",0,"7425-7725","X",null,null,null,"X",null,null,null,null,null,null,null,1421,null,null,null,"X",null,null,null,null,null,"Y"]
["Greece","GRC",0,"7425-7725","X",null,null,null,null,null,"X",null,null,null,null,null,1222,null,"ECC REC (02)06 Annex1","X","X","X",1,31,98,0.1]
[]
["UK","GBR",0,"7425-7900","X",null,null,null,null,null,null,null,null,"X",null,940,null,null,"ITU-R F.385-9","X","X","X"]
[]
["Slovak Republic","SVK",0,"7700-8300","X",null,null,null,"X",null,"X",null,null,null,null,null,35,null,"ITU-R F.386-4, Annex 1",null,null,"X",8,30,58,-100,null,"x","no new links"]
[]
["Slovenia","SVN",0,"7725–8275","X",null,null,null,"X",null,null,null,"X",null,null,6,42,null,"ITU-R F 386-8 An6  (29.65 MHz, DS 311.32 MHz)",null,null,"X",15,35,60,5,"x*",null,"congested in backbone directions"]
["Bosnia and Herzegovina","BIH",0,"7725–8275","X",null,null,null,null,null,"X",null,"X",null,null,34,143,null,"ITU-R F.386, Annex 6",null,"X","X",4,38,83,null,"X",null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Serbia","SRB",0,"7725–8275","X",null,null,null,null,null,"X",null,null,null,null,null,8,null,"ITU-R F.386-8 annex 6",null,"X","X",9.44,35.68,70.27,300]
["Greece","GRC",0,"7725–8275","X",null,null,null,null,null,"X",null,null,null,null,null,1157,null,"ITU-R F. 386-6 Annex 1",null,"X","X",2,40,150,0.1]
[]
["Telia","TELIASON",0,"7750-7900"]
["Austria","AUT",0,"7750-7900",null,null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Croatia","HRV",0,"7750-7900","X",null,null,null,null,null,"X",null,"X",null,null,null,146,null,"Band 7725 - 8275",null,null,"X",21.1,50.3,91.4,null,"x"]
["Czech Republic","CZE",0,"7750-7900",null,null,null,null,null,null,null,null,null,null,"MD"]
["Cyprus","CYP",0,"7750-7900",null,null,null," "]
["Denmark","DNK",0,"7750-7900"]
["Estonia","EST",0,"7750-7900"]
["Finland","FIN",0,"7750-7900","X",null,null,null,null,null,null,null,"X",null,null,45,7,null,"National  ",null,"X"]
["France","FRA",0,"7750-7900"]
["Hungary","HUN",0,"7750-7900","X",null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,40,null,0.15]
["Iceland","ICE",0,"7750-7900"]
["Ireland","IRL",0,"7750-7900"]
["Italy","ITA",0,"7750-7900"]
["Lithuania","LTU",0,"7750-7900","X",null,null,null,"X",null,null,null,null,null,null,null,0,null,"local"]
["Luxembourg","LUX",0,"7750-7900","X",null,null,null,"X",null,"X",null,"X",null,null,0,0,null,"Nat. freq. plan",null,"X","X",null,null,null,"N/A","NO","NO"]
["Netherlands","NLD",0,"7750-7900"]
["Portugal","PRT",0,"7750-7900","X",null,null,null,"X",null,"X",null,null,null,null,null,26,null,"8 LOW: ITU-R F.386",null,"X","X",2,"30",75,50]
["Russia","RUS",0,"7750-7900","No","No"]
["Switzerland","CHE",0,"7750-7900",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast"]
[]
["Latvia","LVA",0,"7800-7900",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band 7850-7900 MHz"]
[]
["Norway","NOR",0,"7900-8200",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ECC REC (02)06"]
[]
["Telia","TELIASON",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,8,null,"ECC REC (02)06",null,8,null,16,null,68,null,"X",null,null,"NEC 770"]
["Telia","TELIASON",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,37,null,null,null,11,26,13,null,68,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,1,null,null,null,null,1,null,34,null,"++",null,null,null,"Ericsson TN"]
["Austria","AUT",0,"7900-8500","X",null,null,null,"X",null,"X",null,"X",null,null,null,73,null,"ECC REC (02)06",null,"X","X",1,35,60]
["Croatia","HRV",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,14,null,"Band 8275 - 8500",null,"X",null,7.5,20.100000000000001,31.4]
["Czech Republic","CZE",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"ECC REC (02)06"]
["Cyprus","CYP",0,"7900-8500","X",null,null,null,null,null,null,null,"X",null,null,14,null,null,"ECC REC (02)06","X","X"," ",8.2899999999999991,null,40.020000000000003]
["Denmark","DNK",0,"7900-8500","X",null,null,null,null,null,null,null,null,null,null,null,4," ","ECC REC (02)06",null,null,null,20]
["Estonia","EST",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,45,null,"ECC REC (02)06",null,45,null,15,35,40,"+20"]
["Finland","FIN",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["France","FRA",0,"7900-8500","X",null,null,null,"X",null,"X",null,null,null,null,null,2529,null,"ECC REC (02)06",1322,947,260,0.04,"15<x>60",105,"- 10 %"]
["France","FRA",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UIT-RF-386-4"]
["Hungary","HUN",0,"7900-8500","X",null,null,null,null,null,null,null,null,null,"7900-8400 MHz Satellite Systems uplink (military); Harmonized NATO band type 1.",null,null,null,"ECC REC (02)06"]
["Hungary","HUN",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,3,null,null,"X","X",null,null,20]
["Iceland","ICE",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["Ireland","IRL",0,"7900-8500"," X",null,null,null,null,null," X",null,null,null,null,null,315,null,"ECC REC (02)06"," X","X","X",5,36,81," 48"]
["Italy","ITA",0,"7900-8500","X",null,null,null,"X",null,"X",null,null,null,null,null,2231,null,"national",null,"X","X",null,30,null,0.1,"almost"]
["Italy","ITA",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,5,null,"national",null,null,"X"]
["Latvia","LVA",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,152,null,"ECC REC (02)06",null,null,"X",12,35,50,50,null,null,"Military band 7975-8024 MHz"]
["Lithuania","LTU",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,116,null,"ECC REC (02)06"]
["Luxembourg","LUX",0,"7900-8500","X",null,null,null,"X",null,"X",null,"X",null,null,4,6,null,"ECC REC (02)06",null,"X","X",5.0999999999999996,"20-80",62,"N/A","NO","NO"]
["Netherlands","NLD",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["Portugal","PRT",0,"7900-8500","X",null,null,null,"X",null,null,null,"X",null,"FSS, EESS, Military (7.975-8.025 GHz)",7,9,null,"8 HIGH: ITU-R F.386","X",null,null,6,"40",88,-100]
["Russia","RUS",0,"7900-8500","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",4584,null,"F.386 ITU-R","X","X","X",30,55,65]
["Sweden","SWE",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,494,null,"ECC REC (02)06",null,"X",null,null,null,null,"Y","N"]
["Switzerland","CHE",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ECC REC (02)06"]
[]
["Bosnia and Herzegovina","BIH",0,"8275-8500","X",null,null,null,null,null,"X",null,null,null,null,null,17,null,"ITU-R F.386, Annex 2",null,"X",null,7,25,65,null,"X"]
["Serbia","SRB",0,"8275-8500","X",null,null,null,null,null,"X",null,null,null,null,null,10,null,"ITU-R F.386-8 annex 2",null,"X","X",21,53.77,98.71,300]
["Slovenia","SVN",0,"8275-8500","X",null,null,null,"X",null,"X",null,null,null,null,null,14,null,"ITU-R F.386-8 An2 (28 MHz , DS 119 MHz, 14 MHz, DS 126 MHz)",null,"X",null,20,35,70,30,"x*",null,"congested in backbone directions"]
[]
["Greece","GRC",0,"8275-8500 ","X",null,null,null,null,null,"X",null,null,null,null,null,170,null,"ITU-R F. 386-6 Annex 3","X","X",null,1.8,47,120,"stable"]
[]
["Austria","AUT",0,"10000-10680","X",null,null,null,"X",null,"X",null,null,null,null,null,158,null,"ERC/REC 12-05",null,"x",null,1,30,80]
["Bosnia and Herzegovina","BIH",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,103,null,null,"ERC/REC 12-05","X","X",null,1,27,80,"+15",null,null,"10000-10680 MHz: Shared band between P-P links and FWA. We still do not have active implemented FWA systems."]
["Bosnia and Herzegovina","BIH",0,"10000-10680",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC 12-05 Annex A"]
["Switzerland","CHE",0,"10000-10680","X",null,null,null,"X",null,"X",null,null,null,null,null,64,null,"ERC/REC 12-05",18,46,null,15,18.3,48.5,"growth"]
["Cyprus","CYP",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,56,null,null,"ERC/REC 12-05","X","X"," ",0.53,null,70]
["Czech Republic","CZE",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"ERC/REC 12-05"]
["Czech Republic","CZE",0,"10000-10680","X",null,null,"X","X",null,null,null,null,null,null,null,21]
["Denmark","DNK",0,"10000-10680","X",null,null,null,null,null,null,null,null,null,null,null,null,47,"ERC/REC 12-05"]
["Denmark","DNK",0,"10000-10680",null,"X",null,null,null,null,null,null,null,null,null,null,"No info"]
["Denmark","DNK",0,"10000-10680","X",null,null,null,null,null,null,null,null,null,null,null,1]
["Estonia","EST",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Finland","FIN",0,"10000-10680","X",null,null,null,null,"X",null,null,null,null,null,null,null,11,"ERC/REC 12-05",null,"X"]
["France","FRA",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["UK","GBR",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Greece","GRC",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,107,null,null,"national plan",null,null,null,1.2,19,75]
["Croatia","HRV",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,2,null,null,"ERC/REC 12-05",null,"x"]
["Croatia","HRV",0,"10000-10680",null,"X",null,null,null,"X"]
["Hungary","HUN",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,93,null,null,"ERC/REC 12-05",null,null,null,null,40]
["Iceland","ICE",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Ireland","IRL",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Ireland","IRL",0,"10000-10680"," X",null,null,null," X",null,null,null,null,null,null,null,null,30,"National Legislation: S.I. 79 of 2003\nNational Legislation: S.I. 530 of 2003 European Legislation: Decision 2008/411/EC ",null,null,null,null,null,null," 75"]
["Italy","ITA",0,"10000-10680","X",null,null,null,null,null,"X",null,"X",null,null,{"$f":"935+529+446","v":1910},34,null,"ERC/REC 12-05",null,"X",null,3,25,84,1,"yes"]
["Italy","ITA",0,"10000-10680","X",null,null,null,null,null,"X",null,"X",null,null,{"$f":"236+24","v":260},80,null,"ERC/REC 12-05",null,null,"x",5.5,35,50,1,"yes"]
["Luxembourg","LUX",0,"10000-10680","X",null,null,null,"X",null,"X",null,"X",null,null,2,0,null,"ERC/REC 12-05",null,"X","X",32,"10-50",62,"N/A","NO","NO"]
["Luxembourg","LUX",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"10000-10680","X",null,null,null,"X",null,null,null,null,null,null,null,105,null,"ERC/REC 12-05","X",null,null,null,null,null,-80,null,null,"10300-10500 MHz"]
["Latvia","LVA",0,"10000-10680",null,"X",null,null,null,"X",null,null,null,null,null,null,null,66,"ERC/REC 12-05 and ERC/REC 13-04",null,"X",null,null,10,null,50]
["Netherlands","NLD",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Norway","NOR",0,"10000-10680",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-05"]
["Portugal","PRT",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,"AM, SAP/SAB, SRD",null,null,null,"ERC/REC 12-05"]
["Russia","RUS",0,"10000-10680","X","X",null,null,null,"X","X",null,"X",null,null,"less than 1%",247,1490,"ERC/REC 12-05","X","X","X",15,30,40]
["Serbia","SRB",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,76,3,null,"national plan","X",null,null,0.7,24.72,114.99,20]
["Slovak Republic","SVK",0,"10000-10680",null,"X",null,null,null,"X",null,null,null,null,null,null,null,110,"ERC/REC 12-05","x","x",null,null,null,null,10]
["Slovenia","SVN",0,"10000-10680","X",null,null,null,"X",null,null,null,"X",null,null,53,null,null,"ERC/REC 12-05",null,"x","x",2,25,65,-100,null,"x","BWA when SAP/SAB P to P video links analogue cease operation"]
["Slovenia","SVN",0,"10000-10680","X",null,null,null,"X",null,null,null,"X",null,null,null,8,null,"ERC/REC 12-05",null,"x","x",2,25,62,-100,null,"x","BWA when SAP/SAB P to P video links analogue cease operation"]
["Sweden","SWE",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05\nNew ITU-R Rec under dev.",null,null,null,null,null,null,"Y","N",null,"Blockassignment?"]
["Telia","TELIASON",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
[]
["Lithuania","LTU",0,"10150-10300 and 10500-10650","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-05"]
["Lithuania","LTU",0,"10150-10300 and 10500-10650",null,"X",null,null,null,"X",null,null,null,null,null,null,null,6,"ERC/REC 12-05",null,null,null,null,null,null,100]
[]
["Lithuania","LTU",0,"10300-10500","X",null,null,null,"X",null,"X",null,null,null,null,null,420,null,"ERC/REC 12-05",420]
[]
["Austria","AUT",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,21,null,"ERC/REC 12-06"]
["Bosnia and Herzegovina","BIH",0,"10700-11700","X",null,null,null,null,null,"X",null,"X",null,null,37,38,null,"ERC/REC 12-06","X","X",null,1,25,64,"+15",null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Switzerland","CHE",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,80,null,"ERC/REC 12-06",null,null,80,10,14.9,34.9,"growth",null,null,"heavily used by FSS"]
["Cyprus","CYP",0,"10700-11700","X",null,null,null,null,null,"X",null,"X",null,null,3,30,null,"ERC/REC 12-06",null,"X"," ",2.0099999999999998,null,34.130000000000003]
["Czech Republic","CZE",0,"10700-11700","X",null,null,null,null,"X",null,null,null,null,null,null,null,1845,"ERC/REC 12-06",null,null,null,null,null,null,20]
["Denmark","DNK",0,"10700-11700","X",null,null,null,null,null,null,null,null,null,null,null,null,1,"ERC/REC 12-06"]
["Estonia","EST",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Finland","FIN",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["France","FRA",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,524,null,"ERC/REC 12-06",null,null,524,1.5,"15<x>50",46,"+ 26 %"]
["Greece","GRC",0,"10700-11700","X",null,null,null,null,null,"X",null,null,null,null,null,785,null,"ERC/REC 12-06",null,null,"X",1.7,19,63,0.3]
["Croatia","HRV",0,"10700-11700","X",null,null,null,null,null,"X",null,null,null,null,null,8,null,"ERC/REC 12-06",null,null,"x",7.5,20.2,29.8]
["Hungary","HUN",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Hungary","HUN",0,"10700-11700","X",null,null,null,"X",null,null,null,null,null,null,null,186,null,"ERC/DEC/(00)08",null,null,"X",null,14]
["Iceland","ICE",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Ireland","IRL",0,"10700-11700"," X",null,null,null,null,null,"X",null,null,null,null,null,648,null,"ERC/REC 12-06",null,"X","X",1.5,24,56," 39"]
["Ireland","IRL",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null," National Legislation: S.I. 370 of 2009"]
["Italy","ITA",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,3110,null,"ERC/REC 12-06",null,"X","X",null,18,null,0.15,"yes"]
["Italy","ITA",0,"10700-11700","X",null,null,null,null,null,"X",null,"X",null,null,58,99,null,"ERC/REC 12-06",null,"X","X",3,22,60,0.15,"yes"]
["Lithuania","LTU",0,"10700-11700","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 12-06"]
["Luxembourg","LUX",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Latvia","LVA",0,"10700-11700","X",null,null,null,null,null,null,null,"X",null,null,38,null,null,"ITU-R F.387",null,null,null,0.3,10,32,-50,null,null,"Analog fixed links"]
["Netherlands","NLD",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Norway","NOR",0,"10700-11700",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ITU rec F.387-10"]
["Norway","NOR",0,"10700-11700","X",null,null,null,null,null,null,null,null,"X",null,null,234,null,null,null,null,"x",0.5,23,66.5]
["Portugal","PRT",0,"10700-11700","X",null,null,null,"X",null,"X",null,"X",null,"FSS, VSAT, SNG, SIT, AES, Euteltracs",null,117,null,"ERC/REC 12-06",null,"X","X",2,"20",41,5]
["Russia","RUS",0,"10700-11700","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",1207,null,"ERC/REC 12-06","X","X","X",15,30,40]
["Russia","RUS",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.387 ITU-R"]
["Serbia","SRB",0,"10700-11700","X",null,null,null,null,null,"X",null,null,null,null,null,48,null,"ERC/REC 12-06",null,null,"X",7.13,15.72,37.700000000000003,300]
["Slovak Republic","SVK",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,0,null,"ERC/REC 12-06",null,null,"x",null,null,null,100,null,null,"operation expected"]
["Slovenia","SVN",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,13,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",7,40,46,50,null,null,null,"In accordance with CEPT and ITU limitations"]
["Slovenia","SVN",0,"10700-11700","X",null,null,null,"X",null,null,null,"X",null,null,3,null,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",35,40,46,5,null,null,null,"In accordance with CEPT and ITU limitations"]
["Slovenia","SVN",0,"10700-11700","X",null,null,null,"X",null,null,null,"X",null,null,null,3,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",33,40,47,5,null,null,null,"In accordance with CEPT and ITU limitations"]
["Sweden","SWE",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,7,1,null,"ERC/REC 12-06"]
["Telia","TELIASON",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
[]
["Austria","AUT",0,"11700-12500"]
["Bosnia and Herzegovina","BIH",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/DEC(00)08"]
["Bosnia and Herzegovina","BIH",0,"11700-12500",null,"X",null,null,null,null,null,null,"X",null,null,null,null,16,null,null,null,null,null,null,null,"+10"]
["Switzerland","CHE",0,"11700-12500"]
["Cyprus","CYP",0,"11700-12500","X",null,null,null,null,null,null,null,"X",null,null,10,null,null,null,null,"X"," ",2.75,null,30.18]
["Czech Republic","CZE",0,"11700-12500","X",null,null,null,"X",null,null,null,null,null,null,31,null,null,null,null,null,null,null,null,null,10]
["Denmark","DNK",0,"11700-12500"]
["Estonia","EST",0,"11700-12500"]
["Finland","FIN",0,"11700-12500"]
["France","FRA",0,"11700-12500"]
["UK","GBR",0,"11700-12500"]
["Greece","GRC",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Croatia","HRV",0,"11700-12500"]
["Hungary","HUN",0,"11700-12500",null,null,null,"X",null,null,null,null,"X",null,null,null,null,144,null,null,null,null,null,null,null,null,"x"]
["Iceland","ICE",0,"11700-12500"]
["Ireland","IRL",0,"11700-12500"]
["Italy","ITA",0,"11700-12500","X",null,null,null,null,null,"X",null,null,null,null,22,1,null,null,null,"x",null,1.97,27.6,62.94]
["Lithuania","LTU",0,"11700-12500"]
["Luxembourg","LUX",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Latvia","LVA",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BROADCASTING-SATELLITE"]
["Netherlands","NLD",0,"11700-12500"]
["Portugal","PRT",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,"RAD-S, SIT"]
["Russia","RUS",0,"11700-12500","No","No"]
["Serbia","SRB",0,"11700-12500",null,"X",null,null,null,null,null,null,"X",null,null,null,null,15,null,null,null,"X"]
["Slovak Republic","SVK",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovenia","SVN",0,"11700-12500",null,"X",null,null,null,"X",null,null,null,null,"MMDS",null,null,20,"National (200/400 MHz)",null,null,"x",5,30,40,10,null,null,null,"assigned for local/regional coverage"]
["Sweden","SWE",0,"11700-12500"]
["Telia","TELIASON",0,"11700-12500"]
[]
["Telia","TELIASON",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,302,null,"ERC/REC 12-02",210,null,92,3,null,50,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,22,null,null,null,null,22,9,null,42,"-",null,null,null,"NERA Citylink"]
["Telia","TELIASON",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,80,null,null,32,48,null,5,null,29,0,null,null,null,"Eric sson ML"]
["Austria","AUT",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,137,null,"ERC/REC 12-02",null,null,"x",3,25,52]
["Bosnia and Herzegovina","BIH",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,31,null,"ERC/REC 12-02","X","X","X",2,20,34,"+15"]
["Croatia","HRV",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,244,null,"ERC/REC 12-02",null,"x",null,1.5,19.2,49.2,20,"x"]
["Croatia","HRV",0,"12750-13250","X",null,null,null,null,null,null,null,"X",null,null,1]
["Czech Republic","CZE",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,1288,null,"ERC/REC 12-02",null,null,null,null,null,null,10]
["Cyprus","CYP",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,278,null,"ERC/REC 12-02","X","X"," ",0.28999999999999998,null,40.94,null,"X"]
["Denmark","DNK",0,"12750-13250","X",null,null,null,null,null,null,null,null,null,null,null,4,null,"ERC/REC 12-02",null,null,null,12]
["Estonia","EST",0,"12750-13250",null,null,null,null,null,null,null,null,null,null,null,null,80,null,"ERC/REC 12-02",null,80,null,11,22,34]
["Finland","FIN",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,2120,null,"ERC/REC 12-02",null,"X","X",0.4,14,49,0.2,"x",null,"Local congestion"]
["France","FRA",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,6613,null,"ERC/REC 12-02",2401,3711,501,0.1,"5<x>35",103,"+ 2 %","X"]
["Germany","GER",0,"12750-13250","x",null,null,null,"x",null,null,null,null,null,null,4100,null,null,"ERC/REC 12-02",null,null,"x",0.99,12,48.5]
["Greece","GRC",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,1004,null,"ERC/REC 12-02","X","X","X",1.5,16,55,0.5]
["Hungary","HUN",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,1710,null,"ERC/REC 12-02",null,"X",null,null,12,null,null,"x"]
["Iceland","ICE",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,12,null,"ERC/REC 12-02",null,6,6,10,20,30,0]
["Ireland","IRL",0,"12750-13250"," X",null,null,null,null,null,"X",null,null,null,null,2,1078,null,"ERC/REC 12-02","X","X","X",1.5,19,53," 27"," X"]
["Ireland","IRL",0,"12750-13250",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Italy","ITA",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,6106,null,"ERC/REC 12-02",null,"X","X",7,16,30,0.15,"yes"]
["Latvia","LVA",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,630,null,"ERC/REC 12-02",null,"X",null,2,35,47,20]
["Latvia","LVA",0,"12750-13250",null,"X",null,null,null,null,null,null,"X",null,null,null,null,7,"national plan","X",null,null,null,5,null,null,null,null,"MMDS"]
["Lithuania","LTU",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,222,null,"ERC/REC 12-02"]
["Luxembourg","LUX",0,"12750-13250","X",null,null,null,"X",null,"X",null,"X",null,null,8,22,null,"ERC/REC 12-02",null,"X","X",5.6,"5-35",32,"N/A","NO","NO"]
["Luxembourg","LUX",0,"12750-13250",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Netherlands","NLD",0,"12750-13250","X",null,null,null,null,null,null,null,null,"X",null,null,201,null,"ERC/REC 12-02",null,"X","X",8.35,18.2,31.5]
["Norway","NOR",0,"12750-13250",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-02"]
["Norway","NOR",0,"12750-13250","X",null,null,null,null,null,null,null,null,"X",null,null,1240,null,null,null,"X","X",0.1,14.7,90]
["Portugal","PRT",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,49,null,"ITU-R F.497","X",null,null,2,"25",46,-50]
["Portugal","PRT",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,368,null,"ERC/REC 12-02","X","X","X",1,"15",57,10]
["Russia","RUS",0,"12750-13250","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",16553,null,"ERC/REC 12-02 e ITU-R F.497","X","X","X",10,25,35]
["Serbia","SRB",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,564,null,"ERC/REC 12-02","X","X","X",2.15,19.579999999999998,58.65,50]
["Slovak Republic","SVK",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,620,null,"ERC/REC 12-02","X","X","X",4,15,48,20]
["Slovenia","SVN",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,178,null,"ERC/REC 12-02",null,"X","X",2,25,54,5,"x"]
["Slovenia","SVN",0,"12750-13250","X",null,null,null,"X",null,null,null,"X",null,null,null,21,null,"ERC/REC 12-02",null,null,"X",5,20,40,5,"x"]
["Sweden","SWE",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,775,null,"ERC/REC 12-02",null,null,null,null,null,null,null,"Y"]
["Switzerland","CHE",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,470,null,"ERC/REC 12-02",174,290,6,10,14.2,46.4,"unchanged",null,null,"heavily used by FSS"]
["UK","GBR",0,"12750-13250","X",null,null,null,null,null,null,null,null,"X",null,3840,340,null,"ERC/REC 12-02","X","X","X"]
[]
["Telia","TELIASON",0,"14250-14500"]
["Austria","AUT",0,"14250-14500"]
["Bosnia and Herzegovina","BIH",0,"14250-14500"]
["Croatia","HRV",0,"14250-14500"]
["Czech Republic","CZE",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"sat. services planned"]
["Cyprus","CYP",0,"14250-14500","X",null,null,null,null,null,null,null,"X",null,null,14,null,null,"ERC/REC 13-03",null,"X"," ",8.2899999999999991,null,36.46]
["Denmark","DNK",0,"14250-14500"]
["Estonia","EST",0,"14250-14500"]
["Finland","FIN",0,"14250-14500"]
["France","FRA",0,"14250-14500","X",null,null,null,"X",null,"X",null,null,null,null,null,374,null,null,374,null,null,10,"5<x>35",100,"-5%"]
["Greece","GRC",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Hungary","HUN",0,"14250-14500"]
["Iceland","ICE",0,"14250-14500"]
["Ireland","IRL",0,"14250-14500"]
["Italy","ITA",0,"14250-14500","X",null,null,null,null,null,null,null,"X",null,null,1030,null,null,"national",null,null,"X",3,11,27,0.05,"yes"]
["Latvia","LVA",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIXED-SATELLITE"]
["Lithuania","LTU",0,"14250-14500"]
["Luxembourg","LUX",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Netherlands","NLD",0,"14250-14500"]
["Norway","NOR",0,"14250-14500"]
["Portugal","PRT",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,"FSS, VSAT, SNG, AES"]
["Russia","RUS",0,"14250-14500","X","X",null,null,null,null,null,null,null,null,null,null,150,null,null,"X","X","X",8,20,30]
["Serbia","SRB",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it have not been used yet"]
["Slovak Republic","SVK",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovenia","SVN",0,"14250-14500"]
["Sweden","SWE",0,"14250-14500"]
["Switzerland","CHE",0,"14250-14500"]
["UK","GBR",0,"14250-14500"]
[]
["Bosnia and Herzegovina","BIH",0,"14400-15350","X",null,null,null,null,null,"X",null,null,null,null,null,162,null,"ITU-R F.636","X","X",null,1,15,45,null,null,null,"14400-15350 MHz: Planned leaving of ITU rec. and fully harmonization according to ERC/REC 12-07"]
[]
["Telia","TELIASON",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,944,null,"ERC/REC 12-07",620,324,null,1,null,39,"-",null,null,null,"Eric sson ML"]
["Telia","TELIASON",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,93,null,null,93,null,null,3,null,30,null,"X",null,null,"NEC Pasolink"]
["Austria","AUT",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,631,null,"ERC/REC 12-07","x","x","x",1,15,44]
["Bosnia and Herzegovina","BIH",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,278,null,"ERC/REC 12-07","X","X",null,1,15,45]
["Croatia","HRV",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,"X",null,null,20,null,null,"ERC/REC 12-07",null,null,null,0.6,9.9,22.7]
["Czech Republic","CZE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,20,null,"ERC/REC 12-07"]
["Cyprus","CYP",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,"X",null,null,12,null,null,"ERC/REC 12-07",null,"X",null,0.45,null,38.17]
["Denmark","DNK",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,null,null,null,null,299,null,"ERC/REC 12-07",null,null,null,12]
["Estonia","EST",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,60,null,"ERC/REC 12-07",null,60,null,12,23,33,"- 5"]
["Finland","FIN",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07"]
["Finland","FIN",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,1950,null,"ITU-R F.636",null,"X",null,0.1,8.6999999999999993,10.9,-0.15]
["France","FRA",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07"]
["Germany","GER",0,"14500-14620 and 15230-15350","x",null,null,null,"x",null,null,null,null,null,null,10235,null,null,"ERC/REC 12-07",null,"x",null,2.25,14,54.5,null,"x"]
["Greece","GRC",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,2863,null,"ERC/REC 12-07","X","X","X",0.5,15,75,0.5,"heavily used"]
["Hungary","HUN",0,"14500-14620 and 15230-15350"," ",null,null,null," ",null,null,null,null,null,null,null," ",null,"ERC/REC 12-07",null,null,null,null," "]
["Hungary","HUN",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,"15230-15350 MHz Non-Civil Digital P-P links",null,120,null,null,"X","X",null,null," ",null,null,"x",null,"non-civil usage"]
["Iceland","ICE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,120,null,"ERC/REC 12-07",57,57,6,5,15,25,25]
["Ireland","IRL",0,"14500-14620 and 15230-15350"," X",null,null,null,null,null," X",null,null,null,null,null,1718,null,"ERC/REC 12-07\nNational Legislation: S.I. 370 of 2009"," X","X","X",1.7,17,53," 29"," X"]
["Italy","ITA",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,4070,null,"ERC/REC 12-07","X","X","X",7,16,33,0.15,"yes"]
["Italy","ITA",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,1562,null,"national",null,"X",null,null,null,null,null,"yes"]
["Latvia","LVA",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,48,null,"ERC/REC 12-07",null,"X",null,3,25,37,20]
["Lithuania","LTU",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,262,null,"ERC/REC 12-07"]
["Luxembourg","LUX",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,"X",null,null,0,64,null,"ERC/REC 12-07",null,"X","X",1.4,"5-30",34.700000000000003,"N/A","NO","NO"]
["Netherlands","NLD",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,null,"X",null,null,116,null,"ERC/REC 12-07","x","x","x",7.71,14.7,34.9,20]
["Norway","NOR",0,"14500-14620 and 15230-15350"]
["Portugal","PRT",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,362,null,"ERC/REC 12-07","X","X",null,1,"15",37,5]
["Serbia","SRB",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,433,null,"ERC/REC 12-07","X","X","X",1.35,16.98,39.26,20]
["Slovak Republic","SVK",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,230,null,"ERC/REC 12-07","x","x",null,9.5,15,48,10]
["Slovenia","SVN",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07",null,null,null,null,null,null,null,null,null,"Defence systems:","Land military systems (FS, MS)"]
["Sweden","SWE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,2629,null,"Nat ch.plan(expdate 2016)",null,null,null,null,null,null,null,"Y"]
["Switzerland","CHE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,263,null,"ERC/REC 12-07",110,153,null,10,14.6,37.1,"unchanged"]
["UK","GBR",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,null,"X",null,2050,2050,null,"ERC/REC 12-07","X","X","X"]
["Russia","RUS",0,"14500-14620 and 15230-15350","X","X",null,null,null,null,"X",null,"X",null,null,12,13320,null,"ERC/REC 12-07 e ITU-R F.636","X","X","X",8,20,30]
[]
["Slovenia","SVN",0,"14613-14725 and 15033-15145","X",null,null,null,"X",null,"X",null,null,null,null,null,82,null,"ITU-R F.636-3 (Ch. 5,6,7,8)",null,"x",null,7,25,45,-10,null,"x"]
["Slovenia","SVN",0,"14613-14725 and 15033-15145",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07",null,null,null,null,null,null,null,null,"x","Defence systems:","Land military systems (FS, MS)"]
[]
["Czech Republic","CZE",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FS considered"]
["Greece","GRC",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Italy","ITA",0,"17300-17700","X",null,null,null,"X",null,null,null,null,null,null,null,33,null,"national",null,"X"]
["Latvia","LVA",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HDFSS"]
["Portugal","PRT",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,"FSS, HDFSS"]
["Russia","RUS",0,"17300-17700","No","No"]
["Serbia","SRB",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["Slovak Republic","SVK",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
[]
["Iceland","ICE",0,"17700-19700","X",null,null,null,"X",null,null,null,null,null,null,null,60,null,"ERC/REC 12-03",40,10,10,10,15,20,25]
["Ireland","IRL",0,"17700-19700"," X",null,null,null,null,null," X",null,null,null,null,null,686,null,"ERC/REC 12-03\nNational Legislation: S.I. 370 of 2009",null," X","X",0.3,9,45," 28"," X"]
["Italy","ITA",0,"17700-19700","X","X",null,null,"X",null,"X",null,null,null,null,null,{"$f":"14300+1512","v":15812},null,"ERC/REC 12-03","X","X","X",0.3,6,12,0.25,"highly"]
["Italy","ITA",0,"17700-19700","X",null,null,null,null,null,"X",null,"X",null,null,71,35,null,null,null,"X","X",1.3,4,7.5,0.25]
["Lithuania","LTU",0,"17700-19700","X",null,null,null,"X",null,null,null,null,null,null,null,490,null,"ERC/REC 12-03"]
["Luxembourg","LUX",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,null,0,47,null,"ERC/REC 12-03",null,null,"X",4.8,"4-25",24.1,"N/A","NO","NO"]
["Luxembourg","LUX",0,"17700-19700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"17700-19700","X",null,null,null,"x",null,null,null,null,null,null,null,390,null,"ERC/REC 12-03",null,null,"X",1,20,43,20]
["Netherlands","NLD",0,"17700-19700","X",null,null,null,null,null,null,null,null,"X",null,null,1020,null,"ERC/REC 12-03",null,"x","x",7.7,5.27,34.9,20]
["Netherlands","NLD",0,"17700-19700","X",null,null,null,null,null,null,null,null,"X",null,null,43,null,"F-5958-8 Annex 8",null,"x","x",5.63,13.11,18.649999999999999,0]
["Norway","NOR",0,"17700-19700",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-03"]
["Norway","NOR",0,"17700-19700","X",null,null,null,null,null,null,null,null,"X",null,null,387,null,null,null,null,"x",0.5,10.199999999999999,44.8]
["Portugal","PRT",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,131,null,"ITU-R F.595","X",null,null,2,"10",29,10]
["Portugal","PRT",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,1087,null,"ERC/REC 12-03",null,"X","X",0,"7",35,20]
["Russia","RUS",0,"17700-19700","X","X",null,null,null,null,null,null,null,null,null,null,24277,null,"ERC/REC 12-03 and ITU-R F.595-9 ","X","X","X",5,12,20]
["Serbia","SRB",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,459,null,"ERC/REC 12-03 and ITU-R F.595-9 ","X","X","X",0.91,10.029999999999999,35.159999999999997,100]
["Slovak Republic","SVK",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,null,null,2170,null,"ERC/REC 12-03","x","x","x",1,10,38,20]
["Slovenia","SVN",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,null,null,361,null,"ERC/REC 12-03",null,null,"x",5,15,35,20,"x**",null,"congested in urban/sub urban regions"]
["Slovenia","SVN",0,"17700-19700",null,"X",null,null,"X",null,"X",null,null,null,null,null,300,null,"ERC/REC 12-03",null,"x","x",5,15,35,0,"x**",null,"congested in urban/sub urban regions"]
["Sweden","SWE",0,"17700-19700","X",null,null,null,"X",null,null,null,null,null,null,null,2242,null,"ERC/REC 12-03",null,null,null,null,null,null,"Y","N"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,3,null,"ERC/REC 12-03",null,null,3,9,null,11,null,"X",null,null,"NEC 900"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,23,null,null,null,null,23,3,null,14,0,null,null,null,"NERA Citylink"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,738,null,null,null,645,93,4,null,28,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,1,null,null,null,null,1,null,9,null,"++",null,null,null,"Ericsson TN"]
[]
["Austria","AUT",0,"21200-22000","X",null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Bosnia and Herzegovina","BIH",0,"21200-22000","X",null,null,null,null,null,"X",null,null,null,null,null,256,null,null,"X","X","X","0.5",5,20,null,null,null,"21200-22000 MHz: Planned leaving of band and full harmonization according to T/R 13-02 Annexes A1, A2, A3"]
["Cyprus","CYP",0,"21200-22000","X",null,null,null,null,null,"X",null,null,null,null,null,97,null,null,"X","X"," ",0.2,null,18.27,null,"X"]
["Greece","GRC",0,"21200-22000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Use"]
["Hungary","HUN",0,"21200-22000","X",null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,40,null,null,"X"]
["Italy","ITA",0,"21200-22000","X",null,null,null,null,null,"X",null,null,null,null,26,7,null,null,null,"X",null,0.19,2.44,7.25]
["Lithuania","LTU",0,"21200-22000","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"local"]
["Latvia","LVA",0,"21200-22000","X",null,null,null,"x",null,null,null,null,null,null,2,null,null,"national plan","X",null,null,3,5,8,100]
["Portugal","PRT",0,"21200-22000",null,null,null,null,null,null,null,null,null,null,"SRR"]
["Serbia","SRB",0,"21200-22000","X",null,null,null,null,null,null,null,"X",null,null,3,null,null,"ITU-R F.637-3 annex 5 ","X",null,null,3.11,4.9800000000000004,7.15]
["Slovak Republic","SVK",0,"21200-22000","X",null,null,null,"X",null,null,null,"X",null,null,0,null,null,"ITU-R F.637",null,null,null,null,null,null,null,null,null,"currently no links"]
[]
["Russia","RUS",0,"21200-23600","X","X",null,null,null,null,null,null,null,null,null,null,16816,null,"F.637 ITU-R","X","X","X",2,4,8]
[]
["Austria","AUT",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,2885,null,"T/R 13-02 Annexes A1, A2, A3","x","x","x",1,10,20]
["Bosnia and Herzegovina","BIH",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,421,null,"T/R 13-02 Annexes A1, A2, A3","X","X","X","0.5",5,20,"+20"]
["switzerland","CHE",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,1900,null,"T/R 13-02 Annexes A1, A2, A3",787,1113,null,5,7.4,29.9,"unchanged","city areas congested, HIGH/LOW situation",null,"problem: SRR"]
["Cyprus","CYP",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,738,null,"T/R 13-02 Annexes A1, A2, A3","X","X"," ",0.25,null,15.16,null,"X"]
["Czech Republic","CZE",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,3707,null,"T/R 13-02 Annexes A1, A2, A3",null,null,null,null,null,null,5]
["Denmark","DNK",0,"22000-22600 and 23000-23600",null,"X",null,null,null,null,null,null,null,null,null,null,"No info",null,"T/R 13-02 Annexes A1, A2, A3"]
["Denmark","DNK",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,null,null,null,650]
["Estonia","EST",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,788,null,"T/R 13-02 Annexes A1, A2, A3",null,788,null,3,14,24,"+25"]
["Finland","FIN",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,2770,null,"T/R 13-02 Annexes A1, A2, A3",null,"X","X",0.1,4.5999999999999996,19,0.15,"x",null,"Local congestion"]
["France","FRA",0,"22000-22600 and 23000-23600","X","X",null,null,"X",null,"X",null,null,null,null,null,12195,null,"T/R 13-02 Annexes A1, A2, A3",4614,7498,83,0.1,"3<x>20",32,"+ 9 %"]
["France","FRA",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IUT-RF 637-3"]
["UK","GBR",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,"X",null,4750,null,null,"T/R 13-02 ","X","X","X"]
["Germany","GER",0,"22000-22600 and 23000-23600","x",null,null,null,"x",null,null,null,null,null,null,19401,null,null,"ERC/REC 13-02 ",null,"x",null,0.13,8,51.1]
["Croatia","HRV",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,1220,null,"T/R 13-02 Annexes A1, A2, A3",null,"x",null,0.18,5.5,21.1,10]
["Hungary","HUN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,"22442-22600 MHz Emergency Services Digital P-P links",null,40,null,"T/R 13-02 Annexes A1, A2, A3","X","X",null,null,null,null,null,"x"]
["Hungary","HUN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,"23450-23600 MHz Emergency services Digital P-P links",null,3512,null,"T/R 13-02 Annexes A1, A2, A3","X","X",null,null,null,null,null,"x"]
["Iceland","ICE",0,"22000-22600 and 23000-23600","X",null,null,null,"x",null,null,null,null,null,null,null,18,null,"T/R 13-02 Annexes A1, A2, A3",5,11,2,1,6,25,25]
["Ireland","IRL",0,"22000-22600 and 23000-23600"," X",null,null,null,null,null," X",null,null,null,null,null,2178,null,"T/R 13-02 Annexes A1, A2, A3"," X","X","X",0.2,6.7,24," 36"," X"]
["Ireland","IRL",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Italy","ITA",0,"22000-22600 and 23000-23600","X","X",null,null,"X",null,"X",null,null,null,null,2,{"$f":"10970+1101","v":12071},null,"T/R 13-02 Annexes A1, A2, A3","X","X","X",2.1800000000000002,2.95,3.17,0.25,"yes"]
["Lithuania","LTU",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,1362,null,"T/R 13-02 Annexes A1, A2, A3"]
["Luxembourg","LUX",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,"X",null,null,1,243,null,"T/R 13-02 Annexes A1, A2, A3",null,"X",null,0.3,"3-20",15,"N/A","NO","NO"]
["Luxembourg","LUX",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,592,null,"T/R 13-02 Annexes A1, A2, A3",null,null,"X",0.15,15,25,30]
["Netherlands","NLD",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,"X",null,null,1450,null,"T/R 13-02 Annexes A1, A2, A3","x","x","x",3,7.65,14.78,30]
["Norway","NOR",0,"22000-22600 and 23000-23600",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annexes A1, A2, A3"]
["Norway","NOR",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,"X",null,2,64,null,null,null,null,"x",0.3,5.7,25.4]
["Portugal","PRT",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,"SRR",null,10,null,"Report 936-2 Annex 6","X",null,null,1,"5",12,-100]
["Portugal","PRT",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,"SRR",null,908,null,"T/R 13-02 Annexes A1","X","X","X",null,"5",12,10]
["Serbia","SRB",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,1288,null,"T/R 13-02 Annexes A1","X","X","X",0.14000000000000001,4.74,24.41,100]
["Slovak Republic","SVK",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,1582,null,"T/R 13-02 Annex A1","x","x","x",0.5,5,13,10]
["Slovenia","SVN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,767,null,"T/R 13-02 Annex A1",null,"x",null,3,7,10,5,"x**",null,"congested in urban/sub urban regions"]
["Slovenia","SVN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,10,null,"T/R 13-02 Annex A1",null,null,"x",2,4,5,20,"x**",null,"congested in urban/sub urban regions"]
["Sweden","SWE",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,1322,null,"T/R 13-02 Annexes A1, A2, A3",null,null,null,null,null,null,null,"Y"]
["Telia","TELIASON",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,506,null,"T/R 13-02 Annexes A1, A2, A3",303,203,null,1,null,18,"-",null,null,null,"Eric sson ML"]
["Telia","TELIASON",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,338,null,null,null,316,22,3,null,17,"+",null,null,null,"NEC NEO"]
[]
["Greece","GRC",0,"22000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,1724,null,"T/R 13-02 Annex A","X","X","X","0.04",4,16,0.4]
[]
["Czech Republic","CZE",0,"22600-22700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENG/OB"]
[]
["Cyprus","CYP",0,"22600-23000","X",null,null,null,null,null,"X",null,null,null,null,37,null,null,"National","X","X"," ",0.2,null,18.14,null,null,"X"]
["Denmark","DNK",0,"22600-23000","X",null,null,null,null,null,null,null,null,null,null,null,1]
["France","FRA",0,"22600-23000","X",null,null,null,"X",null,"X",null,null,null,null,null,124,null,null,124,null,null,0.1,10,32,"+ 1%"]
["Greece","GRC",0,"22600-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,"No current FS use.\nAllocation for analogue links. SAP/SAB, ENG/OB"]
["Hungary","HUN",0,"22600-23000","X",null,null,null,null,null,null,null,"X",null,null,1,null,null,null,null,null,null,null,40,null,null,"x"]
["Italy","ITA",0,"22600-23000","x",null,null,null,null,null,"X",null,null,null,null,1,null,null,null,null,"x",null,null,0.19]
["Lithuania","LTU",0,"22600-23000","X",null,null,null,"X",null,null,null,"X",null,null,1,null,null,"local"]
["Latvia","LVA",0,"22600-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAP/SAB "]
["Portugal","PRT",0,"22600-23000","X",null,null,null,"X",null,"?",null,null,null,"SRR",null,null,null,"T/R 13-02 Annexes A2, A3",null,null,null,null,null,null,"no use at the moment"]
["Serbia","SRB",0,"22600-23000","X",null,null,null,null,null,null,null,"X",null,null,94,null,null,"ITU-R F.637-3 annex 5 ","X",null,null,0.21,2.5,11.87]
["Slovak Republic","SVK",0,"22600-23000","x",null,null,null,"X",null,null,null,"X",null,null,0,null,null,"ITU-R F.637",null,null,null,null,null,null,null,null,null,"currently no links"]
["Slovenia","SVN",0,"22600-23000","x",null,null,null,"X",null,"X",null,null,null,null,null,"planned",null,"T/R 13-02 Annex A2","x","x"]
["Slovenia","SVN",0,"22600-23000",null,null,null,null,"X",null,null,null,"X","X",null,"planned",null,null,"T/R 13-02 Annex A3","x","x"]
[]
["Czech Republic","CZE",0,"22700-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no utilisation"]
[]
["Czech Republic","CZE",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAB"]
["Denmark","DNK",0,"24250-24500","X",null,null,null,null,null,null,null,null,null,null,null,1]
["Greece","GRC",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC REP 38",null,null,null,null,null,null,"-",null,null,"No current use.\nAllocation for analogue links. SAP/SAB, ENG/OB"]
["Hungary","HUN",0,"24250-24500","X","X",null,null,"X","X",null,null,null,null,null,null,41,31,null,"X","X","X",null,7,null,0.25,"x",null,"ù"]
["Lithuania","LTU",0,"24250-24500","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"local"]
["Luxembourg","LUX",0,"24250-24500",null,"X",null,null,null,"X","X",null,"X",null,null,null,null,4,"Nat. freq. plan",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"24250-24500","X",null,null,null,"X",null,"X",null,"X",null,null,0,10,null,"Nat. freq. plan",null,"X",null,null,"2-15",null,"N/A","NO","NO"]
["Latvia","LVA",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAB/SAP, SRR"]
["Portugal","PRT",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,"SRR, SRD"]
["Russia","RUS",0,"24250-24500","No","No",null,null,null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["Slovak Republic","SVK",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
[]
["Czech Republic","CZE",0,"24500-24745/25500-25753",null,"X",null,null,null,"X",null,null,null,null,null,null,null,133,"T/R 13-02 Annex B",null,null,null,null,null,null,10]
[]
["Austria","AUT",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,2365,null,"T/R 13-02 Annex B","x","x","x",1,6,24]
["Austria","AUT",0,"24500-26500"]
["Bosnia and Herzegovina","BIH",0,"24500-26500","X","X",null,null,null,null,"X",null,null,null,null,null,3,null,"T/R 13-02 Annex B","X","X","X",1,4,6,"+35",null,null,"24500-26500, 27500-29500 MHz: Shared band between P-P links and FWA. Actually, block assignments for P-P links in process. We still do not have active implemented FWA systems."]
["Bosnia and Herzegovina","BIH",0,"24500-26500",null,"X",null,null,"X","X"]
["switzerland","CHE",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,38,null,"T/R 13-02 Annex B",null,null,38,2,2.9,5.9,"growth",null,null,"problem: SRR"]
["switzerland","CHE",0,"24500-26500"]
["Cyprus","CYP",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Cyprus","CYP",0,"24500-26500"]
["Denmark","DNK",0,"24500-26500",null,"X",null,null,null,null,null,null,null,null,null,null,null,"No info","T/R 13-02 Annex B"]
["Denmark","DNK",0,"24500-26500","X",null,null,null,null,null,null,null,null,null,null,null,null,135]
["Estonia","EST",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Estonia","EST",0,"24500-26500"]
["Finland","FIN",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Finland","FIN",0,"24500-26500"]
["France","FRA",0,"24500-26500","X","X",null,null,"X","X","X",null,null,null,null,null,215,75,"T/R 13-02 Annex B",null,88,127,0.12,"3<x>20",15,"+ 3 %"]
["France","FRA",0,"24500-26500"]
["UK","GBR",0,"24500-26500","X",null,null,null,null,null,null,null,null,"X",null,3570,null,null,"T/R 13-02","X","X","X"]
["UK","GBR",0,"24500-26500"]
["Germany","GER",0,"24500-26500","x",null,null,null,"x","x",null,null,null,null,null,15880,null,null,"ERC/REC 13-02 ",null,"x",null,0.1,4,10.9]
["Germany","GER",0,"24500-26500",null,"x",null,null,null,null,null,null,null,null,null,null,null,836]
["Greece","GRC",0,"24500-26500",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC 13-02","-",null,null,null,null,null,"-",null,null,"5 issued licenses"]
["Croatia","HRV",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Croatia","HRV",0,"24500-26500"]
["Hungary","HUN",0,"24500-26500","X","X",null,null,"X","X",null,null,null,null,null,null,83,31,"T/R 13-02 Annex B","X","X","X",null,7,null,0.25,"x",null,"PMP systems"]
["Hungary","HUN",0,"24500-26500"]
["Iceland","ICE",0,"24500-26500","X",null,null,null,"x",null,null,null,null,null,null,null,2,null,"T/R 13-02 Annex B",null,null,2,12,15,18,10]
["Ireland","IRL",0,"24500-26500"," X",null,null,null,"X",null," X",null,null,null,null,null,636,null,"T/R 13-02 Annex B"," X","X","X",0.05,5,17," 43"," X"]
["Ireland","IRL",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Ireland","IRL",0,"24500-26500",null," X",null,null,null,null," X",null,null,null,null,null,null,null," National Legislation: S.I. 762 of 2007"]
["Ireland","IRL",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ireland","IRL",0,"24500-26500","X",null,null,null,null,"X",null,null,null,null,null,null,null,15,"National Legislation: S.I. 79 of 2003",null,null,null,null,null,null,55]
["Ireland","IRL",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 530 of 2003"]
["Italy","ITA",0,"24500-26500",null,"X",null,null,null,"X","X",null,null,null,null,null,null,"not known","T/R 13-02 Annex B",null,null,null,null,null,null,0.15,"not yet"]
["Italy","ITA",0,"24500-26500"]
["Lithuania","LTU",0,"24500-26500","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"T/R 13-02 Annex B"]
["Lithuania","LTU",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,84,"T/R 13-02 Annex B",null,null,null,null,null,null,30]
["Luxembourg","LUX",0,"24500-26500",null,"X",null,null,null,"X","X",null,"X",null,null,null,null,4,"T/R 13-02 Annex B",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"24500-26500","X",null,null,null,"X",null,"X",null,"X",null,null,0,10,null,"Nat. freq. plan",null,"X",null,null,"2-15",null,"N/A","NO","NO"]
["Latvia","LVA",0,"24500-26500","X",null,null,null,"x",null,null,null,null,null,null,null,6,null,"T/R 13-02 Annex B",null,null,"X",1.4,5,6]
["Latvia","LVA",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,52,null,null,"X",null,null,5,null,50]
["Netherlands","NLD",0,"24500-26500","x",null,null,null,null,null,null,null,null,"X",null,null,908,null,"T/R 13-02 Annex B","x","x","x",2.5499999999999998,6.42,14.52,30]
["Netherlands","NLD",0,"24500-26500",null,null,null,null,null,"x",null,null,null,"X",null,null,null,90,"T/R 13-02 Annex B",null,null,null,null,null,null,10]
["Norway","NOR",0,"24500-26500",null,"x",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annex B"]
["Norway","NOR",0,"24500-26500","x",null,null,null,null,null,null,null,null,"X",null,3,65,null,null,null,"x","x",0.5,4.8,21.1]
["Portugal","PRT",0,"24500-26500",null,"X",null,null,null,"X","X",null,null,null,"SRR, SRD, Military (25.25-25.492 GHz and 26.25-27.5 GHz)",null,null,125,"T/R 13-02 Annex B","X","X",null,null,"5",null,0]
["Portugal","PRT",0,"24500-26500"]
["Russia","RUS",0,"24500-26500","X","X",null,null,null,"X","X",null,null,null,null,null,447,null,"T/R 13-02 Annex B","X","X","X",2,4,8]
["Russia","RUS",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["Serbia","SRB",0,"24500-26500","X",null,null,null,null,null,"X",null,null,null,null,null,660,null,"T/R 13-02 Annex B","X","X","X",0.6,2.21,12.5,100]
["Serbia","SRB",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,4]
["Slovak Republic","SVK",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,1230,null,"T/R 13-02 Annex B","x","x","x",0.1,3.5,8,20]
["Slovak Republic","SVK",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,40,null,"x","x",null,null,null,null,10]
["Slovenia","SVN",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,109,null,"T/R 13-02 Annex B (25.165-25.557 GHz/>26.173 GHz)",null,"x",null,3,6,8,100,null,null,null,"used instead of the congested 23 GHz band"]
["Slovenia","SVN",0,"24500-26500","X",null,null,null,null,"X","X",null,null,null,null,null,null,22,"T/R13-02 AnnexB (25.053-25.165GHz/26.061-26.173GHz)",null,"x",null,null,null,null,-5]
["Slovenia","SVN",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,"BWA",null,null,"planned","T/R13-02 Annex B (24.549–25.053GHz/25.557–26.061GHz)",null,"x","x",1,3,5,null,null,null,"BWA"]
["Sweden","SWE",0,"24500-26500",null,"X",null,null,"X","X","X",null,null,null,null,null,5601,null,"T/R 13-02 Annex B",null,null,null,null,null,null,"Y"]
["Sweden","SWE",0,"24500-26500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null," ERC / REC / (00) 05",null,null,null,null,null,null,null,"N"]
["Telia","TELIASON",0,"24500-26500",null,"X",null,null,null,null,"X",null,null,null,null,null,161,null,"T/R 13-02 Annex B",99,18,44,2,null,10,"-",null,null,null,"Eric sson ML"]
["Telia","TELIASON",0,"24500-26500",null,"X",null,null,null,null,null,null,null,null,null,null,629,null,null,null,574,55,1,null,12,"+",null,null,null,"NEC NEO"]
[]
["Czech Republic","CZE",0,"24745-25500/25753-26500","X",null,null,null,"X",null,null,null,null,null,null,null,4537,null,null,null,null,null,null,null,null,10]
[]
["Czech Republic","CZE",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,"MD"]
["Czech Republic","CZE",0,"26500-27500"]
["Greece","GRC",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Hungary","HUN",0,"26500-27500",null,null,null,null,"X",null,null,null,null,null,"Land military systems. P-P links Harmonized NATO band type 2.(planned)",null,null,null,null,null,null,null,null,null,null,null,"X"]
["Latvia","LVA",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band"]
["Portugal","PRT",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,"SRR, SRD, Military (26.25-27.5 GHz)"]
["Russia","RUS",0,"26500-27500","X","X",null,null,null,"X","X",null,null,null,null,null,26,null,"F.748 ITU-R","X","X","X",2,4,8]
["Serbia","SRB",0,"26500-27500",null,null,null,null,null,null,null,null,null,"X"]
["Slovak Republic","SVK",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
[]
["Austria","AUT",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,156,null,"T/R 13-02 Annex C",null,null,"x",1,2,4]
["Austria","AUT",0,"27500-29500"]
["Bosnia and Herzegovina","BIH",0,"27500-29500","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,"+5",null,null,"24500-26500, 27500-29500 MHz: Shared band between P-P links and FWA. Actually, block assignments for P-P links in process. We still do not have active implemented FWA "]
["Bosnia and Herzegovina","BIH",0,"27500-29500",null,"X",null,null,"X","X"]
["switzerland","CHE",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,"starts now",null,"T/R 13-02 Annex C",null,null,null,null,null,null,"growth"]
["switzerland","CHE",0,"27500-29500"]
["Cyprus","CYP",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Cyprus","CYP",0,"27500-29500"]
["Czech Republic","CZE",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,41,"T/R 13-02 Annex C"]
["Czech Republic","CZE",0,"27500-29500","X","X",null,null,"X","X",null,null,null,null,null,null,189]
["Denmark","DNK",0,"27500-29500","X",null,null,null,null,null,null,null,null,null,null,null,null,18,"T/R 13-02 Annex C"]
["Denmark","DNK",0,"27500-29500"]
["Estonia","EST",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Estonia","EST",0,"27500-29500"]
["Finland","FIN",0,"27500-29500","X",null,null,null,null,null,"X",null,null,null,null,null,380,null,"T/R 13-02 Annex C",null,"X","X",0.1,1.1000000000000001,7.2,0.9,"x",null,"Local congestion"]
["Finland","FIN",0,"27500-29500"]
["France","FRA",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["France","FRA",0,"27500-29500"]
["UK","GBR",0,"27500-29500"]
["UK","GBR",0,"27500-29500"]
["Germany","GER",0,"27500-29500",null,"x",null,null,"x","x",null,null,null,null,null,1424,null,29,"ERC/REC 13-02 ",null,null,null,0.18,3,13.3]
["Greece","GRC",0,"27500-29500",null,null,null,null,"X","X",null,null,null,null,null,null,null,null,"ECC/DEC/(05)01","no current use",null,null,null,null,null,"-",null,null,"27828,5-27940,5 and 27940,5-28444,5 MHz paired with 28948,5-29452,5 new row by EETT allocated to digital P-P and P-MP links"]
["Croatia","HRV",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Croatia","HRV",0,"27500-29500"]
["Hungary","HUN",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Hungary","HUN",0,"27500-29500"]
["Iceland","ICE",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Ireland","IRL",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Ireland","IRL",0,"27500-29500"]
["Italy","ITA",0,"27500-29500",null,"X",null,null,null,"X","X",null,null,null,null,null,null,"not known","T/R 13-02 Annex C",null,null,null,null,null,null,0.15,"not yet"]
["Italy","ITA",0,"27500-29500"]
["Lithuania","LTU",0,"27500-29500","X",null,null,null,"X",null,null,null,null,null,null,null,20,null,"T/R 13-02 Annex C",null,20]
["Lithuania","LTU",0,"27500-29500",null,"X",null,null,null,"X",null,null,"X",null,null,null,null,8,"54MHz/3,2MHz",null,null,null,null,null,null,0,null,null,"LMDS (do not comply T/R 13-02)"]
["Luxembourg","LUX",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Luxembourg","LUX",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Latvia","LVA",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,51,null,null,null,"X",null,null,null,50]
["Netherlands","NLD",0,"27500-29500","X",null,null,null,null,null,null,null,null,"X",null,null,185,null,"T/R 13-02 Annex C",null,null,"x",2.52,4.21,6.8730000000000002,30]
["Netherlands","NLD",0,"27500-29500"]
["Norway","NOR",0,"27500-29500",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annex C"]
["Norway","NOR",0,"27500-29500","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Portugal","PRT",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,"FSS, HDFSS",null,null,21,"T/R 13-02 Annex C",null,"X",null,null,"5",null,0]
["Portugal","PRT",0,"27500-29500"]
["Russia","RUS",0,"27500-29500","X","X",null,null,null,"X","X",null,null,null,null,null,1,null,"T/R 13-02 Annex C","X","X","X",2,4,8]
["Russia","RUS",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["Serbia","SRB",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["Serbia","SRB",0,"27500-29500"]
["Slovak Republic","SVK",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,110,null,"T/R 13-02 Annex C","x","x","x",0.2,2.5,4.5,10]
["Slovak Republic","SVK",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,15,null,"x","x",null,null,null,null,10]
["Slovenia","SVN",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,"planned",null,"T/R 13-02 Annex C (27.8285 – 27.9405 GHz/28.8365 – 28.9485 GHz)",null,"x",null,0.5,3,5]
["Slovenia","SVN",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,"planned","T/R13-02 Annex C (27.9405 – 28.4445 GHz/28.9485 – 29.4525 GHz)",null,"x","x",0.3,2,4]
["Sweden","SWE",0,"27500-29500",null,"X",null,null,"X","X","X",null,null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,"Y"]
["Telia","TELIASON",0,"27500-29500",null,"X",null,null,null,null,"X",null,null,null,null,null,6,null,"T/R 13-02 Annex C",null,null,6,1,null,4,"++",null,null,null,"Ericsson TN"]
["Telia","TELIASON",0,"27500-29500"]
[]
["Czech Republic","CZE",0,"31000-31300","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,5]
["UK","GBR",0,"31000-31300","X",null,null,null,null,null,null,null,null,null,"X",null,null,null,"national arrangement"]
["Germany","GER",0,"31000-31300",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,"x",null,null,null,null,null,null,null,"not open"]
["Hungary","HUN",0,"31000-31300","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02","X","X","X",null,5,null,null,"x",null,"FDD mode PP systems"]
["Lithuania","LTU",0,"31000-31300","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ECC/REC/(02)02"]
["Luxembourg","LUX",0,"31000-31300","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ECC/REC/(02)02",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"31000-31300",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"31000-31300","?",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,null,null,null,"Fixed links, FWA"]
["Portugal","PRT",0,"31000-31300",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,"Planned"]
["Russia","RUS",0,"31000-31300","No","No",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02"]
[]
["Austria","AUT",0,"31800-33400"]
["Bosnia and Herzegovina","BIH",0,"31800-33400"]
["switzerland","CHE",0,"31800-33400","X",null,null,null,"X",null,"X",null,null,null,null,null,102,null,"ERC/REC/(01)02",null,69,33,0.5,2.2999999999999998,4.5999999999999996,"growth"]
["Cyprus","CYP",0,"31800-33400"]
["Czech Republic","CZE",0,"31800-33400","X",null,null,null,"X",null,null,null,null,null,null,null,50,null,"ERC/REC/(01)02",null,null,null,null,null,null,50]
["Denmark","DNK",0,"31800-33400",null,"X",null,null,null,null,null,null,null,null,null,null,"No info",null,"ERC/REC/(01)02"]
["Estonia","EST",0,"31800-33400"]
["Finland","FIN",0,"31800-33400","X",null,null,null,null,null,"X",null,null,null,null,null,1,null,"ERC/REC/(01)02",null,"X","X",null,null,null,100]
["France","FRA",0,"31800-33400","X","X",null,null,"X",null,"X",null,null,null,null,null,null,null,"ERC/REC/(01)02"]
["UK","GBR",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it have not been used yet"]
["Germany","GER",0,"31800-33400","x",null,null,null,"x",null,null,null,null,null,null,1466,null,null,"ERC/REC/(01)02",null,"x",null,0.1,2.2999999999999998,6.8,20]
["Greece","GRC",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Croatia","HRV",0,"31800-33400"]
["Hungary","HUN",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,"x"]
["Hungary","HUN",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(04)06",null,null,null,null,null,null,null,"x"]
["Iceland","ICE",0,"31800-33400"]
["Ireland","IRL",0,"31800-33400"]
["Italy","ITA",0,"31800-33400"]
["Lithuania","LTU",0,"31800-33400","X",null,null,null,"X",null,null,null,null,null,null,null,28,null,"ERC/REC/(01)02"]
["Luxembourg","LUX",0,"31800-33400","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC/(01)02",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan "]
["Latvia","LVA",0,"31800-33400",null,"X",null,null,"X",null,null,null,null,null,null,null,43,null,"ERC/REC/(01)02",null,null,"X",0.2,3,4.5999999999999996,100]
["Netherlands","NLD",0,"31800-33400","X",null,null,null,null,null,null,null,null,"X",null,null,515,null,"ERC/REC/(01)02","x","x","x",0.253,3.57,6.27,30]
["Norway","NOR",0,"31800-33400",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC/(01)02"]
["Norway","NOR",0,"31800-33400","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Portugal","PRT",0,"31800-33400","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,null,null,"Not used at the moment."]
["Russia","RUS",0,"31800-33400","No","No",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02"]
["Russia","RUS",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(04)06"]
["Serbia","SRB",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,null,null,"it have not been used yet"]
["Slovak Republic","SVK",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,100,null,null,"operation expected"]
["Slovenia","SVN",0,"31800-33400","x",null,null,null,"X",null,"X",null,null,null,null,null,"planned Upper part",null,"ERC/REC/(01)02",null,"x","x",0.2,2,4]
["Slovenia","SVN",0,"31800-33400",null,"x",null,null,null,"X",null,null,null,null,"BWA",null,"planned Lower part",null,"ERC/REC/(01)02/ ECC/REC/(04)06",null,"x","x",0.2,1,3,null,null,null,"BWA"]
["Sweden","SWE",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,1887,null,"ERC/REC/(01)02"]
["Sweden","SWE",0,"31800-33400","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(04)06",null,null,null,null,null,null,"Y","N"]
["Telia","TELIASON",0,"31800-33400","X",null,null,null,null,null,"X",null,null,null,null,null,1085,null,"ERC/REC/(01)02",null,996,89,0.2,null,8.6999999999999993,"+",null,null,null,"NEC NEO"]
[]
["Russia","RUS",0,"36000-37000","X","X",null,null,null,null,"X",null,null,null,null,null,132,null,"F.749 ITU-R","X","X","X",0.1,3,5]
[]
["Austria","AUT",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,5273,null,"T/R 12-01","x","x","x",1,5,17]
["Bosnia and Herzegovina","BIH",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,1,23,null,"T/R 12-01","X",null,null,"0.1",1,5,"+5"]
["switzerland","CHE",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,3134,null,"T/R 12-01",1248,1886,null,1,2.6,7.9,"unchanged","city areas congested, HIGH/LOW situation"]
["Cyprus","CYP",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 12-01"]
["Czech Republic","CZE",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,5603,null,"T/R 12-01",null,null,null,null,null,null,5]
["Denmark","DNK",0,"37000-39500","X",null,null,null,null,null,null,null,null,null,null,null,158,null,"T/R 12-01"]
["Denmark","DNK",0,"37000-39500",null,"X",null,null,null,null,null,null,null,null,null,null,"No info"]
["Estonia","EST",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,232,null,"T/R 12-01",169,63,null,0.7,5,10,"+10"]
["Finland","FIN",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,45,null,"T/R 12-01",null,"X","X",0.2,1.7,6.1,0.1]
["France","FRA",0,"37000-39500","X","X",null,null,"X",null,"X",null,null,null,null,null,8304,null,"T/R 12-01",2223,6057,24,0.1,"0<x>6",15,"+8%"]
["UK","GBR",0,"37000-39500","X",null,null,null,null,null,null,null,null,"X",null,12050,null,null,"T/R 12-01","X","X","X"]
["Germany","GER",0,"37000-39500","x",null,null,null,"x",null,null,null,null,null,null,30594,null,null,"ERC/REC 12-01 ",null,"x",null,0.02,2.2999999999999998,13.2]
["Greece","GRC",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,984,null,"T/R 12-01",null,"X","X","0.05","1.5","6.8",0.2]
["Croatia","HRV",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,335,null,"T/R 12-01",null,"x",null,7.0000000000000007E-2,0.42,4.9000000000000004,20]
["Hungary","HUN",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,6454,null,"T/R 12-01","X","X","X",null,4]
["Hungary","HUN",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,"37926-38178 and 39186-39500 MHz Non-Civil P-P links.   39186-39500 MHz Emergency services. 37-39.5 GHz NJFA military requirement for existing and future fixed systems.",null,100,null,"ERC/DEC/(00)02","X","X","X"]
["Iceland","ICE",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,1,null,"T/R 12-01",1,null,null,null,5]
["Ireland","IRL",0,"37000-39500"," X",null,null,null,null,null,"X",null,null,null,null,null,2924,null,"T/R 12-01"," X","X","X",1.6E-2,1.9,10.7," 31"," X"]
["Ireland","IRL",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Italy","ITA",0,"37000-39500","X","X",null,null,"X",null,"X",null,null,null,null,null,10412,null,"T/R 12-01","X","X","X",null,"0,8/10",null,0.25,"yes"]
["Lithuania","LTU",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,268,null,"T/R 12-01",null,268]
["Luxembourg","LUX",0,"37000-39500","X",null,null,null,"X",null,"X",null,"X",null,null,1,110,null,"T/R 12-01",null,"X",null,0.13,"1-6",5.4,"N/A","NO","NO"]
["Luxembourg","LUX",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Latvia","LVA",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,27,null,"T/R 12-01",null,null,"X",0.2,3,4.7,20]
["Netherlands","NLD",0,"37000-39500","X",null,null,null,null,null,null,null,null,"X",null,null,6377,null,"T/R 12-01","x","x","x",0.05,2.15,10.266,30]
["Norway","NOR",0,"37000-39500",null,"x",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 12-01 Annex A"]
["Norway","NOR",0,"37000-39500","X",null,null,null,null,null,null,null,null,"X",null,null,64,null,null,null,null,"x",0.1,3.6,16.399999999999999]
["Norway","NOR",0,"37000-39500"]
["Portugal","PRT",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,"FS",null,617,null,"T/R 12-01","X","X","X",0,"2",6,5]
["Russia","RUS",0,"37000-39500","X","X",null,null,null,null,"X",null,null,null,null,null,16865,null,"T/R 12-01","X","X","X",0.1,3,5]
["Russia","RUS",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.749 ITU-R"]
["Serbia","SRB",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,426,null,"T/R 12-01","X","X","X",0.16,1.4,4.8600000000000003,300]
["Slovak Republic","SVK",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,1600,null,"T/R 12-01","x","x","x",0.1,2,9,20]
["Slovenia","SVN",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,580,null,"T/R 12-01",null,"x",null,0.1,2,4,30,"x***",null,null,"HI/LO problem"]
["Slovenia","SVN",0,"37000-39500","X",null,null,null,"X",null,"X"]
["Sweden","SWE",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,6188,null,"T/R 12-01"]
["Sweden","SWE",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"T/R 12-01",null,null,null,null,null,null,"Y","N"]
["Telia","TELIASON",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,173,null,"T/R 12-01",95,78,null,0.1,null,5.4,0,null,null,null,"Ericsson ML"]
[]
["Austria","AUT",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Bosnia and Herzegovina","BIH",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["switzerland","CHE",0,"40500-43500","X",null,null,null,"X",null,"X",null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"growth. Starts now"]
["Cyprus","CYP",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Czech Republic","CZE",0,"40500-43500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"yes",null,null,"P-P and P-MP planned"]
["Denmark","DNK",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Estonia","EST",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Finland","FIN",0,"40500-43500","X",null,null,null,null,null,"X",null,null,null,null,null,null,null,"ECC/REC/(01)04",null,"X","X",null,null,null,null,null,null,"Opens 2011"]
["France","FRA",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Germany","GER",0,"40500-43500","x",null,null,null,"x",null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,"x",null,null,null,null,null,null,"will be opened 2011"]
["Greece","GRC",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Use"]
["Croatia","HRV",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Hungary","HUN",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Iceland","ICE",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Ireland","IRL",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Italy","ITA",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Lithuania","LTU",0,"40500-43500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,0,"ECC/REC/(01)04"]
["Luxembourg","LUX",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Latvia","LVA",0,"40500-43500",null,"X",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,null,null,null,"MWS (MVDS)"]
["Netherlands","NLD",0,"40500-43500","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,100]
["Norway","NOR",0,"40500-43500",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ECC/REC/(01)04 Annex A"]
["Norway","NOR",0,"40500-43500","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Portugal","PRT",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,"MWS, MVDS",null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"Planned "]
["Russia","RUS",0,"40500-43500","X","X",null,null,null,"X","X",null,null,null,null,null,73,null,"ECC/REC/(01)04","X","X","X",0.1,3,5]
["Serbia","SRB",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["Slovak Republic","SVK",0,"40500-43500",null,"X",null,null,null,"X",null,null,"X",null,null,null,null,3,"ECC/REC/(01)04",null,"x"]
["Slovenia","SVN",0,"40500-43500",null,"X",null,null,null,"X",null,null,null,null,"MWS",null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"planned Upper part",null,null,"MWS"]
["Slovenia","SVN",0,"40500-43500","X",null,null,null,"X",null,"X",null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"planned Lower part (only small part)"]
["Sweden","SWE",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04\n(New ITU-R Rec under dev.)",null,null,null,null,null,null,"Y","N",null,"Blockassignments?"]
["Telia","TELIASON",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
[]
["Czech Republic","CZE",0,"47200-48500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["Latvia","LVA",0,"47200-48500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAP/SAB, HAPS "]
["Portugal","POR",0,"47200-48500",null,null,null,null,null,null,null,null,null,null,"HDFSS (47.5-47.9 GHz)"]
["Russia","RUS",0,"47200-48500"]
[]
["Czech Republic","CZE",0,"48500-50200","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["Hungary","HUN",0,"48500-50200",null,null,null,null,"X",null,null,null,null,null,"Non-Civil Digital P-P links",null,null,null,"ERC/REC 12-10"]
["Lithuania","LTU",0,"48500-50200","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 12-10"]
["Luxembourg","LUX",0,"48500-50200","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-10",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"48500-50200","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"Fixed links"]
["Norway","NOR",0,"48500-50200","X","X",null,null,null,null,null,null,null,"X",null,null,0,null,"ERC/REC 12-10"]
["Portugal","POR",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,"HDFSS (48.2-48.54 GHz and 49.44-50.2 GHz)",null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,"Planned"]
["Russia","RUS",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10"]
["Serbia","SRB",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Slovenia","SVN",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,null,null,"planned",null,"ERC/REC 12-10"]
[]
["Czech Republic","CZE",0,"50400-51400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["Denmark","DNK",0,"50400-51400","X",null,null,null,null,null,null,null,null,null,null,null,1]
["Latvia","LVA",0,"50400-51400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Future satellite and terrestrial applications"]
["Portugal","POR",0,"50400-51400",null,null,null,null,null,null,null,null,null,"X"]
["Russia","RUS",0,"50400-51400"]
[]
["switzerland","CHE",0,"51400-52600",null,"X",null,null,"X",null,"X",null,null,null,null,null,837,null,"ERC/REC 12-11",193,644,null,0.15,0.8,2.8,"growth"]
["Czech Republic","CZE",0,"51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["UK","GBR",0,"51400-52600","X",null,null,null,null,null,null,null,null,null,null,0,null,null,"ERC/REC 12-11"]
["Germany","GER",0,"51400-52600","x",null,null,null,"x",null,null,null,null,null,null,null,null,0,"ERC/REC 12-11",null,"x"]
["Hungary","HUN",0,"51400-52600","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,null,null,"30 original value"]
["Lithuania","LTU",0,"51400-52600","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 12-11"]
["Luxembourg","LUX",0,"51400-52600","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-11",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"51400-52600","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"Fixed links"]
["Portugal","POR",0,"51400-52600",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,"Planned"]
["Russia","RUS",0,"51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11"]
["Serbia","SRB",0,"51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Slovenia","SVN",0,"51400-52600","X",null,null,null,"X",null,"X",null,null,null,null,null,"planned",null,"ERC/REC 12-11",null,"x","x",0.1,2,4]
[]
["switzerland","CHE",0,"55780-57000",null,"X",null,null,"X",null,"X",null,null,null,null,null,0,null,"ERC/REC 12-12",null,null,null,null,null,null,"no equipment available"]
["Czech Republic","CZE",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["UK","GBR",0,"55780-57000","X",null,null,null,null,null,null,null,null,null,null,0,null,null,"ERC/REC 12-12"]
["Germany","GER",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,0,"ERC/REC 12-12",null,"x",null,null,null,null,null,null,null,"not open"]
["Greece","GRC",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12 Annex 3",null,null,null,null,null,null,"Maximum PFD=-26dBW/MHz",null,null,"No current use. Allocation for digital P-P links"]
["Hungary","HUN",0,"55780-57000","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,30]
["Luxembourg","LUX",0,"55780-57000","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-12",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"55780-57000","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"Fixed links"]
["Norway","NOR",0,"55780-57000","X","X",null,null,null,null,null,null,null,"X",null,null,0,null,"ERC/REC 12-09"]
["Portugal","POR",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,"EESS",null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,"Planned"]
["Russia","RUS",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12"]
["Serbia","SRB",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Slovenia","SVN",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,"planned",null,"ERC/REC 12-12"]
["Sweden","SWE",0,"55780-57000",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,"N"]
[]
["switzerland","CHE",0,"57000-58000",null,"X",null,null,"X",null,"X",null,null,null,null,null,292,null,"ECC/REC/(09)01",292,null,null,0.1,0.3,2.2000000000000002,"reduction"]
[]
["Czech Republic","CZE",0,"57000-59000","X",null,null,null,"X",null,null,null,null,null,null,null,3,null,"ECC/REC/(09)01",null,null,null,null,null,null,"yes"]
["UK","GBR",0,"57000-59000",null,null,null,"X",null,null,null,null,null,"X",null,null,null,null,"no channel plan"]
["Greece","GRC",0,"57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-09 Annex A",null,null,null,null,null,null,"Radio Frequency Rights of Use not required. Maximum EIRP=15dBW",null,null,"No current use. Allocation for digital P-P links"]
["Hungary","HUN",0,"57000-59000","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,null,null,"25 original"]
["Ireland","IRL",0,"57000-59000","X",null,null,null,null,null," X",null,null,null,null,null,1,null,"ECC/REC/(09)01\nNational Legislation: S.I. 370 of 2009"," X",null,null,1.4,1.4,1.4," 0"]
["Luxembourg","LUX",0,"57000-59000","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"57000-59000",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"SRD, Fixed links, FWA"]
["Portugal","POR",0,"57000-59000","?","?",null,null,"X","X","X",null,null,null,"EESS, SRD",null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"No use at the moment."]
["Russia","RUS",0,"57000-59000","X","X",null,null,null,null,"X",null,null,null,null,null,420,null,"ECC/REC/(09)01","X","X",null,0.1,1,2]
["Russia","RUS",0,"57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.1497 ITU-R"]
["Serbia","SRB",0,"57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Slovenia","SVN",0,"57000-59000",null,null,null,"X","X",null,null,null,null,null,null,null,"N/A",null,"ECC/REC/(09)01",null,null,"x",null,1,null,"N/A"]
["Sweden","SWE",0,"57000-59000",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Y","N",null,"Exemption"]
[]
["Norway","NOR",0,"57000-64000","X","X",null,null,null,null,null,null,null,"X",null,null,1,null,"ECC/REC/(09)01",null,null,1,null,0.4]
[]
["Germany","GER",0,"57100-58900",null,null,null,"x","x",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01","x"]
[]
["switzerland","CHE",0,"58000-63000",null,null,null,"X",null,null,null,null,null,null,null,null,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"no equipment available"]
[]
["Germany","GER",0,"59000-63000",null,null,null,"x","x",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,"x"]
[]
["Czech Republic","CZE",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,"MD shared",null,null,null,"ECC/REC/(09)01"]
["UK","GBR",0,"59000-64000",null,null,null,"X",null,null,null,null,null,"X",null,null,null,null,"no channel plan"]
["Hungary","HUN",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,"59000-61000 MHz Harmonized NATO band type 2. (planned for P-P)",null,null,null,"ECC/REC/(09)01"]
["Luxembourg","LUX",0,"59000-64000","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"N/A","NO","NO"]
["Latvia","LVA",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"SRD,  Military band 59-61 GHz"]
["Portugal","POR",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,"SRD, ISM, Military (59-61 GHz)",null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Planned"]
["Russia","RUS",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01"]
["Serbia","SRB",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Sweden","SWE",0,"59000-64000",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Y","N",null,"Exemption"]
[]
["Russia","RUS",0,"71000-76000 and  81000-86000",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07"]
["switzerland","CHE",0,"71000-76000 and  81000-86000","X",null,null,null,"X",null,"X",null,null,null,null,null,"starts now",null,"ECC/REC/(05)07",null,null,null,null,null,null,"equipment not clear defined"]
["Czech Republic","CZE",0,"71000-76000 and  81000-86000",null,null,null,"X","X",null,null,null,null,null,null,null,57,null,"ECC/REC/(05)07",null,null,null,null,null,null,100]
["France","FRA",0,"71000-76000 and  81000-86000","X",null,null,null,"X",null,"X",null,null,null,null,null,0,null,"ECC/REC/(05)07"]
["UK","GBR",0,"71000-76000 and  81000-86000","X",null,null,null,null,null,null,null,null,"X",null,null,30,null,"no channel plan",null,null,"X"]
["Germany","GER",0,"71000-76000 and  81000-86000","x",null,null,null,"x",null,null,null,null,null,null,null,null,0,"ECC/REC/(05)07",null,null,"x"]
["Greece","GRC",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"No current use. Allocation for digital P-P links"]
["Hungary","HUN",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,"71000-74000 and 81000-84000 MHz Common Civil and Non-Civil band for P-P links",null,null,null,"ECC/REC/(05)07"]
["Ireland","IRL",0,"71000-76000 and  81000-86000","X",null,null,null,null,null," X",null,null,null,null,null,5,null,"ECC/REC/(05)07\nNational Legislation: S.I. 370 of 2009",null,null," X",0.1,1,2.9," 0"]
["Lithuania","LTU",0,"71000-76000 and  81000-86000",null,null,null,"X","X",null,null,null,null,null,null,0,0,null,"ECC/REC/(05)07"]
["Latvia","LVA",0,"71000-76000 and  81000-86000","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"Military band 71-74 GHz, 81-84 GHz. Fixed links 74-76GHz, 84-86 GHz"]
["Norway","NOR",0,"71000-76000 and  81000-86000","X","X",null,null,null,null,null,null,null,"X",null,null,4,null,"ECC/REC/(05)07",null,null,"x",1,1.8,3.4]
["Portugal","POR",0,"71000-76000 and  81000-86000","?","?",null,null,"X","X","X",null,null,null,"SRD, AM (75.5-76 GHz), Military (71-74 GHz and 81-84 GHz)",null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,"No use at the moment."]
["Serbia","SRB",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Sweden","SWE",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,"Y","N",null,"Light Lic?"]
[]
["Slovenia","SVN",0,"74000-76000 and 84000-86000","X",null,null,null,"X",null,null,null,null,"X",null,null,"planned",null,"ECC/REC/(05)07",null,null,"x"]
[]
["Czech Republic","CZE",0,"92000-95000","X",null,null,null,"X",null,null,null,null,null,null,null,3]
["Hungary","HUN",0,"92000-95000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5.149"]
["Latvia","LVA",0,"92000-95000"]
["Portugal","POR",0,"92000-95000",null,null,null,null,null,null,null,null,null,"X"]
["Russia","RUS",0,"92000-95000",null,null,null,"X"]
["Sweden","SWE",0,"92000-95000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N",null,"Light Lic?"]

{"sheet":"Ranges summary","index":4,"n_rows":90,"n_cols":80,"rows_kept":90,"cut":false,"hidden":false,"merged":[[499,32,500,32],[499,4,500,4],[499,14,500,14],[499,15,500,15],[499,16,500,16],[499,22,500,22],[499,23,500,23],[499,24,500,24],[499,28,500,28],[499,30,500,30],[499,31,500,31]]}
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,63,64,65,66,67,68,69,70,71,72,73,74,75,76,77,78,79,80]
["Respondent","Country code","Band index","Frequency band (MHz)","Licensing regime",null,null,null,null," Topo-logy",null,null,"Application",null,null,null,null,"Number of P-P links",null,"Number of CS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)",null,"Link characteristics",null,null,null,null,null,"Future trends (e.g. in the next 5 years)"]
[null,null,null,null,null,null,null,null,null,"FWA",null,null,"Network Infrastruc-ture",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop length (km)"]
[null,null,null,null,"Link by link","Block","Light licensed","Licence exempt","link-by-link + Block","P-P","P-MP","PtP + PMP","Mobile backhaul","Others","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"National plans","LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth","Anticipated reduction","Currently congested","Planned reallocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
[1,0.38500000000000001,1,"370-400",1,null,null,null,null,null,null,null,null,null,1,null,null,129,null,null,null,null,1,null,null,1,null,100]
[24,1.4335,2,"1350-1375 and 1492-1517",18,4,null,null,1,9,5,1,7,null,4,5,null,998,230,113,27,2,15,2,1,0.02,null,90,7,3,3,2]
[26,1.4135,3,"1375-1400 and 1427-1452",22,2,null,null,1,13,4,3,9,null,4,4,null,130,1623,57,25,1,15,2,null,0.1,null,95,6,2,null,2]
[1,1.4624999999999999,4,"1400-1525",1,null,null,null,null,null,null,null,1,null,null,null,null,null,530,null,null,1,1]
[1,1.4784999999999999,5,"1427-1530",1,null,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,null,null,1,null,1]
[2,1.5209999999999999,6,"1517-1525",2,null,null,null,null,1,null,null,null,null,2,null,null,457,null,null,null,2,2,null,null,2,null,52,1,1,null,1]
[1,1.5275000000000001,7,"1525-1530",1,null,null,null,null,1,null,null,null,null,1,null,null,6,null,null,null,1,1,null,null,2,null,52,null,1,null,1]
[1,1.75,8,"1700-1710 and 1785-1800",1,null,null,null,null,null,null,null,null,null,1,null,null,615,null,null,null,1,1,1,null,0.4,null,90]
[28,2.1575000000000002,9,"2025-2110 and 2200-2290",20,2,null,null,2,6,5,null,7,null,4,2,1,316,600,121,27,4,11,8,1,0.09,null,238.26,5,1,null,1]
[1,2.35,10,"2300-2400",1,null,null,null,null,1,null,null,null,null,null,null,null,null,275,null,null,1,1]
[27,3.5,11,"3400-3600",8,20,null,1,3,6,21,5,6,null,3,null,1,9,2427,12423,26,null,5,6,1,2,null,135,9,2,null,1]
[1,3.5049999999999999,12,"3410-3600",1,1,null,null,null,null,null,null,null,null,null,2,null,null,null,null,1]
[6,3.7,13,"3600-3800",5,5,null,null,null,4,4,1,null,null,3,2,null,10,152,66,8,null,null,3,4,10,null,90,1,2,null,3]
[22,3.9,14,"3600-4200",15,7,null,null,1,8,4,1,10,null,9,3,1,307,1381,175,25,1,2,8,9,2,null,238.26,3,4,null,1]
[7,4,15,"3800-4200",8,1,null,null,null,4,null,null,2,null,3,2,null,298,668,null,8,null,null,2,5,2.5,null,101,1,1,2]
[9,4.7,16,"4400-5000",3,1,null,null,1,1,1,1,1,null,2,2,null,null,484,null,1,1,2,2,2,40,null,90,null,null,null,1]
[1,5.7874999999999996,17,"5725-5795 and 5815-5850",null,null,null,1,null,null,null,null,null,null,null,1,null,null,null,null,null,1]
[25,5.8875000000000002,18,"5850-5925",6,3,null,2,1,4,4,1,4,null,4,1,1,189,1379,623,1,2,1,3,2,9.4700000000000006,null,238,2]
[1,6.5250000000000004,19,"5925-6245 and  6425-7125",2,null,null,null,null,2,null,null,null,null,null,null,null,null,56,null,2,null,null,null,2,22,null,52,2]
[3,6.1749999999999998,20,"5925-6425",3,null,null,null,null,2,null,null,1,null,null,1,null,1214,81,null,3,null,null,null,3,8.5,null,67.3,1]
[1,6.1749999999999998,21,"5925–6425 ",2,1,null,null,null,3,null,null,1,null,2,null,null,null,12,null,3,null,null,null,1,5,null,75,2,null,1]
[24,6.5250000000000004,22,"5925-7125",24,2,null,null,2,13,2,1,17,null,6,3,null,144,13245,1942,26,1,2,8,14,0.5,null,134,11,null,4,1]
[3,6.7750000000000004,23,"6425-7125",3,null,null,null,null,2,null,null,1,null,null,1,null,2895,14,null,3,null,null,1,3,4.3,null,103.9,1]
[1,6.77,24,"6430-7110",1,null,null,null,null,1,null,null,1,null,null,null,null,null,2,null,1,null,null,null,1,44,null,54]
[4,7.2750000000000004,25,"7125-7425",6,null,null,null,null,5,null,null,3,null,1,1,null,917,245,null,5,null,1,2,4,4.2,null,96,3,1,2,1]
[1,7.4249999999999998,26,"7125-7725",1,null,null,null,null,null,null,null,1,null,null,null,null,null,138,null,1,null,1,1,1,11.67,null,104.2,1]
[19,7.4375,27,"7125-7750",23,1,null,null,1,11,null,null,16,null,5,1,null,42,14792,null,23,1,9,15,13,0.49,null,99.5,8,1,4,2]
[1,7.4625000000000004,28,"7125-7800",1,null,null,null,null,1,null,null,null,null,null,null,null,null,104,null,1,null,null,null,1,14,null,54,1]
[1,7.5750000000000002,29,"7425–7725",2,null,null,null,null,2,null,null,1,null,1,null,null,null,31,null,2,null,null,null,2,3,null,60,2]
[5,7.5750000000000002,30,"7425-7725",5,null,null,null,null,3,null,null,2,null,null,1,null,3157,3159,null,3,null,2,3,3,1,null,113,2,null,1]
[1,7.6624999999999996,31,"7425-7900",1,null,null,null,null,null,null,null,null,null,null,1,null,940,null,null,1,null,1,1,1]
[1,8,32,"7700-8300",1,null,null,null,null,1,null,null,1,null,null,null,null,null,35,null,1,null,null,null,1,8,null,58,null,1,null,1]
[4,8,33,"7725–8275",4,null,null,null,null,1,null,null,3,null,2,null,null,40,1350,null,4,null,null,3,4,2,null,150,3,null,2]
[19,7.8250000000000002,34,"7750-7900",6,null,null,null,null,3,null,null,3,null,5,null,null,45,179,null,1,2,null,3,3,2,null,91.4,2,null,1,1]
[1,7.85,35,"7800-7900"]
[1,8.0500000000000007,36,"7900-8200",null,1,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1]
[21,8.1999999999999993,37,"7900-8500",19,1,null,null,1,9,null,null,11,null,5,null,null,25,10626,null,19,2,5,9,7,0.04,null,105,6,1,1,1]
[3,8.3874999999999993,38,"8275-8500",3,null,null,null,null,1,null,null,3,null,null,null,null,null,41,null,3,null,null,3,1,7,null,98.71,2,null,2]
[1,8.3874999999999993,39,"8275-8500 ",1,null,null,null,null,null,null,null,1,null,null,null,null,null,170,null,1,null,1,1,null,1.8,null,120]
[27,10.34,40,"10000-10680",20,7,null,1,1,9,6,1,6,null,12,1,null,2662,721,1754,29,3,6,12,5,0.53,null,114.99,8,3,null,3]
[1,10.4,41,"10150-10300 and 10500-10650",1,1,null,null,null,1,1,null,1,null,null,null,null,null,null,6,2,null,null,null,null,null,null,null,1]
[1,10.4,42,"10300-10500",1,null,null,null,null,1,null,null,1,null,null,null,null,null,420,null,1]
[27,11.2,43,"10700-11700",23,2,null,null,1,11,1,null,15,null,8,2,null,146,7152,1846,30,1,2,7,14,0.3,null,66.5,14,1]
[27,12.1,44,"11700-12500",3,3,null,1,null,1,1,null,1,null,4,null,null,63,1,195,null,1,null,2,2,1.97,null,62.94,3,null,1]
[29,13,45,"12750-13250",33,3,null,null,1,17,null,null,20,null,5,4,null,7951,43362,7,31,2,11,18,17,0.1,null,103,15,1,8,1]
[28,14.375,46,"14250-14500",4,1,null,null,1,1,null,null,1,null,2,null,null,1044,524,null,1,1,1,2,2,3,null,100,1]
[1,14.875,47,"14400-15350",1,null,null,null,null,null,null,null,1,null,null,null,null,null,162,null,1,null,1,1,null,1,null,45]
[29,14.925000000000001,48,"14500-14620 and 15230-15350",27,1,null,null,1,14,null,null,15,null,4,2,null,12329,34505,null,28,2,12,18,9,0.1,null,75,9,2,4,1]
[1,14.879,49,"14613-14725 and 15033-15145",1,null,null,null,null,1,null,null,1,null,null,null,null,null,82,null,2,null,null,1,null,7,null,45,null,1,null,2]
[8,17.5,50,"17300-17700",1,null,null,null,null,1,null,null,null,null,null,null,null,null,33,null,null,1,null,1]
[15,18.7,51,"17700-19700",21,4,null,null,2,11,null,null,14,null,1,4,null,71,50762,null,18,1,5,10,14,0.91,null,45,13,null,4,1]
[11,21.6,52,"21200-22000",9,null,null,null,null,3,null,null,3,null,4,null,null,31,360,null,2,2,4,3,1,0.19,null,20,1,null,2]
[1,22.4,53,"21200-23600",1,1,null,null,1,null,null,null,null,null,null,null,null,null,16816,null,1,null,1,1,1,2,null,8]
[27,22.8,54,"22000-22600 and 23000-23600",30,4,null,null,2,18,null,null,18,null,1,4,null,24156,55535,null,29,1,13,17,13,0.1,null,51.1,17,1,7,1]
[1,22.8,55,"22000-23600",1,null,null,null,null,null,null,null,1,null,null,null,null,null,1724,null,1,null,1,1,1,4,null,16,1]
[1,22.65,56,"22600-22700"]
[12,22.8,57,"22600-23000",10,null,null,null,null,6,null,null,4,null,5,1,null,134,125,null,5,1,4,4,null,0.1,null,32,1,null,1,1]
[1,22.85,58,"22700-23000"]
[10,24.375,59,"24250-24500",4,2,null,null,1,3,2,1,2,null,2,null,null,null,52,35,1,null,1,2,1,null,null,null,1,null,1,2]
[1,25.1265,60,"24500-24745/25500-25753",null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,133,1,null,null,null,null,null,null,null,1]
[28,25.5,61,"24500-26500",22,22,null,null,4,16,19,6,17,null,2,5,null,19453,13168,1513,33,4,11,18,12,0.05,null,24,17,1,2,2]
[1,25.622499999999999,62,"24745-25500/25753-26500",1,null,null,null,null,1,null,null,null,null,null,null,null,null,4537,null,null,null,null,null,null,null,null,null,1]
[8,27,63,"26500-27500",1,1,null,null,1,1,1,null,1,null,null,1,null,null,26,null,1,null,1,1,1,2,null,8,null,null,1]
[29,28.5,64,"27500-29500",13,15,null,null,3,11,13,5,10,null,1,3,null,1424,1047,183,29,null,3,7,7,0.1,null,13.3,9,null,1]
[9,31.15,65,"31000-31300",5,null,null,null,null,4,null,null,1,null,null,null,1,null,null,null,8,1,1,2,1,null,null,null,1,null,1,1]
[29,32.6,66,"31800-33400",13,5,null,null,1,10,2,1,6,null,null,3,null,1466,3711,null,23,null,1,5,5,0.1,null,8.6999999999999993,8,null,2,1]
[1,36.5,67,"36000-37000",1,1,null,null,1,null,null,null,1,null,null,null,null,null,132,null,1,null,1,1,1,0.1,null,5]
[29,38.25,68,"37000-39500",28,5,null,null,3,16,null,null,17,null,1,4,1,42646,77277,null,3,1,12,17,15,0.1,null,68,15,null,2,1]
[28,42,69,"40500-43500",8,6,null,null,1,4,4,null,4,null,1,2,null,null,73,3,27,null,1,3,3,0.1,null,5,2]
[4,47.85,70,"47200-48500",1,null,null,null,null,1]
[10,49.35,71,"48500-50200",5,1,null,null,1,4,null,null,1,null,null,1,null,null,null,null,10,null,null,null,null,null,null,null,null,null,null,1]
[5,50.9,72,"50400-51400",1,null,null,null,null,null,null,null,null,null,null,1,null,null,1]
[12,52,73,"51400-52600",7,1,null,null,null,6,null,null,3,null,null,1,null,null,837,null,12,null,null,2,1,0.1,null,4,1,null,null,1]
[14,56.39,74,"55780-57000",5,2,null,1,1,4,null,null,2,null,null,1,null,null,null,null,14,null,null,1,null,null,null,null,null,null,null,1]
[1,57.5,75,"57000-58000",null,1,null,null,null,1,null,null,1,null,null,null,null,null,292,null,1,null,null,null,null,0.1,null,2.2000000000000002,null,1]
[12,58,76,"57000-59000",5,1,null,4,1,6,2,2,4,null,null,1,null,null,424,null,12,1,2,1,1,0.1,null,2,null,1,null,1]
[1,60.5,77,"57000-64000",1,1,null,null,1,null,null,null,null,null,null,1,null,null,1,null,1]
[1,58,78,"57100-58900",null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1]
[1,60.5,79,"58000-63000",null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1]
[1,61,80,"59000-63000",null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,null,1]
[9,61.5,81,"59000-64000",1,null,null,2,null,2,null,null,1,null,null,1,null,null,null,null,8,null,null,null,null,null,null,null,null,null,null,1]
[15,78.5,82,"71000-76000 and  81000-86000",7,1,null,3,1,6,1,1,4,null,null,2,null,null,96,null,14,1,null,null,4,0.1,null,3.4,1]
[1,80,83,"74000-76000 and 84000-86000",1,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,1,null,null,null,1]
[6,93.5,84,"92000-95000",1,null,null,1,null,1,null,null,null,null,null,1,null,null,3]
[]
[null,null,null,null,540,145,0,20,44,313,105,31,290,0,121,81,6,126459,367990,21195,637,48,177,245,223,null,null,null,223,34,60,43]

{"sheet":"Sheet1","index":5,"n_rows":49,"n_cols":80,"rows_kept":49,"cut":false,"hidden":false,"merged":[]}
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,63,64,65,66,67,68,69,70,71,72,73,74,75,76,77,78,79,80]
[null,null,"Frequency (GHz)",null,"Licensing regime",null,null,null,null," Topo-logy",null,null,"Application",null,null,null,null,"Number of P-P links",null,"Number of CS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)",null,"Link characteristics",null,null,null,null,null,"Future trends (e.g. in the next 5 years)"]
[null,null,null,null,null,null,null,null,null,"FWA",null,null,"Network Infrastruc-ture",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop length (km)"]
[null,null,null,null,"Link by link","Block","Light licensed","Licence exempt","link-by-link + Block","P-P","P-MP","PtP + PMP","Mobile backhaul","Others","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"National plans","LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth","Anticipated reduction","Currently congested","Planned reallocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
[null,null,0,null,1,null,null,null,null,null,null,null,null,null,1,null,null,129,null,null,null,null,1]
[null,null,1,null,46,6,null,null,2,24,10,4,17,null,12,9,null,2206,2383,170,52,8,36,5,1,null,null,null,14,8,3,7]
[null,null,2,null,21,2,null,null,2,7,5,null,7,null,4,2,1,316,875,121,27,5,12,8,1,null,null,null,5,1,null,1]
[null,null,3,null,29,33,null,1,4,18,29,7,16,null,15,7,2,326,3960,12664,60,1,7,17,14,null,null,null,13,8,null,5]
[null,null,4,null,11,2,null,null,1,5,1,1,3,null,5,4,null,298,1152,null,9,1,2,4,7,null,null,null,1,1,2,1]
[null,null,5,null,6,3,null,3,1,4,4,1,4,null,4,2,1,189,1379,623,1,3,1,3,2,null,null,null,2]
[null,null,6,null,35,3,null,null,2,23,2,1,21,null,8,5,null,4253,13410,1942,38,1,2,9,24,null,null,null,17,null,5,1]
[null,null,7,null,39,1,null,null,1,22,null,null,23,null,7,4,null,5056,18469,null,36,1,14,22,25,null,null,null,17,2,7,3]
[null,null,8,null,5,null,null,null,null,2,null,null,4,null,2,null,null,40,1385,null,5,null,null,3,5,null,null,null,3,1,2,1]
[null,null,7,null,6,null,null,null,null,3,null,null,3,null,5,null,null,45,179,null,1,2,null,3,3,null,null,null,2,null,1,1]
[null,null,8,null,23,2,null,null,1,10,null,null,15,null,5,1,null,25,10837,null,24,2,6,13,8,null,null,null,8,1,3,1]
[null,null,10,null,22,8,null,1,1,11,7,1,8,null,12,1,null,2662,1141,1760,32,3,6,12,5,null,null,null,9,3,null,3]
[null,null,11,null,23,2,null,null,1,11,1,null,15,null,8,2,null,146,7152,1846,30,1,2,7,14,null,null,null,14,1]
[null,null,12,null,3,3,null,1,null,1,1,null,1,null,4,null,null,63,1,195,null,1,null,2,2,null,null,null,3,null,1]
[null,null,13,null,33,3,null,null,1,17,null,null,20,null,5,4,null,7951,43362,7,31,2,11,18,17,null,null,null,15,1,8,1]
[null,null,14,null,33,2,null,null,2,16,null,null,18,null,6,2,null,13373,35273,null,32,3,14,22,11,null,null,null,10,3,4,3]
[null,null,17,null,1,null,null,null,null,1,null,null,null,null,null,null,null,null,33,null,null,1,null,1]
[null,null,18,null,21,4,null,null,2,11,null,null,14,null,1,4,null,71,50762,null,18,1,5,10,14,null,null,null,13,null,4,1]
[null,null,21,null,9,null,null,null,null,3,null,null,3,null,4,null,null,31,360,null,2,2,4,3,1,null,null,null,1,null,2]
[null,null,22,null,42,5,null,null,3,24,null,null,23,null,6,5,null,24290,74200,null,36,2,19,23,15,null,null,null,19,1,8,2]
[null,null,24,null,4,2,null,null,1,3,2,1,2,null,2,null,null,null,52,35,1,null,1,2,1,null,null,null,1,null,1,2]
[null,null,25,null,23,23,null,null,4,17,20,6,17,null,2,5,null,19453,17705,1646,34,4,11,18,12,null,null,null,19,1,2,2]
[null,null,27,null,1,1,null,null,1,1,1,null,1,null,null,1,null,null,26,null,1,null,1,1,1,null,null,null,null,null,1]
[null,null,28,null,13,15,null,null,3,11,13,5,10,null,1,3,null,1424,1047,183,29,null,3,7,7,null,null,null,9,null,1]
[null,null,31,null,5,null,null,null,null,4,null,null,1,null,null,null,1,null,null,null,8,1,1,2,1,null,null,null,1,null,1,1]
[null,null,32,null,13,5,null,null,1,10,2,1,6,null,null,3,null,1466,3711,null,23,null,1,5,5,null,null,null,8,null,2,1]
[null,null,36,null,1,1,null,null,1,null,null,null,1,null,null,null,null,null,132,null,1,null,1,1,1]
[null,null,38,null,28,5,null,null,3,16,null,null,17,null,1,4,1,42646,77277,null,3,1,12,17,15,null,null,null,15,null,2,1]
[null,null,42,null,8,6,null,null,1,4,4,null,4,null,1,2,null,null,73,3,27,null,1,3,3,null,null,null,2]
[null,null,47,null,1,null,null,null,null,1]
[null,null,49,null,5,1,null,null,1,4,null,null,1,null,null,1,null,null,null,null,10,null,null,null,null,null,null,null,null,null,null,1]
[null,null,50,null,1,null,null,null,null,null,null,null,null,null,null,1,null,null,1]
[null,null,52,null,7,1,null,null,null,6,null,null,3,null,null,1,null,null,837,null,12,null,null,2,1,null,null,null,1,null,null,1]
[null,null,56,null,5,2,null,1,1,4,null,null,2,null,null,1,null,null,null,null,14,null,null,1,null,null,null,null,null,null,null,1]
[null,null,57,null,null,1,null,null,null,1,null,null,1,null,null,null,null,null,292,null,1,null,null,null,null,null,null,null,null,1]
[null,null,58,null,5,1,null,4,1,6,2,2,4,null,null,1,null,null,424,null,12,1,2,1,1,null,null,null,null,1,null,1]
[null,null,60,null,1,1,null,null,1,null,null,null,null,null,null,1,null,null,1,null,1]
[null,null,58,null,null,null,null,1,null,1,null,null,null,null,null,null,null,null,null,null,1,null,1]
[null,null,60,null,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,1]
[null,null,61,null,1,null,null,3,null,3,null,null,1,null,null,1,null,null,null,null,9,null,null,null,1,null,null,null,null,null,null,1]
[null,null,78,null,7,1,null,3,1,6,1,1,4,null,null,2,null,null,96,null,14,1,null,null,4,null,null,null,1]
[null,null,80,null,1,null,null,null,null,1,null,null,null,null,null,1,null,null,null,null,1,null,null,null,1]
[null,null,93,null,1,null,null,1,null,1,null,null,null,null,null,1,null,null,3]
[]
[null,null,null,null,{"$f":"SUM(E4:E47)","v":540},145,0,20,44,313,105,31,290,0,121,81,6,126459,367990,21195,637,48,177,245,223,null,null,null,{"$f":"SUM(AC4:AC47)","v":223},{"$f":"SUM(AD4:AD47)","v":34},{"$f":"SUM(AE4:AE47)","v":60},{"$f":"SUM(AF4:AF47)","v":43},{"$f":"SUM(AG4:AG47)","v":0}]

{"sheet":"below 2 GHz","index":6,"n_rows":84,"n_cols":26,"rows_kept":84,"cut":false,"hidden":false,"merged":[[3,11,3,12],[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[0,14,2,14]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L6:M102)","v":9198},null,{"$f":"SUBTOTAL(9,N6:N102)","v":340}]
["BIH","370-400","X",null,null,null,null,null,"X",null,null,129,null,null,null,"X",null,null,1,30,100,null,null,null,"370-400 MHz: Planned migration of P-P links to 1350-1375/1492-1517 and 1375-1400/1427-1452 MHz"]
["TELIASON","1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["TELIASON","1375-1400 and 1427-1452","X",null,null,null,null,"X",null,null,null,null,17,null,"T/R 13-01 Annex B","X",null,null,4,null,19,0,null,null,null,"IDR140"]
["AUT","1350-1375 and 1492-1517","X",null,null,"X",null,"X",null,null,null,null,10,null,"T/R 13-01 Annex A","x",null,null,3,20,60]
["AUT","1375-1400 and 1427-1452","X",null,null,"X",null,"X",null,null,null,null,8,null,"T/R 13-01 Annex B","x",null,null,3,20,60]
["BIH","1350-1375 and 1492-1517","X",null,null,null,null,null,"X",null,null,48,null,null,"T/R 13-01 Annex A","X",null,null,"0.5",7,70,"+15"]
["BIH","1375-1400 and 1427-1452","X",null,null,null,null,null,"X",null,null,5,null,null,"T/R 13-01 Annex B","X",null,null,5,20,90,"+15"]
["HRV","1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["HRV","1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["CZE","1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,"MD",null,null,null,"T/R 13-01 Annex A"]
["CZE","1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,"MD",null,null,null,"T/R 13-01 Annex B"]
["CYP","1350-1375 and 1492-1517","X",null,null," ",null,null,"X",null,null,13,null,null,"T/R 13-01 Annex A","X",null,null,0.9,null,58.65]
["CYP",null,"X",null,null," ",null,null,"X",null,null,17,null,null,null,"X",null,null,0.9,null,73.55]
["CYP","1375-1400 and 1427-1452","X",null,null," ",null,null,"X",null,null,6,null,null,"T/R 13-01 Annex B","X",null,null,3.52,null,35.47]
["CYP",null,"X",null,null," ",null,null,"X",null,null,8,null,null,null,"X",null,null,22.62,null,74.209999999999994]
["DNK","1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["DNK","1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["EST","1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["EST","1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["FIN","1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A",null,null,null,null,null,null,null,null,null,"Planned opening 2011-2012"]
["FIN","1375-1400 and 1427-1452","X",null,null,null,null,"X",null,null,null,null,4,null,"T/R 13-01 Annex B","X","X",null,null,null,null,null,null,null,"Planned closing 2011-2012"]
["FRA","1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["FRA","1375-1400 and 1427-1452","X",null,null,"X",null,"X",null,null,null,null,1259,null,"T/R 13-01 Annex B",1259,null,null,0.1,null,95,"+ 10 %"]
["GRC","1700-1710 and 1785-1800 new row by EETT","X",null,null,null,null,null,"X",null,null,615,null,null,"national plan","X","X",null,0.4,14,90,null,"congested in urban areas"]
["HUN","1350-1375 and 1492-1517","X",null,null,"X","X","X",null,null,"Non-Civil P-P, P-MP systems",null,null,null,"T/R 13-01 Annex A",null,null,null,null,null,null,0.1]
["HUN","1375-1400 and 1427-1452","X",null,null,"X","X",null,null,null,null,null,null,null,"T/R 13-01 Annex B","X",null,null,null,20,null,0.1]
["HUN",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,"X",null,null,null,20]
["ICE","1350-1375 and 1492-1517","x",null,null,"X",null,null,null,null,null,null,0,null,"T/R 13-01 Annex A",null,null,null,null,null,null,0]
["ICE","1375-1400 and 1427-1452","x",null,null,"X",null,null,null,null,null,null,2,null,"T/R 13-01 Annex B",null,null,null,null,25,null,0]
["IRL","1350-1375 and 1492-1517"," X",null,null,null,null," X",null,null,null,0,69,null,"T/R 13-01 Annex A"," X","X","X",0.02,23,83,48,null," X"]
["IRL",null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009 "]
["IRL","1375-1400 and 1427-1452"," X",null,null,null,null," X",null,null,null,37,18,null,"T/R 13-01 Annex B"," X",null,null,0.45,23,69," 0",null," X"]
["IRL",null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009 "]
["ITA","1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["ITA","1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["ITA","1400 - 1525","X",null,null,null,null,"X",null,null,null,null,530,null,"national","X"]
["LVA","1350-1375 and 1492-1517","X",null,null,"X",null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["LVA",null,null,"X",null,null,"X",null,null,null,null,null,null,30,"national plan","X",null,null,null,null,null,-50]
["LVA","1375-1400 and 1427-1452","X",null,null,"X",null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["LTU","1350-1375 and 1492-1517","X",null,null,"X",null,null,null,null,null,0,0,null,"T/R 13-01 Annex A"]
["LTU",null,null,"X",null,null,"X","X",null,null,null,null,null,8,"local",null,null,null,null,null,null,-100]
["LTU","1375-1400 and 1427-1452","X",null,null,"X",null,null,null,null,null,0,0,null,"T/R 13-01 Annex B"]
["LTU",null,null,"X",null,null,"X","X",null,null,null,null,null,8,"local",null,null,null,null,null,null,-100]
["LUX","1350-1375 and 1492-1517","X",null,null,"X",null,"X",null,null,null,0,0,null,"T/R 13-01 Annex A","X",null,null,null,null,null,"N/A","NO","NO"]
["LUX",null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["LUX","1375-1400 and 1427-1452","X",null,null,"X",null,"X",null,null,null,0,0,null,"T/R 13-01 Annex B","X",null,null,null,null,null,"N/A","NO","NO"]
["LUX",null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["NLD","1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["NLD","1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["NLD",null,"X",null,null,null,null,null,null,"X",null,2,7,null,"nat. plan 1427 - 1517","x",null,null,39.299999999999997,58.9,71.400000000000006,10]
["NOR","1350-1375 and 1492-1517","X",null,null,null,null,null,null,"X",null,8,46,null,"T/R 13-01 Annex A","x",null,null,1,12,42]
["NOR","1375-1400 and 1427-1452","X",null,null,null,null,null,null,"X",null,1,26,null,"T/R 13-01 Annex B","x",null,null,1,18,42.5]
["PRT","1350-1375 and 1492-1517","X",null,null,"X",null,null,null,null,null,null,55,null,"T/R 13-01 Annex A","X",null,null,12,"40",57,5]
["PRT",null,"X",null,null,null,"X",null,null,null,null,null,null,9,"T/R 13-01 Annex A","X",null,null,2,"10",18,0]
["PRT","1375-1400 and 1427-1452","X",null,null,"X","X",null,null,null,null,null,null,null,"T/R 13-01 Annex B","X",null,null,null,"40",null,"No use at the moment."]
["PRT","1517-1525","X",null,null,null,null,null,"X",null,null,365,null,null,"National plan (STL)","X",null,null,null,"15",null,5]
["RUS","1350-1375 and 1492-1517","X","X",null,null,null,"X",null,null,null,null,25,49,"T/R 13-01 Annex A","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["RUS","1375-1400 and 1427-1452","X","X",null,null,null,"X",null,null,null,null,30,49,"T/R 13-01 Annex B","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["SRB","1350-1375 and 1492-1517",null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["SRB","1375-1400 and 1427-1452",null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["SVK","1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["SVK","1427 - 1530","X",null,null,null,"X",null,null,null,null,null,null,null,"Rep.CCIR 379-5, DS 65,5MHz","x",null,null,null,null,null,-100,null,"x","no new links"]
["SVK",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"relocation to other band"]
["SVN","1350-1375 and 1492-1517","X",null,null,"X",null,null,"X",null,null,52,null,null,"T/R 13-01 Annex A","x",null,null,2,15,52,100,null,null,"From band 1517.5 - 1530 MHz"]
["SVN",null,null,"X",null,null,null,null,null,"X",null,null,"N/A",null,"T/R 13-01 Annex A","x",null,null,5,20,90,0,"x",null,null,"assigned all SVN (2MHz Ch.1)"]
["SVN",null,"X",null,null,null,"X","X",null,null,null,null,null,17,"T/R 13-01 Annex A","x",null,null,5,15,50,2,"x"]
["SVN",null,"X",null,null,"X",null,"X",null,null,null,null,20,null,"T/R 13-01 Annex A","x",null,null,5,20,90,10,"x"]
["SVN","1375-1400 and 1427-1452","X",null,null,"X",null,null,"X",null,null,12,null,null,"T/R 13-01 Annex B","x",null,null,2,15,52,200,null,null,"From band 1517.5 - 1530 MHz"]
["SVN",null,"X",null,null,"X",null,"X",null,null,null,null,1,null,"T/R 13-01 Annex B",null,null,null,5,10,30,200]
["SVN","1517 - 1525","X",null,null,"X",null,null,"X",null,null,92,null,null,"national (500kHz)","x",null,null,2,15,52,-50,null,"x","realocated into 1.4 GHz bands"]
["SVN","1525 - 1530","X",null,null,"X",null,null,"X",null,null,6,null,null,"national (500kHz)","x",null,null,2,15,52,-100,null,"x","realocated into 1.4 GHz bands"]
["SWE","1375-1400 and 1427-1452","X",null,null,"X",null,null,null,null,null,59,99,null,"T/R 13-01 Annex B",null,null,null,null,null,null,null,"N"]
["CHE","1350-1375 and 1492-1517","X",null,null,"X",null,null,null,"X",null,null,15,null,"T/R 13-01 Annex A",15,null,null,20,null,30.5,"reduction"]
["CHE","1375-1400 and 1427-1452","X",null,null,"X",null,null,null,"X",null,null,152,null,"T/R 13-01 Annex B",152,null,null,20,null,61.9,"reduction"]
["GBR","1350-1375 and 1492-1517","X",null,null,null,null,null,null,"X",null,860,null,null,"T/R 13-01 Annex A","X"]
[]
[null,null,{"$f":"COUNTA(C6:C79)","v":47},{"$f":"COUNTA(D6:D79)","v":6},0,29,10,18,12,9,3,{"$f":"SUM(L6:L79)","v":2206},{"$f":"SUM(M6:M79)","v":2393},{"$f":"SUM(N6:N79)","v":170},null,40,5,1,{"$f":"MIN(S$6:S$79)","v":0.02},{"$f":"MIN(T$6:T$79)","v":7},{"$f":"MIN(U$6:U$79)","v":18}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$6:S$79)","v":3},{"$f":"MEDIAN(T$6:T$79)","v":20},{"$f":"MEDIAN(U$6:U$79)","v":60}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$6:S$79)","v":40},{"$f":"MAX(T$6:T$79)","v":80},{"$f":"MAX(U$6:U$79)","v":95}]
["Note ","PRT","in counting links, for bidirectional links, more than 1 channel counts 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$6:S$79,0.9)","v":25.955999999999989},{"$f":"PERCENTILE(T$6:T$79,0.9)","v":52.120000000000019},{"$f":"PERCENTILE(U$6:U$79,0.9)","v":90}]

{"sheet":"2-3 GHz","index":7,"n_rows":46,"n_cols":25,"rows_kept":46,"cut":false,"hidden":false,"merged":[[3,11,3,12],[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[0,14,2,14],[5,1,6,1],[16,1,17,1],[19,1,20,1],[19,11,20,11],[19,12,20,12],[32,1,33,1],[34,21,34,24],[19,21,20,21],[19,22,20,22],[19,23,20,23],[19,24,20,24],[21,1,24,1],[30,1,31,1],[19,15,20,15],[19,16,20,16],[19,17,20,17],[19,18,20,18],[19,19,20,19],[19,20,20,20],[19,13,20,13]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M101)","v":2382},null,{"$f":"SUBTOTAL(9,N5:N101)","v":242}]
["TELIASON","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["AUT","2025-2110 and 2200-2290","X",null,null,null,null,null,"X",null,"mo",null,null,null,"T/R 13-01 Annex C"]
["AUT",null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["BIH","2025-2110 and 2200-2290","X",null,null,null,null,null,"X",null,null,27,null,null,"T/R 13-01 Annex C","X",null,null,"1",55,99,"+10"]
["HRV","2025-2110 and 2200-2290","X",null,null,null,null,null,"X",null,null,182,null,null,"National plan","X",null,null,0.09,8.9,55.6]
["CZE","2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,"MD shared",null,null,110,"T/R 13-01 Annex C",null,null,null,null,null,null,0]
["CYP","2025-2110 and 2200-2290",null,null," ",null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,"X"]
["DNK","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["EST","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["FIN","2025-2110 and 2200-2290","X",null,null,null,null,"X",null,null,null,null,12,null,"T/R 13-01 Annex C","X","X"]
["FRA","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["GRC","2025-2110 and 2200-2290","X",null,null,null,null,"X",null,null,null,null,206,null,"T/R 13-01 Annex C","X","X",null,0.6,21,60,"reduction"]
["HUN","2025-2110 and 2200-2290","X",null,null,"X",null,null,null,null,"2070-2110 and 2245-2290 MHz Non-Civil digital P-P links",null,3,null,"T/R 13-01 Annex C","X","X",null,null,20]
["HUN",null,"X",null,null,"X",null,null,null,null,"2025-2070 and 2200-2245 MHz NJFA requirement: NATO Tactical Radio Relay",null,null,null,null,"X","X",null,null,20]
["ICE","2025-2110 and 2200-2290","X",null,null,"X",null,null,null,null,null,null,90,null,"T/R 13-01 Annex C",45,45,null,20,40,70,0]
["IRL","2025-2110 and 2200-2290","X",null,null,null,null," X",null,null,null,null,47,null,"T/R 13-01 Annex C"," X","X",null,1.5,24,66," 0"]
["IRL",null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["ITA","2025-2110 and 2200-2290","X",null,null,null,"X","X",null,null,null,12,21,null,"T/R 13-01 Annex C","x",null,null,6.71,30.92,64.77,0.15]
["ITA",null,"X",null,null,null,"X","X",null,null,null,95,3,null,"T/R 13-01 Annex C",null,"x",null,3.28,52.12,238.26,0.15]
["ITA",null,"X",null,null,null,"X","X",null,null,null,null,122,null,"T/R 13-01 Annex C",null,null,"x",0.49,67.06,238.26,0.15]
["ITA",null,"X",null,null,null,"X",null,null,null,null,null,null,10,"T/R 13-01 Annex C","X",null,null,null,null,null,0.05,"stable"]
["ITA","2300-2400","X",null,null,"X",null,null,null,null,null,null,275,null,"national","X"]
["LVA","2025-2110 and 2200-2290","X",null,null,"X",null,null,null,null,null,null,3,null,"T/R 13-01 Annex C","X",null,null,5,null,41]
["LTU","2025-2110 and 2200-2290","X",null,null,"X",null,null,null,"X",null,null,5,null,"T/R 13-01 Annex C",5]
["LUX","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["NLD","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["NOR","2025-2110 and 2200-2290","X","X",null,null,null,null,null,null,"X",null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,null,"SAP/SAB"]
["NOR",null,"X",null,null,null,null,null,null,"X",null,null,2,null,null,null,"x",null,17,19.7,22,null,null,null,"Offshore"]
["PRT","2025-2110 and 2200-2290","X",null,null,"X",null,null,null,null,"TCR, SAP/SAB",null,11,null,"T/R 13-01 Annex C","X",null,null,2,"40",193,0]
["PRT",null,"X",null,null,"X",null,null,null,null,"TCR, SAP/SAB",null,2,null,"National plan",null,"X",null,20,"40",64,0]
["RUS","2025-2110 and 2200-2290","X","X",null,null,null,"X",null,null,null,null,73,1,"T/R 13-01 Annex C","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["SRB","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defense systems"]
["SVK","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["SVN","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["SWE","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["CHE","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,"No civil FS use",null,null,null,"T/R 13-01 Annex C"]
["GBR","2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,null,"row missing in the questionnaire"]
[]
[null,null,{"$f":"COUNTA(C6:C41)","v":22},{"$f":"COUNTA(D6:D41)","v":2},1,8,5,7,4,2,{"$f":"COUNTA(#REF!)","v":1},{"$f":"SUM(L6:L41)","v":316},{"$f":"SUM(M6:M41)","v":875},{"$f":"SUM(N6:N41)","v":121},null,{"$f":"COUNTA(P6:P41)","v":15},{"$f":"COUNTA(Q6:Q41)","v":10},{"$f":"COUNTA(R6:R41)","v":1},{"$f":"MIN(S$5:S$41)","v":0.09},{"$f":"MIN(T$5:T$41)","v":8.9},{"$f":"MIN(U$5:U$41)","v":22}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$41)","v":4.1399999999999997},{"$f":"MEDIAN(T$5:T$41)","v":27.46},{"$f":"MEDIAN(U$5:U$41)","v":66}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$41)","v":40},{"$f":"MAX(T$5:T$41)","v":80},{"$f":"MAX(U$5:U$41)","v":238.26}]
["Note ","PRT","in counting links, for bidirectional links, more than 1 channel counts 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$41,[1]TOT!$S$1)","v":28.999999999999986},{"$f":"PERCENTILE(T$5:T$41,[1]TOT!$S$1)","v":72.882999999999996},{"$f":"PERCENTILE(U$5:U$41,[1]TOT!$S$1)","v":238.26}]

{"sheet":"3-4,2 GHz","index":8,"n_rows":93,"n_cols":27,"rows_kept":93,"cut":false,"hidden":false,"merged":[[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[3,11,3,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,11,2,11],[1,12,2,12],[1,13,2,13],[1,15,1,17],[1,18,1,20],[0,14,2,14]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,"unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)",null,null,null,null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M103)","v":10504},null,{"$f":"SUBTOTAL(9,N5:N103)","v":25328}]
["TELIASON","3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03"]
["AUT","3400-3600","X",null,null,null,"X","X",null,null,null,null,null,240,"ERC/REC 14-03","X",null,null,3,15,30]
["BIH","3400-3600","X",null,null,null,null,"X","X",null,null,9,1,null,"ERC/REC 14-03 Annex B","X","X",null,null,2,null,null,null,null,"3400-3600 MHz: Only two channels are available for P-P links out of FWA systems. We still do not have active implemented FWA systems.\n3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["BIH","3400-3600",null,"X",null,"X","X",null,null,null,null,null,null,null,null,null,"X","X",null,null,null,"+25",null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["HRV","3400-3600",null,"X",null,null,"X",null,null,null,null,null,null,67,"ERC/REC 14-03",null,null,null,null,null,null,-30]
["CZE","3400-3600","X","X",null,"X","X",null,null,null,null,null,null,667,"ERC/REC 14-03",null,null,null,null,null,null,100,null,null,"P-MP, FWA planned"]
["CYP","3400-3600","P.C.",null,null,null,null,null,null,null,null,null,null,null,"2008/411/EC"]
["DNK","3400-3600","X",null,null,null,null,null,null,null,null,null,null,29,"ERC/REC 14-03"]
["DNK","3400-3600",null,"X",null,null,null,null,null,null,null,null,null,null," ",null,null,null,null,null,null,null,null,null,"No info"]
["EST","3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,null,null,null,"No info"]
["FIN","3400-3600",null,"X",null,null,"X",null,null,null,null,null,null,540,"ERC/REC 14-03"]
["FRA","3400-3600","X","X",null,"X","X","X",null,null,null,null,236,1135,"ERC/REC 14-03",236,null,null,2,"20<x>80",135,"-30"]
["GER","3400-3600",null,"x",null,null,"x",null,null,null,null,null,null,392,"ERC/REC 14-03",null,"x"]
["GRC","3400-3600",null,"X",null,"X","X",null,null,null,null,null,null,null,"ERC/REC 14-03","-",null,null,null,null,null,"4 issued licenses"]
["HUN","3400-3600",null," "," ",null," ",null,null,null,null,null,null,null,"ERC/REC 14-03"]
["HUN","3400-3600",null,"X","X",null,"X",null,null,null,null,null,null,383,"ECC/DEC/(07)02",null,null,null,null,null,null,"20"]
["ICE","3400-3600",null,"X",null,null,"X",null,null,null,null,null,null,20,"ERC/REC 14-03",null,null,null,null,10]
["IRL","3400-3600"," X",null,null,null," X",null,null,null,null,null,null,120,"ERC/REC 14-03",null,null,null,null,null,null," 66"]
["ITA","3400-3600",null,"X",null,null,"X",null,null,null,null,null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,null,null,null,"No info"]
["LVA","3400-3600",null,"X",null,null,"X",null,null,null,null,null,null,69,"ERC/REC 14-03",null,"X",null,null,10,null,50]
["LTU","3400-3600","X",null,null,"X",null,null,null,null,null,0,0,null,"ERC/REC 14-03"]
["LTU","3400-3600",null,"X",null,null,"X",null,null,null,null,null,null,402,"ERC/REC 14-03",null,null,null,null,null,null,50,null,null,"Fixed and mobile P-MP (BWA)"]
["LUX","3400-3600",null,"X",null,null,"X","X",null,null,null,null,null,3,"Nat. freq. Plan",null,null,null,null,null,null,"N/A","NO","NO"]
["NLD","3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03"]
["PRT","3400-3600",null,"X",null,null,"X",null,null,null,null,null,null,64,"ERC/REC 14-03","X",null,null,null,"20",null," BWA"]
["RUS","3400-3600","X","X",null,null,"X","X","X",null,null,null,2190,8033,"ERC/REC 14-03","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["SRB","3400-3600",null,"X",null,null,"X",null,null,null,null,null,null,51,"ERC/REC 14-03",null,null,null,null,null,null,50]
["SVK","3400-3600",null,"X",null,null,"X",null,null,null,null,null,null,198,"ERC/REC 14-03","X",null,null,null,null,null,10]
["SVN","3400-3600",null,"X",null,null,"X",null,null,null,"BWA",null,null,10,"ERC/REC 14-03",null,"X",null,5,30,70,400]
["SWE","3400-3600",null,"X",null,"X","X","X","X",null,"X",null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,"Y","N",null,"IMT-?"]
["CHE","3400-3600",null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ERC/REC 14-03"]
["NOR","3410-3600",null,"X",null,null,null,null,null,"X",null,null,null,null,"ERC/REC 14-03 Annex A"]
["NOR","3410-3600","X",null,null,null,null,null,null,"X",null,null,0]
["BIH","3600-3800","X",null,null,null,null,null,"X",null,null,9,null,null,"ERC/REC 12-08",null,"X","X",null,null,null,null,null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["BIH","3600-3800",null,"X",null,"X","X",null,null,null,null,null,null,65,null,null,null,"X",null,null,null,"+25"]
["CZE","3600-3800","X",null,null,"X",null,null,null,null,null,null,150,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,"X","DEC EC/411/EC"]
["GER","3600-3800",null,"x",null,null,"x",null,null,null,null,null,null,0,"ERC/REC 14-03",null,"x"]
["NOR","3600-3800",null,"X",null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-08"]
["NOR","3600-3800","X",null,null,null,null,null,null,"X",null,null,0]
["SRB","3600-3800",null,"X",null,null,"X",null,null,null,null,null,null,1,"ERC/REC 12-08"]
["SVN","3600-3800","X",null,null,"X",null,null,"X",null,null,null,2,null,"ERC/REC 12-08",null,null,"X",null,null,null,-100,null,"x","BWA"]
["SVN","3600-3800","X",null,null,"X",null,null,"X",null,null,1,null,null,"ERC/REC 12-08",null,null,"X",10,45,90,-100,null,"x","BWA"]
["SVN","3600-3800",null,"X",null,null,"X",null,null,null,"BWA",null,null,"planned","ERC/REC 12-08",null,"X",null,null,null,null,">400",null,null,"BWA"]
["TELIASON","3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
["AUT","3600-4200","X",null,null,"X",null,"X",null,null,null,null,90,null,"ERC/REC 12-08",null,"X",null,13,50,100]
["HRV","3600-4200","X",null,null,null,null,null,"X",null,null,null,9,null,"ERC/REC 12-08",null,"X"]
["HRV","3600-4200","X",null,null,null,null,"X",null,null,null,1,70,null,null,null,null,"X",20.2,44.2,91.4,10]
["CYP","3600-4200","P.C. (3.6-3.8 GHz)",null,null,null,null,null,null,null,null,null,null,null,"2008/411/EC"]
["DNK","3600-4200","X",null,null,null,null,null,null,null,null,null,null,21,"ERC/REC 12-08"]
["DNK","3600-4200",null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No info"]
["EST","3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"No info"]
["FIN","3600-4200","X",null,null,null,null,"X","X",null,null,null,160,null,"ERC/REC 12-08",null,null,"X"]
["FIN","3600-4200",null,null,null,null,null,null,"X",null,null,40,null,null,"National","Analog","Analog",null,null,null,null,null,null,null,"Will be phased out"]
["FIN","3600-4200","X",null,null,null,null,null,"X",null,null,120,null,null,"ITU-R F.382","Analog","Analog",null,null,null,null,null,null,null,"Will be phased out"]
["FRA","3600-4200","X",null,null,"X",null,"X",null,null,null,null,11,null,"ERC/REC 12-08",null,null,11,2,"20<x>80",135,"-20"]
["HUN","3600-4200","X"," "," ","X",null,null,null,null,null,null,20,null,"ERC/REC 12-08",null,null,"X",null,30,null,"25"]
["HUN","3600-4200"]
["ICE","3600-4200","X",null,null,"X",null,null,null,null,null,null,7,null,"ERC/REC 12-08",null,null,7,20,30,40,0]
["IRL","3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
["ITA","3600-4200","X",null,null,"X",null,"X",null,null,null,null,77,null,"ERC/REC 12-08",null,null,"X",13.6,60,238,-5]
["ITA","3600-4200","X",null,null,null,null,"X","X",null,null,105,9,null,"ERC/REC 12-08",null,"X","X",17.46,88.5,238.26,-5]
["ITA","3600-4200",null,"X",null,null,null,"X","X",null,null,null,210,null,"ERC/REC 12-08",null,null,"X",13.6,67.34,238.26,-5]
["LVA","3600-4200",null,"X",null,null,"X",null,null,null,null,null,null,154,"ERC/REC 12-08",null,"X",null,null,10,null,50]
["LTU","3600-4200","X",null,null,"X",null,null,null,"X",null,null,30,null,"ERC/REC 12-08",null,null,30]
["LTU","3600-4200",null,"X",null,null,"X",null,null,"X",null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"3600-3800 future for BWA"]
["LUX","3600-4200","X",null,null,"X",null,"X","X",null,null,1,0,null,"Nat. freq. Plan",null,"X","X",null,"20-80",null,"N/A","NO","NO"]
["NLD","3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
["PRT","3600-4200",null,"X",null,null,"X",null,null,null,"VSAT (3.8-4.2 GHz)",null,null,null,"ERC/REC 12-08","X","X",null,null,"20",null,null,null,null,"BWA in 3.3 -3.6GHz and FSS in 3.8-4.2GHz"]
["RUS","3600-4200","X","X",null,null,null,"X","X",null,null,null,688,null,"ERC/REC 12-08","X","X","X",40,80,90]
["RUS","3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,"F.635 ITU-R"]
["SVK","3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"N.A. FWA planned"]
["SWE","3600-4200",null,"X",null,"X","X","X","X",null,"X",null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,"Y","N",null,"IMT-?"]
["CHE","3600-4200",null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ERC/REC 12-08"]
["GBR","3600-4200","X",null,null,null,null,null,null,"X",null,40,null,null,"ERC/REC 12-08",null,"X","X"]
["BIH","3800-4200","X",null,null,null,null,null,"X",null,null,11,3,null,"ERC/REC 12-08 Annex B",null,null,null,27,35,85,"+40"]
["CZE","3800-4200","X",null,null,"X",null,null,null,null,null,null,479,null,"ERC/REC 12-08"]
["GER","3800-4200","x",null,null,"x",null,null,null,null,null,269,null,null,"ERC/REC 12-08",null,null,"x",14.4,42,64.8]
["GRC","3800-4200","X",null,null,null,null,"X",null,null,null,null,163,null,"ERC/REC 12-08 Annex B",null,"X","X",5,55,101,"reduction"]
["NOR","3800-4200",null,"X",null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-08"]
["NOR","3800-4200","X",null,null,null,null,null,null,"X",null,null,2,null,null,null,"X",null,2.5,2.7,2.9,null,null,null,null,null,"Offshore"]
["SRB","3800-4200","X",null,null,null,null,"X",null,null,null,null,3,null,"ITU-R F.382-8",null,null,"X",72.09,74.02,77.89]
["SVN","3800-4200","X",null,null,"X",null,null,"X",null,null,null,18,null,"ERC/REC 12-08",null,null,"X",30,60,90,null,"X*",null,"congested in backbone directions"]
["SVN","3800-4200","X",null,null,"X",null,null,"X",null,null,18,null,null,"ERC/REC 12-08",null,null,"X",10,30,90,null,"X*",null,"congested in backbone directions"]
[]
[null,null,{"$f":"COUNTA(C5:C87)","v":39},{"$f":"COUNTA(D5:D87)","v":36},3,22,30,18,18,9,7,{"$f":"SUM(L5:L87)","v":624},{"$f":"SUM(M5:M87)","v":4628},{"$f":"SUM(N5:N87)","v":12664},null,{"$f":"COUNTA(P5:P87)","v":11},{"$f":"COUNTA(Q5:Q87)","v":21},{"$f":"COUNTA(R5:R87)","v":22},{"$f":"MIN(S$5:S$87)","v":2},{"$f":"MIN(T$5:T$87)","v":2},{"$f":"MIN(U$5:U$87)","v":2.9}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$87)","v":13.6},{"$f":"MEDIAN(T$5:T$87)","v":42},{"$f":"MEDIAN(U$5:U$87)","v":90}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$87)","v":72.09},{"$f":"MAX(T$5:T$87)","v":88.5},{"$f":"MAX(U$5:U$87)","v":238.26}]
["Note ","PRT","in counting links, for bidirectional links, more than 1 channel counts 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$87,0.9)","v":40},{"$f":"PERCENTILE(T$5:T$87,0.9)","v":78.804000000000002},{"$f":"PERCENTILE(U$5:U$87,0.9)","v":238.02600000000001}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$87,[1]TOT!$S$1)","v":41.604500000000023},{"$f":"PERCENTILE(T$5:T$87,[1]TOT!$S$1)","v":80},{"$f":"PERCENTILE(U$5:U$87,[1]TOT!$S$1)","v":238.26}]

{"sheet":"4,4-5 GHz","index":9,"n_rows":24,"n_cols":25,"rows_kept":24,"cut":false,"hidden":false,"merged":[[5,11,5,12],[2,0,4,0],[2,1,4,1],[2,2,2,4],[2,5,2,10],[2,11,2,12],[2,15,2,20],[2,21,2,24],[3,5,3,6],[3,15,3,17],[3,18,3,20],[2,14,4,14],[20,1,21,1],[6,1,7,1],[8,1,9,1],[10,1,11,1],[12,1,13,1],[15,1,16,1],[18,1,19,1]]}
["All empty but"]
[]
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L7:M103)","v":968},null,{"$f":"SUBTOTAL(9,N7:N103)","v":0}]
["AUT","4400-5000","X",null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["AUT"]
["CZE","4400-5000",null,null,null,null,null,null,null,null,"MD",null,null,null,null,null,null,null,null,null,null,null,null,null,"civil/MD sharing"]
["CZE"]
["CYP","4400-5000",null,null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X"]
["CYP"]
["HUN","4400-5000","X",null,null,"X","X",null,null,null,"Harmonized NATO band type 1. Land military systems, Tactical Radio Relay",null,140,null,null,"X","X","X",null,null,null,null,null,null,"non-civil usage"]
["HUN"]
["LVA","4400-5000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band"]
["PRT","4400-5000",null,null,null,null,null,null,null,"X","Military"]
["PRT"]
["RUS","4400-5000","X","X",null,null,null,"X","X",null,null,null,344,null,"F.382 ITU-R","X","X","X",40,80,90]
["SRB","4400-5000",null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["SRB"]
["CHE","4400-5000",null,null,null,null,null,null,null,null,"No civil FS use"]
["CHE"]
[]
[null,null,{"$f":"COUNTA(C7:C22)","v":3},{"$f":"COUNTA(D7:D22)","v":1},1,1,1,1,2,2,5,{"$f":"SUM(L7:L22)","v":0},{"$f":"SUM(M7:M22)","v":484},{"$f":"SUM(N7:N22)","v":0},null,{"$f":"COUNTA(P7:P22)","v":2},{"$f":"COUNTA(Q7:Q22)","v":2},{"$f":"COUNTA(R7:R22)","v":2},{"$f":"PERCENTILE(S$5:S$22,[1]TOT!$S$1)","v":40},{"$f":"PERCENTILE(T$5:T$22,[1]TOT!$S$1)","v":80},{"$f":"PERCENTILE(U$5:U$22,[1]TOT!$S$1)","v":90}]

{"sheet":"5,7-5,95 GHz","index":10,"n_rows":41,"n_cols":25,"rows_kept":41,"cut":false,"hidden":false,"merged":[[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[3,11,3,12],[0,14,2,14],[15,1,16,1],[19,1,20,1],[22,1,23,1],[25,1,26,1],[0,15,0,20]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M101)","v":3136},null,{"$f":"SUBTOTAL(9,N5:N101)","v":1246}]
["TELIASON","5850-5925"]
["AUT","5850-5925","X",null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["BIH","5850-5925"]
["HRV","5850-5925"]
["CZE","5850-5925",null,null,null,null,null,null,null,null,"MD",null,null,null,null,null,null,null,null,null,null,null,null,null,"civil/MD sharing"]
["CYP","5850-5925","X",null,null,null,null,null,"X",null,null,2,null,null,null,null,"X"," ","PORTABLE"]
["DNK","5850-5925"]
["EST","5850-5925"]
["FIN","5850-5925"]
["FRA","5850-5925"]
["GRC","5850-5925"]
["HUN","5850-5925","X",null,null,"X","X","X",null,null,"Non-Civil BFWA systems",null,null,null,"ECC/DEC/(06)04"]
["HUN",null,"X",null,null,"X"]
["ICE","5850-5925"]
["IRL","5850-5925"]
["ITA","5850-5925","X",null,null,"X",null,null,"X",null,null,71,null,null,"national",null,null,"x",20,50,238,1,"yes"]
["ITA",null,null,"X",null,null,null,"X","X",null,null,116,null,null,"national",null,"x",null,9.4700000000000006,61.58,121.23,1,"yes"]
["LVA","5850-5925",null,"X",null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Planning BFWA  within 5725-5875 MHz band. BFWA  5905-5925 MHz"]
["LTU","5850-5925","X",null,null,"X",null,"X",null,null,null,null,29,null,null,29]
["LTU",null,null,null,null,null,"X",null,null,"X",null,null,null,null,"5/10/20MHz",null,null,null,null,null,null,null,null,null,"5850-5875, 5905-5925 future P-MP"]
["LUX","5850-5925",null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["NLD","5850-5925"]
["NLD"]
["NOR","5725-5795 and 5815-5850",null,null,"X",null,null,null,null,"X",null,null,null,null,"National plan"]
["PRT","5850-5925",null,null,"X",null,null,null,null,null,"ISM, SRD"]
["RUS","5850-5925","X","X",null,null,"X","X","X",null,null,null,1350,623,null,"X","X","X",30,70,90]
["SRB","5850-5925",null,null,"X",null,null,null,null,null,"X",null,null,null,"ERC/REC 70-03",null,null,null,null,null,null,null,null,null,"SRD"]
["SVK","5850-5925",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["SVN","5850-5925"]
["SWE","5850-5925"]
["CHE","5850-5925",null,null,null,null,null,null,null,null,"ENG-Outside Broadcast"]
["GBR","5725-5850",null,"X",null,null,null,null,null,"X",null,null,null,null,"no channel plan"]
[]
[null,null,{"$f":"COUNTA(C5:C36)","v":7},4,3,4,4,4,5,3,{"$f":"COUNTA(K5:K36)","v":6},{"$f":"SUM(L5:L36)","v":189},{"$f":"SUM(M5:M36)","v":1379},{"$f":"SUM(N5:N36)","v":623},null,{"$f":"COUNTA(P5:P36)","v":2},{"$f":"COUNTA(Q5:Q36)","v":3},{"$f":"COUNTA(R5:R36)","v":3},{"$f":"MIN(S$5:S$36)","v":9.4700000000000006},{"$f":"MIN(T$5:T$36)","v":50},{"$f":"MIN(U$5:U$36)","v":90}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$36)","v":20},{"$f":"MEDIAN(T$5:T$36)","v":61.58},{"$f":"MEDIAN(U$5:U$36)","v":121.23}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$36)","v":30},{"$f":"MAX(T$5:T$36)","v":70},{"$f":"MAX(U$5:U$36)","v":238}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$36,[1]TOT!$S$1)","v":29},{"$f":"PERCENTILE(T$5:T$36,[1]TOT!$S$1)","v":69.158000000000001},{"$f":"PERCENTILE(U$5:U$36,[1]TOT!$S$1)","v":226.32299999999998}]

{"sheet":"5,9-7,1 GHz","index":11,"n_rows":48,"n_cols":26,"rows_kept":48,"cut":false,"hidden":false,"merged":[[3,11,3,12],[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[0,14,2,14],[42,11,42,12],[21,1,22,1],[23,1,24,1],[28,1,29,1],[30,1,31,1],[35,1,37,1],[41,11,41,12]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M102)","v":35326},null,{"$f":"SUBTOTAL(9,N5:N102)","v":3884}]
["TELIASON","5925-7125","X",null,null,null,null,"X",null,null,null,null,19,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,19,6,null,40,null,"X",null,null,"NL 290"]
["AUT","5925-7125","X",null,null,"X",null,"X",null,null,null,null,336,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",5,45,70]
["BIH","5925-7125","X",null,null,null,null,"X",null,null,null,5,302,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",8,60,134,null,"X"]
["HRV","5925-7125","X",null,null,null,null,"X",null,null,null,null,98,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",10.7,34.1,70.8,20,"x"]
["CZE","5925-7125","X",null,null,"X",null,null,null,null,null,null,1642,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["CYP","5925-7125","X",null,null,null,null,"X","X",null,null,17,27,null,"ERC/REC 14-01 and ERC/REC 14-02","X","X"," ",7.19,null,53]
["DNK","5925-7125","X",null,null,null,null,null,null,null,null,null,22,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["EST","5925-7125",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["FIN","5925-7125","X",null,null,null,null,"X","X",null,null,null,160,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",10,30,63,0.8]
["FRA","5925-7125","X",null,null,"X",null,"X",null,null,null,null,3491,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,3491,0.5,"20-80",105,"+ 5 % ","X"]
["GER","5925-6425","x",null,null,"x",null,null,null,null,null,994,null,null,"ERC/REC 14-01",null,null,"x",11.1,40,67.3]
["GER","6425-7125","x",null,null,"x",null,null,null,null,null,2565,null,null,"ERC/REC 14-02",null,null,"x",4.3,30,103.9]
["GRC","5925-7125","X",null,null,null,null,"X",null,null,null,null,638,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",8,45,102,"stable"]
["HUN","5925-7125","X",null,null,"X",null,null,null,null,null,null,299,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,null,null,null,null,0.1]
["ICE","5925-7125","X",null,null,"X",null,null,"X",null,null,6,16,null,"ERC/REC 14-01 and ERC/REC 14-02",3,null,15,10,30,50,0]
["IRL","5925-7125"," X",null,null,null,null," X",null,null,null,2,356,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null," X",8,40,90," 28"]
["ITA","5925-7125","X",null,null,"X",null,"X","X",null,null,102,808,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",6.32,44,83,0.15,"almost"]
["LVA","5925-6245 and  6425-7125","X",null,null,"X",null,null,null,null,null,null,39,null,"ERC/REC 14-01 ",null,null,"X",22,30,36,100]
["LVA",null,"X",null,null,"X",null,null,null,null,null,null,17,null,"ERC/REC 14-02",null,null,"X",28,35,52,100]
["LTU","5925-7125","X",null,null,"X",null,"X",null,null,null,null,137,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["LTU",null,null,null,null,null,"X",null,null,"X",null,null,null,null,"5/10/20MHz",null,null,null,null,null,null,null,null,null,"5925-6425 future for P-MP"]
["LUX","5925-7125","X",null,null,"X",null,"X","X",null,null,10,2,null,"ERC/REC 14-01 and ERC/REC 14-02 and national plan",null,"X","X",3.4,"20-80",63,"N/A","NO","NO"]
["NLD","5925-7125","X",null,null,null,null,null,null,"X",null,null,51,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",21.41,31.11,49.3,20]
["NOR","5925-7125","X","X",null,null,null,null,null,"X",null,null,146,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",2.8,37.5,123]
["PRT","5925-7125","X",null,null,"X",null,"X",null,null,"VSAT, SRD",2,8,null,"ERC/REC 14-01 ",null,"X","X",40,40,88,50]
["PRT",null,"X",null,null,"X",null,"X",null,null,"VSAT, SRD",null,59,null,"ERC/REC 14-02",null,"X","X",15,40,84,10]
["RUS","5925-7125","X","X",null,"X","X","X","X",null,null,null,3411,1942,"ERC/REC 14-01 and ERC/REC 14-02","X","X","X",30,55,65]
["RUS",null,null,null,null,null,null,null,null,null,null,null,null,null,"F.383 ITU-R"]
["SRB","5925-7125","X",null,null,null,null,"X",null,null,null,null,205,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",17,45,79,30]
["SVK","5925-6425","X",null,null,"X",null,"X",null,null,null,null,81,null,"ERC/REC 14-01 ",null,null,"X",8.5,20,54,25]
["SVK","6430-7110","X",null,null,"X",null,"X",null,null,null,null,2,null,"ERC/REC 14-02",null,null,"X",44,49,54,"0-100 ",null,null,"expected growth"]
["SVN","5925 – 6425 ","X",null,null,"X",null,"X",null,null,null,null,6,null,"ERC/REC 14-01 ",null,null,"X",12,50,75,30]
["SVN",null,"X",null,null,"X",null,null,"X",null,null,null,2,null,"ERC/REC 14-01 ",null,null,null,20,55,65,50]
["SVN",null,null,"X",null,"X",null,null,"X",null,null,null,4,null,"ERC/REC 14-01 ",null,null,null,5,25,65,0,"x",null,null,"assigned all SVN (28MHz Ch.7 and 8)"]
["SVN","6425 – 7125","X",null,null,"X",null,"X",null,null,null,null,14,null,"ERC/REC 14-02",null,null,"X",20,40,50,50]
["SWE","5925-7125","X",null,null,"X",null,null,null,null,null,null,952,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,null,null,null,null,null,"Y"]
["CHE","5925-7125","X",null,null,"X",null,"X",null,null,null,null,60,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,60,30,39.700000000000003,81.7,"growth"]
["GBR","5925-6425","X",null,null,null,null,null,null,"X",null,220,null,null,"ERC/REC 14-01 ",null,null,"X"]
["GBR","6425-7125","X",null,null,null,null,null,null,"X",null,330,null,null,"ERC/REC 14-02",null,"X","X"]
[]
[null,null,{"$f":"COUNTA(C5:C43)","v":35},3,0,23,2,21,8,5,{"$f":"COUNTA(K5:K43)","v":2},{"$f":"SUM(L5:L43)","v":4253},{"$f":"SUM(M5:M43)","v":13410},{"$f":"SUM(N5:N43)","v":1942},null,{"$f":"COUNTA(P5:P43)","v":3},{"$f":"COUNTA(Q5:Q43)","v":9},{"$f":"COUNTA(R5:R43)","v":29},{"$f":"MIN(S$5:S$43)","v":0.5},{"$f":"MIN(T$5:T$43)","v":20},{"$f":"MIN(U$5:U$43)","v":36}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$43)","v":10},{"$f":"MEDIAN(T$5:T$43)","v":40},{"$f":"MEDIAN(U$5:U$43)","v":67.3}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$43)","v":44},{"$f":"MAX(T$5:T$43)","v":60},{"$f":"MAX(U$5:U$43)","v":134}]
[null,"Allocation: all link by link. Only block allocation in NOR and SVN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$43,[1]TOT!$S$1)","v":35.999999999999979},{"$f":"PERCENTILE(T$5:T$43,[1]TOT!$S$1)","v":55},{"$f":"PERCENTILE(U$5:U$43,[1]TOT!$S$1)","v":115.79999999999995}]

{"sheet":"7,1-8,5 GHz","index":12,"n_rows":107,"n_cols":26,"rows_kept":107,"cut":false,"hidden":false,"merged":[[3,11,3,12],[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[0,14,2,14],[101,11,101,12],[4,1,5,1],[7,1,9,1],[13,1,14,1],[32,1,33,1],[38,1,39,1],[45,1,46,1],[48,1,49,1],[74,1,77,1],[86,1,87,1],[90,1,91,1],[92,1,93,1]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M103)","v":36036},null,{"$f":"SUBTOTAL(9,N5:N103)","v":0}]
["TELIASON","7125-7750","X",null,null,null,null,"X",null,null,null,null,22,null,"ECC REC (02)06",null,22,null,15,null,42,null,"X",null,null,"NEC 770"]
["TELIASON",null,"X",null,null,null,null,"X",null,null,null,null,128,null,null,74,54,null,7,null,80,null,"X",null,null,"Eric sson ML"]
["TELIASON","7750-7900"]
["TELIASON","7900-8500","X",null,null,null,null,"X",null,null,null,null,8,null,"ECC REC (02)06",null,8,null,16,null,68,null,"X",null,null,"NEC 770"]
["TELIASON",null,"X",null,null,null,null,"X",null,null,null,null,37,null,null,null,11,26,13,null,68,"+",null,null,null,"NEC NEO"]
["TELIASON",null,"X",null,null,null,null,"X",null,null,null,null,1,null,null,null,null,1,null,34,null,"++",null,null,null,"Ericsson TN"]
["AUT","7125-7750","X",null,null,"X",null,null,null,null,null,null,570,null,"ECC REC (02)06",null,"X","X",1,40,78]
["AUT","7750-7900",null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["AUT","7900-8500","X",null,null,"X",null,"X","X",null,null,null,73,null,"ECC REC (02)06",null,"X","X",1,35,60]
["BIH","7125-7750 (7725)","X",null,null,null,null,"X",null,null,null,null,113,null,"ECC REC (02)06",null,"X","X",4,40,90,null,"X"]
["BIH",null,"X",null,null,null,null,"X",null,null,null,10,62,null,"ITU-R F.385",null,"X","X"]
["BIH","7725-8275","X",null,null,null,null,"X","X",null,null,34,143,null,"ITU-R F.386, Annex 6",null,"X","X",4,38,83,null,"X",null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["BIH","8275-8500","X",null,null,null,null,"X",null,null,null,null,17,null,"ITU-R F.386, Annex 2",null,"X",null,7,25,65,null,"X"]
["HRV","7125-7750","X",null,null,null,null,"X",null,null,null,null,171,null,"Bands 7125 - 7425 and 7425 - 7725 with diff. ch. arrangements",null,"X","X",3.8,37.700000000000003,91.4,30,"x"]
["HRV","7750-7900","X",null,null,null,null,"X","X",null,null,null,146,null,"Band 7725 - 8275",null,null,"X",21.1,50.3,91.4,null,"x"]
["HRV","7900-8500","X",null,null,null,null,"X",null,null,null,null,14,null,"Band 8275 - 8500",null,"X",null,7.5,20.100000000000001,31.4]
["CZE","7125-7750","X",null,null,"X",null,null,null,null,null,null,1050,null,"ECC REC (02)06",null,null,null,null,null,null,null,null,"x","civil/MD sharing"]
["CZE","7750-7900",null,null,null,null,null,null,null,null,"MD"]
["CZE","7900-8500",null,null,null,null,null,null,null,null,"MD",null,null,null,"ECC REC (02)06"]
["CYP","7125-7750","X",null,null,null,null,"X","x",null,null,8,48,null,"ECC REC (02)06","X","X"," ",0.49,null,63.77]
["CYP","7750-7900",null,null," "]
["CYP","7900-8500","X",null,null,null,null,null,"X",null,null,14,null,null,"ECC REC (02)06","X","X"," ",8.2899999999999991,null,40.020000000000003]
["DNK","7125-7750","X",null,null,null,null,null,null,null,null,null,225,null,"ECC REC (02)06",null,null,null,20]
["DNK","7750-7900"]
["DNK","7900-8500","X",null,null,null,null,null,null,null,null,null,4," ","ECC REC (02)06",null,null,null,20]
["EST","7125-7750",null,null,null,null,null,null,null,null,null,null,62,null,"ECC REC (02)06",null,62,null,17,35,81]
["EST","7750-7900"]
["EST","7900-8500",null,null,null,null,null,null,null,null,null,null,45,null,"ECC REC (02)06",null,45,null,15,35,40,"+20"]
["FIN","7125-7750","X",null,null,null,null,"X",null,null,null,null,130,null,"ITU-R F.385",null,"X","X",13,36,65,0.05]
["FIN",null,"X",null,null,null,null,"X",null,null,null,null,330,null,"National (ITU-R F.385 mod.)",null,"X","X",2,27,70,0.1]
["FIN","7750-7900","X",null,null,null,null,null,"X",null,null,45,7,null,"National  ",null,"X"]
["FIN","7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["FRA","7125-7750",null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["FRA","7750-7900"]
["FRA","7900-8500","X",null,null,"X",null,"X",null,null,null,null,2529,null,"ECC REC (02)06",1322,947,260,0.04,"15<x>60",105,"- 10 %"]
["FRA",null,null,null,null,null,null,null,null,null,null,null,null,null,"UIT-RF-386-4"]
["GER","7125-7425","x",null,null,"x",null,null,null,null,null,917,null,null,"ECC REC (02)06",null,"x",null,4.2,28,89.9]
["GER","7425-7725","x",null,null,"x",null,null,null,null,null,3157,null,null,"ECC REC (02)06",null,null,"x",5.5,26,71.099999999999994,null,"x"]
["GRC","7425-7725 (upper 7 GHz) new row by EETT","X",null,null,null,null,"X",null,null,null,null,1222,null,"ECC REC (02)06 Annex1","X","X","X",1,31,98,0.1]
["GRC","7725-8275 (lower 8 GHz) new row by EETT","X",null,null,null,null,"X",null,null,null,null,1157,null,"ITU-R F. 386-6 Annex 1",null,"X","X",2,40,150,0.1]
["GRC","8275-8500 (upper 8 GHz) new row by EETT","X",null,null,null,null,"X",null,null,null,null,170,null,"ITU-R F. 386-6 Annex 3","X","X",null,1.8,47,120,"stable"]
["HUN","7125-7750","X",null,null,"X",null,null,"X",null,"7125-7250 MHz Non-Civil P-P links;  7125-7425 MHz Emergency Services\n7425-7725 MHz Civil P-P links 7725-7750 MHz Civil broadcasting infrastructure",null,171,null,"ECC REC (02)06","X","X","X",null,20]
["HUN",null,null,null,null,null,null,null,null,null,"7250-7750 MHz Satellite Systems downlink (military); Harmonized NATO band type 1."]
["HUN","7750-7900","X",null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,40,null,0.15]
["HUN","7900-8500","X",null,null,null,null,null,null,null,"7900-8400 MHz Satellite Systems uplink (military); Harmonized NATO band type 1.",null,null,null,"ECC REC (02)06"]
["HUN",null,"X",null,null,"X",null,null,null,null,null,null,3,null,null,"X","X",null,null,20]
["ICE","7125-7750","X",null,null,"X",null,null,"X",null,null,23,65,null,"ECC REC (02)06",32,28,28,10,30,60,0]
["ICE","7750-7900"]
["ICE","7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["IRL","7125-7750"," X",null,null,null,null," X",null,null,null,1,279,null,"ECC REC (02)06"," X","X","X",7,36,76," 57"]
["IRL","7750-7900"]
["IRL","7900-8500"," X",null,null,null,null," X",null,null,null,null,315,null,"ECC REC (02)06"," X","X","X",5,36,81," 48"]
["ITA",null,"X",null,null,"X",null,"X",null,null,null,null,2231,null,"national",null,"X","X",null,30,null,0.1,"almost"]
["ITA","7750-7900"]
["ITA","7900-8500","X",null,null,null,null,"X",null,null,null,null,5,null,"national",null,null,"X"]
["LVA","7125-7800","X",null,null,"X",null,null,null,null,null,null,104,null,"ITU-R F.385",null,null,"X",14,35,54,50,null,null,"Military band 7250-7331 MHz"]
["LVA","7800-7900",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band 7850-7900 MHz"]
["LVA","7900-8500","X",null,null,"X",null,null,null,null,null,null,152,null,"ECC REC (02)06",null,null,"X",12,35,50,50,null,null,"Military band 7975-8024 MHz"]
["LTU","7125-7750","X",null,null,"X",null,null,null,null,null,null,197,null,"ECC REC (02)06"]
["LTU","7750-7900","X",null,null,"X",null,null,null,null,null,null,0,null,"local"]
["LTU","7900-8500","X",null,null,"X",null,null,null,null,null,null,116,null,"ECC REC (02)06"]
["LUX","7125-7750","X",null,null,"X",null,"X","X",null,null,0,26,null,"ECC REC (02)06",null,"X","X",7.9,"20-80",55.9,"N/A","NO","NO"]
["LUX","7750-7900","X",null,null,"X",null,"X","X",null,null,0,0,null,"Nat. freq. plan",null,"X","X",null,null,null,"N/A","NO","NO"]
["LUX","7900-8500","X",null,null,"X",null,"X","X",null,null,4,6,null,"ECC REC (02)06",null,"X","X",5.0999999999999996,"20-80",62,"N/A","NO","NO"]
["NLD","7125-7750","X",null,null,null,null,null,null,"X",null,null,113,null,"ECC REC (02)06","X","X","X",10.4,27.7,55.6,20]
["NLD","7750-7900"]
["NLD","7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["NOR","7125-7425","X",null,null,null,null,null,null,"X",null,null,135,null,null,null,null,"X",4.2,35.5,96]
["NOR","7425-7725","X",null,null,null,null,null,null,"X",null,null,446,null,null,null,null,"X",1.2,32.299999999999997,113]
["NOR","7900-8200",null,"X",null,null,null,null,null,"X",null,null,null,null,"ECC REC (02)06"]
["PRT","7125-7750","X",null,null,"X",null,"X",null,null,"FSS, Military (7.25-7.3 GHz)",null,7,null,"7 LOW: ITU-R F.385","X",null,null,15,"30",53,0]
["PRT",null,"X",null,null,"X",null,"X",null,null,"FSS, Military (7.25-7.3 GHz)",null,287,null,"7 LOW: ECC REC (02)06","X","X","X",6,"30",63,10]
["PRT",null,"X",null,null,"X",null,"X",null,null,"FSS",null,40,null,"7 HIGH: ITU-R F.385","X","X",null,3,"22",71,-50]
["PRT",null,"X",null,null,"X",null,"X",null,null,"FSS",null,30,null,"7 HIGH: ECC REC (02)06","X","X","X",15,"30",78,50]
["PRT","7750-7900","X",null,null,"X",null,"X",null,null,null,null,26,null,"8 LOW: ITU-R F.386",null,"X","X",2,"30",75,50]
["PRT","7900-8500","X",null,null,"X",null,null,"X",null,"FSS, EESS, Military (7.975-8.025 GHz)",7,9,null,"8 HIGH: ITU-R F.386","X",null,null,6,"40",88,-100]
["RUS","7125-7750","X","X",null,null,null,"X","X",null,null,"less than 1%",10495,null,"F.385 ITU-R","X","X","X",30,55,65]
["RUS","7750-7900","No","No"]
["RUS","7900-8500","X","X",null,null,null,"X","X",null,null,"less than 1%",4584,null,"F.386 ITU-R","X","X","X",30,55,65]
["SRB","7125-7725","X",null,null,null,null,"X",null,null,null,null,138,null,"ITU-R F.385-9 base","X","X","X",11.67,37.979999999999997,104.2,150]
["SRB","7725-8275","X",null,null,null,null,"X",null,null,null,null,8,null,"ITU-R F.386-8 annex 6",null,"X","X",9.44,35.68,70.27,300]
["SRB","8275-8500","X",null,null,null,null,"X",null,null,null,null,10,null,"ITU-R F.386-8 annex 2",null,"X","X",21,53.77,98.71,300]
["SVK","7125-7425","X",null,null,"X",null,"X",null,null,null,null,30,null,"ECC REC (02)06",null,null,"X",17,25,44.5,50]
["SVK",null,"X",null,null,"X",null,"X",null,null,null,null,14,null,"ITU-R F.385, DS 161MHz","X","X",null,7,25,58,-100,null,"x","no new links"]
["SVK","7425-7725","X",null,null,"X",null,"X",null,null,null,null,70,null,"ITU-R F.385-9, DS 161MHz","X","X",null,5,25,55,10]
["SVK","7700-8300","X",null,null,"X",null,"X",null,null,null,null,35,null,"ITU-R F.386-4, Annex 1",null,null,"X",8,30,58,-100,null,"x","no new links"]
["SVN","7125-7425","X",null,null,"X",null,"X",null,null,null,null,23,null,"ECC REC (02)06",null,null,"X",10,25,45,10,"x"]
["SVN",null,"X",null,null,"X",null,null,"X",null,null,null,43,null,"ECC REC (02)06",null,null,"X",5,25,65,5,"x"]
["SVN","7425 – 7725","X",null,null,"X",null,"X",null,null,null,null,26,null,"ECC REC (02)06",null,null,"X",10,25,45,20]
["SVN",null,"X",null,null,"X",null,null,"X",null,null,null,5,null,"ECC REC (02)06",null,null,"X",3,25,60,30]
["SVN","7725 – 8275","X",null,null,"X",null,null,"X",null,null,6,42,null,"ITU-R F 386-8 An6  (29.65 MHz, DS 311.32 MHz)",null,null,"X",15,35,60,5,"x*",null,"congested in backbone directions"]
["SVN","8275-8500","X",null,null,"X",null,"X",null,null,null,null,14,null,"ITU-R F.386-8 An2 (28 MHz , DS 119 MHz, 14 MHz, DS 126 MHz)",null,"X",null,20,35,70,30,"x*",null,"congested in backbone directions"]
["SWE","7425-7725","X",null,null,"X",null,null,null,null,null,null,1421,null,null,null,"X",null,null,null,null,null,"Y"]
["SWE","7900-8500","X",null,null,"X",null,null,null,null,null,null,494,null,"ECC REC (02)06",null,"X",null,null,null,null,"Y","N"]
["CHE","7125-7750","X",null,null,"X",null,"X",null,null,null,null,171,null,"ECC REC (02)06",70,81,20,20,30.2,99.5,"growth"]
["CHE","7750-7900",null,null,null,null,null,null,null,null,"ENG-Outside Broadcast"]
["CHE","7900-8500",null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ECC REC (02)06"]
["GBR","7425-7900","X",null,null,null,null,null,null,"X",null,940,null,null,"ITU-R F.385-9","X","X","X"]
[]
[null,null,{"$f":"COUNTA(C5:C102)","v":74},4,1,37,0,45,19,5,{"$f":"COUNTA(K5:K102)","v":13},{"$f":"SUM(L5:L102)","v":5166},{"$f":"SUM(M5:M102)","v":30870},{"$f":"SUM(N5:N102)","v":0},null,{"$f":"COUNTA(P5:P102)","v":24},{"$f":"COUNTA(Q5:Q102)","v":50},{"$f":"COUNTA(R5:R102)","v":48},{"$f":"MIN(S$5:S$102)","v":0.04},{"$f":"MIN(T5:T102)","v":20},{"$f":"MIN(U5:U102)","v":31.4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$102)","v":7.7},{"$f":"MEDIAN(T$5:T$102)","v":35},{"$f":"MEDIAN(U$5:U$102)","v":68}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$102)","v":30},{"$f":"MAX(T$5:T$102)","v":55},{"$f":"MAX(U$5:U$102)","v":150}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$102,[1]TOT!$S$1)","v":21.015000000000001},{"$f":"PERCENTILE(T$5:T$102,[1]TOT!$S$1)","v":52.902500000000003},{"$f":"PERCENTILE(U$5:U$102,[1]TOT!$S$1)","v":107}]

{"sheet":"10-10,68 GHz","index":13,"n_rows":49,"n_cols":25,"rows_kept":49,"cut":false,"hidden":false,"merged":[[3,11,3,12],[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[0,14,2,14],[28,1,29,1],[31,1,32,1],[39,1,40,1],[6,1,7,1],[8,1,9,1],[13,1,15,1],[22,1,23,1],[24,1,25,1],[26,1,27,1]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M101)","v":7606},null,{"$f":"SUBTOTAL(9,N5:N101)","v":3520}]
["TELIASON","10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["AUT","10000-10680","X",null,null,"X",null,"X",null,null,null,null,158,null,"ERC/REC 12-05",null,"x",null,1,30,80]
["BIH","10000-10680","X",null,null,null,null,null,"X",null,null,103,null,null,"ERC/REC 12-05","X","X",null,1,27,80,"+15",null,null,"10000-10680 MHz: Shared band between P-P links and FWA. We still do not have active implemented FWA systems."]
["BIH",null,null,"X",null,"X","X",null,null,null,null,null,null,null,"ERC/REC 12-05 Annex A"]
["HRV","10000-10680","X",null,null,null,null,null,"X",null,null,2,null,null,"ERC/REC 12-05",null,"x"]
["HRV",null,null,"X",null,null,"X"]
["CZE","10000-10300",null,null,null,null,null,null,null,null,"MD",null,null,null,"ERC/REC 12-05"]
["CZE","10300-10680","X",null,"X","X",null,null,null,null,null,null,21]
["CYP","10000-10680","X",null,null,null,null,null,"X",null,null,56,null,null,"ERC/REC 12-05","X","X"," ",0.53,null,70]
["DNK","10000-10680","X",null,null,null,null,null,null,null,null,null,null,47,"ERC/REC 12-05"]
["DNK",null,null,"X",null,null,null,null,null,null,null,null,"No info"]
["DNK",null,"X",null,null,null,null,null,null,null,null,null,1]
["EST","10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["FIN","10000-10680","X",null,null,null,"X",null,null,null,null,null,null,11,"ERC/REC 12-05",null,"X"]
["FRA","10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["GRC","10000-10680","X",null,null,null,null,null,"X",null,null,107,null,null,"national plan",null,null,null,1.2,19,75]
["HUN","10000-10680","X",null,null,null,null,null,"X",null,null,93,null,null,"ERC/REC 12-05",null,null,null,null,40]
["ICE","10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["IRL","10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["IRL",null," X",null,null," X",null,null,null,null,null,null,null,30,"National Legislation: S.I. 79 of 2003\nNational Legislation: S.I. 530 of 2003 European Legislation: Decision 2008/411/EC ",null,null,null,null,null,null," 75"]
["ITA","10000-10680","X",null,null,null,null,"X","X",null,null,{"$f":"935+529+446","v":1910},34,null,"ERC/REC 12-05",null,"X",null,3,25,84,1,"yes"]
["ITA",null,"X",null,null,null,null,"X","X",null,null,{"$f":"236+24","v":260},80,null,"ERC/REC 12-05",null,null,"x",5.5,35,50,1,"yes"]
["LVA","10000-10680","X",null,null,"X",null,null,null,null,null,null,105,null,"ERC/REC 12-05","X",null,null,null,null,null,-80,null,null,"10300-10500 MHz"]
["LVA",null,null,"X",null,null,"X",null,null,null,null,null,null,66,"ERC/REC 12-05 and ERC/REC 13-04",null,"X",null,null,10,null,50]
["LTU","10150-10300 and 10500-10650","X",null,null,"X",null,"X",null,null,null,0,0,null,"ERC/REC 12-05"]
["LTU",null,null,"X",null,null,"X",null,null,null,null,null,null,6,"ERC/REC 12-05",null,null,null,null,null,null,100]
["LTU","10300-10500","X",null,null,"X",null,"X",null,null,null,null,420,null,"ERC/REC 12-05",420]
["LUX","10000-10680","X",null,null,"X",null,"X","X",null,null,2,0,null,"ERC/REC 12-05",null,"X","X",32,"10-50",62,"N/A","NO","NO"]
["LUX",null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["NLD","10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["NOR","10200-10700",null,"X",null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-05"]
["PRT","10000-10680",null,null,null,null,null,null,null,null,"AM, SAP/SAB, SRD",null,null,null,"ERC/REC 12-05"]
["RUS","10000-10680","X","X",null,null,"X","X","X",null,null,"less than 1%",247,1490,"ERC/REC 12-05","X","X","X",15,30,40]
["SRB","10000-10680","X",null,null,null,null,null,"X",null,null,76,3,null,"national plan","X",null,null,0.7,24.72,114.99,20]
["SVK","10000-10680",null,"X",null,null,"X",null,null,null,null,null,null,110,"ERC/REC 12-05","x","x",null,null,null,null,10]
["SVN","10000-10680","X",null,null,"X",null,null,"X",null,null,53,null,null,"ERC/REC 12-05",null,"x","x",2,25,65,-100,null,"x","BWA when SAP/SAB P to P video links analogue cease operation"]
["SVN",null,"X",null,null,"X",null,null,"X",null,null,null,8,null,"ERC/REC 12-05",null,"x","x",2,25,62,-100,null,"x","BWA when SAP/SAB P to P video links analogue cease operation"]
["SWE","10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05\nNew ITU-R Rec under dev.",null,null,null,null,null,null,"Y","N",null,"Blockassignment?"]
["CHE","10000-10680","X",null,null,"X",null,"X",null,null,null,null,64,null,"ERC/REC 12-05",18,46,null,15,18.3,48.5,"growth"]
["GBR","10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
[]
[null,null,{"$f":"COUNTA(C5:C44)","v":22},8,1,11,7,8,12,1,{"$f":"COUNTA(K5:K44)","v":2},{"$f":"SUM(L5:L44)","v":2662},{"$f":"SUM(M5:M44)","v":1141},{"$f":"SUM(N5:N44)","v":1760},null,{"$f":"COUNTA(P5:P44)","v":8},{"$f":"COUNTA(Q5:Q44)","v":13},{"$f":"COUNTA(R5:R44)","v":6},{"$f":"MIN(S$5:S$44)","v":0.53},{"$f":"MIN(T$5:T$44)","v":10},{"$f":"MIN(U$5:U$44)","v":40}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$44)","v":2},{"$f":"MEDIAN(T$5:T$44)","v":25},{"$f":"MEDIAN(U$5:U$44)","v":67.5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$44)","v":32},{"$f":"MAX(T$5:T$44)","v":40},{"$f":"MAX(U$5:U$44)","v":114.99}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$44,[1]TOT!$S$1)","v":22.649999999999988},{"$f":"PERCENTILE(T$5:T$44,[1]TOT!$S$1)","v":37.25},{"$f":"PERCENTILE(U$5:U$44,[1]TOT!$S$1)","v":97.945499999999981}]

{"sheet":"10,7-12,5 GHz","index":14,"n_rows":71,"n_cols":26,"rows_kept":71,"cut":false,"hidden":false,"merged":[[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[32,15,33,15],[32,16,33,16],[32,24,33,24],[32,18,33,18],[32,19,33,19],[32,20,33,20],[32,21,33,21],[32,22,33,22],[32,23,33,23],[32,17,33,17],[3,11,3,12],[0,14,2,14],[32,11,33,11],[32,12,33,12],[32,13,33,13],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M69)","v":14724},null,{"$f":"SUBTOTAL(9,N5:N103)","v":4082}]
["TELIASON","10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["TELIASON","11700-12500"]
["AUT","10700-11700","X",null,null,"X",null,"X",null,null,null,null,21,null,"ERC/REC 12-06"]
["AUT","11700-12500"]
["BIH","10700-11700","X",null,null,null,null,"X","X",null,null,37,38,null,"ERC/REC 12-06","X","X",null,1,25,64,"+15",null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["BIH","11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/DEC(00)08"]
["BIH","11700-12500",null,"X",null,null,null,null,"X",null,null,null,null,16,null,null,null,null,null,null,null,"+10"]
["HRV","10700-11700","X",null,null,null,null,"X",null,null,null,null,8,null,"ERC/REC 12-06",null,null,"x",7.5,20.2,29.8]
["HRV","11700-12500"]
["CZE","10700-11700","X",null,null,null,"X",null,null,null,null,null,null,1845,"ERC/REC 12-06",null,null,null,null,null,null,20]
["CZE","11700-12500","X",null,null,"X",null,null,null,null,null,31,null,null,null,null,null,null,null,null,null,10]
["CYP","10700-11700","X",null,null,null,null,"X","X",null,null,3,30,null,"ERC/REC 12-06",null,"X"," ",2.0099999999999998,null,34.130000000000003]
["CYP","11700-12500","X",null,null,null,null,null,"X",null,null,10,null,null,null,null,"X"," ",2.75,null,30.18]
["DNK","10700-11700","X",null,null,null,null,null,null,null,null,null,null,1,"ERC/REC 12-06"]
["DNK","11700-12500"]
["EST","10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["EST","11700-12500"]
["FIN","10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["FIN","11700-12500"]
["FRA","10700-11700","X",null,null,"X",null,"X",null,null,null,null,524,null,"ERC/REC 12-06",null,null,524,1.5,"15<x>50",46,"+ 26 %"]
["FRA","11700-12500"]
["GRC","10700-11700","X",null,null,null,null,"X",null,null,null,null,785,null,"ERC/REC 12-06",null,null,"X",1.7,19,63,0.3]
["GRC","11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["HUN","10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["HUN","10700-11700","X",null,null,"X",null,null,null,null,null,null,186,null,"ERC/DEC/(00)08",null,null,"X",null,14]
["HUN","11700-12500",null,null,"X",null,null,null,"X",null,null,null,null,144,null,null,null,null,null,null,null,null,"x"]
["ICE","10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["ICE","11700-12500"]
["IRL","10700-11700"," X",null,null,null,null,"X",null,null,null,null,648,null,"ERC/REC 12-06",null,"X","X",1.5,24,56," 39"]
["IRL","10700-11700",null,null,null,null,null,null,null,null,null,null,null,null," National Legislation: S.I. 370 of 2009"]
["IRL","11700-12500"]
["ITA","10700-11700","X",null,null,"X",null,"X",null,null,null,null,3110,null,"ERC/REC 12-06",null,"X","X",null,18,null,0.15,"yes"]
["ITA","10700-11700","X",null,null,null,null,"X","X",null,null,58,99,null,"ERC/REC 12-06",null,"X","X",3,22,60,0.15,"yes"]
["ITA","11700-12500","X",null,null,null,null,"X",null,null,null,22,1,null,null,null,"x",null,1.97,27.6,62.94]
["LVA","10700-11700","X",null,null,null,null,null,"X",null,null,38,null,null,"ITU-R F.387",null,null,null,0.3,10,32,-50,null,null,"Analog fixed links"]
["LVA","11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BROADCASTING-SATELLITE"]
["LTU","10700-11700","X",null,null,"X",null,null,null,null,null,0,0,null,"ERC/REC 12-06"]
["LTU","11700-12500"]
["LUX","10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["LUX","11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["NLD","10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["NLD","11700-12500"]
["NOR","10700-11700",null,"X",null,null,null,null,null,"X",null,null,null,null,"ITU rec F.387-10"]
["NOR","10700-11700","X",null,null,null,null,null,null,"X",null,null,234,null,null,null,null,"x",0.5,23,66.5]
["PRT","10700-11700","X",null,null,"X",null,"X","X",null,"FSS, VSAT, SNG, SIT, AES, Euteltracs",null,117,null,"ERC/REC 12-06",null,"X","X",2,"20",41,5]
["PRT","11700-12500",null,null,null,null,null,null,null,null,"RAD-S, SIT"]
["RUS","10700-11700","X","X",null,null,null,"X","X",null,null,"less than 1%",1207,null,"ERC/REC 12-06","X","X","X",15,30,40]
["RUS","10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,"F.387 ITU-R"]
["RUS","11700-12500","No","No"]
["SRB","10700-11700","X",null,null,null,null,"X",null,null,null,null,48,null,"ERC/REC 12-06",null,null,"X",7.13,15.72,37.700000000000003,300]
["SRB","11700-12500",null,"X",null,null,null,null,"X",null,null,null,null,15,null,null,null,"X"]
["SVK","10700-11700","X",null,null,"X",null,"X",null,null,null,null,0,null,"ERC/REC 12-06",null,null,"x",null,null,null,100,null,null,"operation expected"]
["SVK","11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["SVN","10700-11700","X",null,null,"X",null,"X",null,null,null,null,13,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",7,40,46,50,null,null,null,"In accordance with CEPT and ITU limitations"]
["SVN","10700-11700","X",null,null,"X",null,null,"X",null,null,3,null,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",35,40,46,5,null,null,null,"In accordance with CEPT and ITU limitations"]
["SVN","10700-11700","X",null,null,"X",null,null,"X",null,null,null,3,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",33,40,47,5,null,null,null,"In accordance with CEPT and ITU limitations"]
["SVN","11700-12500",null,"X",null,null,"X",null,null,null,"MMDS",null,null,20,"National (200/400 MHz)",null,null,"x",5,30,40,10,null,null,null,"assigned for local/regional coverage"]
["SWE","10700-11700",null,null,null,null,null,null,null,null,null,7,1,null,"ERC/REC 12-06"]
["SWE","11700-12500"]
["CHE","10700-11700","X",null,null,"X",null,"X",null,null,null,null,80,null,"ERC/REC 12-06",null,null,80,10,14.9,34.9,"growth",null,null,"heavily used by FSS"]
["CHE","11700-12500"]
["GBR","11700-12500"]
[]
[null,null,{"$f":"COUNTA(C5:C66)","v":27},6,1,12,2,16,12,2,{"$f":"COUNTA(K5:K66)","v":3},{"$f":"SUM(L5:L66)","v":209},{"$f":"SUM(M5:M66)","v":7153},{"$f":"SUM(N5:N66)","v":2041},null,{"$f":"COUNTA(P5:P66)","v":2},{"$f":"COUNTA(Q5:Q66)","v":9},{"$f":"COUNTA(R5:R66)","v":20},{"$f":"MIN(S$5:S$66)","v":0.3},{"$f":"MIN(T$5:T$66)","v":10},{"$f":"MIN(U$5:U$66)","v":29.8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$66)","v":2.75},{"$f":"MEDIAN(T$5:T$66)","v":23},{"$f":"MEDIAN(U$5:U$66)","v":46}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$66)","v":35},{"$f":"MAX(T$5:T$66)","v":40},{"$f":"MAX(U$5:U$66)","v":66.5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$66,[1]TOT!$S$1)","v":33.199999999999996},{"$f":"PERCENTILE(T$5:T$66,[1]TOT!$S$1)","v":40},{"$f":"PERCENTILE(U$5:U$66,[1]TOT!$S$1)","v":64.25}]

{"sheet":"12,75-13,25 GHz","index":15,"n_rows":47,"n_cols":26,"rows_kept":47,"cut":false,"hidden":false,"merged":[[3,11,3,12],[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[0,14,2,14],[4,1,6,1],[9,1,10,1],[21,1,22,1],[21,2,22,2],[21,3,22,3],[21,23,22,23],[21,24,22,24],[24,1,25,1],[27,1,28,1],[21,15,22,15],[21,16,22,16],[21,17,22,17],[21,18,22,18],[21,19,22,19],[21,20,22,20],[21,5,22,5],[21,6,22,6],[21,7,22,7],[21,8,22,8],[21,9,22,9],[21,10,22,10],[30,1,31,1],[32,1,33,1],[37,1,38,1],[21,21,22,21],[21,22,22,22],[21,4,22,4]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTALE",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M101)","v":102626},null,{"$f":"SUBTOTAL(9,N5:N101)","v":14}]
["TELIASON","12750-13250","X",null,null,null,null,"X",null,null,null,null,302,null,"ERC/REC 12-02",210,null,92,3,null,50,"+",null,null,null,"NEC NEO"]
["TELIASON",null,"X",null,null,null,null,"X",null,null,null,null,22,null,null,null,null,22,9,null,42,"-",null,null,null,"NERA Citylink"]
["TELIASON",null,"X",null,null,null,null,"X",null,null,null,null,80,null,null,32,48,null,5,null,29,0,null,null,null,"Eric sson ML"]
["AUT","12750-13250","X",null,null,"X",null,"X",null,null,null,null,137,null,"ERC/REC 12-02",null,null,"x",3,25,52]
["BIH","12750-13250","X",null,null,null,null,"X",null,null,null,null,31,null,"ERC/REC 12-02","X","X","X",2,20,34,"+15"]
["HRV","12750-13250","X",null,null,null,null,"X",null,null,null,null,244,null,"ERC/REC 12-02",null,"x",null,1.5,19.2,49.2,20,"x"]
["HRV",null,"X",null,null,null,null,null,"X",null,null,1]
["CZE","12750-13250","X",null,null,"X",null,null,null,null,null,null,1288,null,"ERC/REC 12-02",null,null,null,null,null,null,10]
["CYP","12750-13250","X",null,null,null,null,"X",null,null,null,null,278,null,"ERC/REC 12-02","X","X"," ",0.28999999999999998,null,40.94,null,"X"]
["DNK","12750-13250","X",null,null,null,null,null,null,null,null,null,4,null,"ERC/REC 12-02",null,null,null,12]
["EST","12750-13250",null,null,null,null,null,null,null,null,null,null,80,null,"ERC/REC 12-02",null,80,null,11,22,34]
["FIN","12750-13250","X",null,null,null,null,"X",null,null,null,null,2120,null,"ERC/REC 12-02",null,"X","X",0.4,14,49,0.2,"x",null,"Local congestion"]
["FRA","12750-13250","X",null,null,"X",null,"X",null,null,null,null,6613,null,"ERC/REC 12-02",2401,3711,501,0.1,"5<x>35",103,"+ 2 %","X"]
["GER","12750-13250","x",null,null,"x",null,null,null,null,null,4100,null,null,"ERC/REC 12-02",null,null,"x",0.99,12,48.5]
["GRC","12750-13250","X",null,null,null,null,"X",null,null,null,null,1004,null,"ERC/REC 12-02","X","X","X",1.5,16,55,0.5]
["HUN","12750-13250","X",null,null,"X",null,null,null,null,null,null,1710,null,"ERC/REC 12-02",null,"X",null,null,12,null,null,"x"]
["ICE","12750-13250","X",null,null,"X",null,null,null,null,null,null,12,null,"ERC/REC 12-02",null,6,6,10,20,30,0]
["IRL","12750-13250"," X",null,null,null,null,"X",null,null,null,2,1078,null,"ERC/REC 12-02","X","X","X",1.5,19,53," 27"," X"]
["IRL",null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["ITA","12750-13250","X",null,null,"X",null,"X",null,null,null,null,6106,null,"ERC/REC 12-02",null,"X","X",7,16,30,0.15,"yes"]
["LVA","12750-13250","X",null,null,"X",null,null,null,null,null,null,630,null,"ERC/REC 12-02",null,"X",null,2,35,47,20]
["LVA",null,null,"X",null,null,null,null,"X",null,null,null,null,7,"national plan","X",null,null,null,5,null,null,null,null,"MMDS"]
["LTU","12750-13250","X",null,null,"X",null,null,null,null,null,null,222,null,"ERC/REC 12-02"]
["LUX","12750-13250","X",null,null,"X",null,"X","X",null,null,8,22,null,"ERC/REC 12-02",null,"X","X",5.6,"5-35",32,"N/A","NO","NO"]
["LUX",null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["NLD","12750-13250","X",null,null,null,null,null,null,"X",null,null,201,null,"ERC/REC 12-02",null,"X","X",8.35,18.2,31.5]
["NOR","12750-13250",null,"X",null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-02"]
["NOR",null,"X",null,null,null,null,null,null,"X",null,null,1240,null,null,null,"X","X",0.1,14.7,90]
["PRT","12750-13250","X",null,null,"X",null,"X",null,null,"FSS",null,49,null,"ITU-R F.497","X",null,null,2,"25",46,-50]
["PRT",null,"X",null,null,"X",null,"X",null,null,"FSS",null,368,null,"ERC/REC 12-02","X","X","X",1,"15",57,10]
["RUS","12750-13250","X","X",null,null,null,"X","X",null,null,"less than 1%",16553,null,"ERC/REC 12-02 e ITU-R F.497","X","X","X",10,25,35]
["SRB","12750-13250","X",null,null,null,null,"X",null,null,null,null,564,null,"ERC/REC 12-02","X","X","X",2.15,19.579999999999998,58.65,50]
["SVK","12750-13250","X",null,null,"X",null,"X",null,null,null,null,620,null,"ERC/REC 12-02","X","X","X",4,15,48,20]
["SVN","12750-13250","X",null,null,"X",null,"X",null,null,null,null,178,null,"ERC/REC 12-02",null,"X","X",2,25,54,5,"x"]
["SVN",null,"X",null,null,"X",null,null,"X",null,null,null,21,null,"ERC/REC 12-02",null,null,"X",5,20,40,5,"x"]
["SWE","12750-13250","X",null,null,"X",null,null,null,null,null,null,775,null,"ERC/REC 12-02",null,null,null,null,null,null,null,"Y"]
["CHE","12750-13250","X",null,null,"X",null,"X",null,null,null,null,470,null,"ERC/REC 12-02",174,290,6,10,14.2,46.4,"unchanged",null,null,"heavily used by FSS"]
["GBR","12750-13250","X",null,null,null,null,null,null,"X",null,3840,340,null,"ERC/REC 12-02","X","X","X"]
[]
[null,null,{"$f":"COUNTA(C5:C42)","v":33},3,0,17,0,20,5,4,{"$f":"COUNTA(K5:K42)","v":2},{"$f":"SUM(L5:L42)","v":7951},{"$f":"SUM(M5:M42)","v":43362},{"$f":"SUM(N5:N42)","v":7},null,{"$f":"COUNTA(P5:P42)","v":15},{"$f":"COUNTA(Q5:Q42)","v":23},{"$f":"COUNTA(R5:R42)","v":23},{"$f":"MIN(S$5:S$42)","v":0.1},{"$f":"MIN(T$5:T$42)","v":5},{"$f":"MIN(U$5:U$42)","v":29},{"$f":"COUNTA(V5:V42)","v":21},{"$f":"COUNTA(W5:W42)","v":11}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$42)","v":2.5750000000000002},{"$f":"MEDIAN(T$5:T$42)","v":19},{"$f":"MEDIAN(U$5:U$42)","v":47}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$42)","v":12},{"$f":"MAX(T$5:T$42)","v":35},{"$f":"MAX(U$5:U$42)","v":103}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$42,[1]TOT!$S$1)","v":10.649999999999999},{"$f":"PERCENTILE(T$5:T$42,[1]TOT!$S$1)","v":25},{"$f":"PERCENTILE(U$5:U$42,[1]TOT!$S$1)","v":80.59499999999997}]

{"sheet":"14-16 GHz","index":16,"n_rows":78,"n_cols":26,"rows_kept":78,"cut":false,"hidden":false,"merged":[[3,11,3,12],[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[0,14,2,14]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M110)","v":97292},null,{"$f":"SUBTOTAL(9,N5:N110)","v":0}]
["TELIASON","14250-14500"]
["AUT","14250-14500"]
["BIH","14250-14500"]
["HRV","14250-14500"]
["CZE","14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"sat. services planned"]
["CYP","14250-14500","X",null,null,null,null,null,"X",null,null,14,null,null,"ERC/REC 13-03",null,"X"," ",8.2899999999999991,null,36.46]
["DNK","14250-14500"]
["EST","14250-14500"]
["FIN","14250-14500"]
["FRA","14250-14500","X",null,null,"X",null,"X",null,null,null,null,374,null,null,374,null,null,10,"5<x>35",100,"-5%"]
["GRC","14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["HUN","14250-14500"]
["ICE","14250-14500"]
["IRL","14250-14500"]
["ITA","14250-14500","X",null,null,null,null,null,"X",null,null,1030,null,null,"national",null,null,"X",3,11,27,0.05,"yes"]
["LVA","14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIXED-SATELLITE"]
["LTU","14250-14500"]
["LUX","14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["NLD","14250-14500"]
["NOR","14250-14500"]
["PRT","14250-14500",null,null,null,null,null,null,null,null,"FSS, VSAT, SNG, AES"]
["RUS","14250-14500","X","X",null,null,null,null,null,null,null,null,150,null,null,"X","X","X",8,20,30]
["SRB","14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it have not been used yet"]
["SVK","14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["SVN","14250-14500"]
["SWE","14250-14500"]
["CHE","14250-14500"]
["GBR","14250-14500"]
["BIH","14400-15350","X",null,null,null,null,"X",null,null,null,null,162,null,"ITU-R F.636","X","X",null,1,15,45,null,null,null,"14400-15350 MHz: Planned leaving of ITU rec. and fully harmonization according to ERC/REC 12-07"]
[null,null,{"$f":"COUNTA(C5:C33)","v":5},{"$f":"COUNTA(D5:D33)","v":1},0,1,0,2,2,0,null,{"$f":"SUM(L5:L33)","v":1044},{"$f":"SUM(M5:M33)","v":686},{"$f":"SUM(N5:N33)","v":0},null,{"$f":"COUNTA(P5:P33)","v":3},{"$f":"COUNTA(Q5:Q33)","v":3},{"$f":"COUNTA(R5:R33)","v":3},{"$f":"MIN(S$5:S$33)","v":1},{"$f":"MIN(T$5:T$33)","v":11},{"$f":"MIN(U$5:U$33)","v":27}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$33)","v":8},{"$f":"MEDIAN(T$5:T$33)","v":15},{"$f":"MEDIAN(U$5:U$33)","v":36.46}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$33)","v":10},{"$f":"MAX(T$5:T$33)","v":20},{"$f":"MAX(U$5:U$33)","v":100}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$33,[1]TOT!$S$1)","v":9.6579999999999995},{"$f":"PERCENTILE(T$5:T$33,[1]TOT!$S$1)","v":19.5},{"$f":"PERCENTILE(U$5:U$33,[1]TOT!$S$1)","v":89}]
["TELIASON","14500-14620 and 15230-15350","X",null,null,null,null,"X",null,null,null,null,944,null,"ERC/REC 12-07",620,324,null,1,null,39,"-",null,null,null,"Eric sson ML"]
["TELIASON","14500-14620 and 15230-15350","X",null,null,null,null,"X",null,null,null,null,93,null,null,93,null,null,3,null,30,null,"X",null,null,"NEC Pasolink"]
["AUT","14500-14620 and 15230-15350","X",null,null,"X",null,"X",null,null,null,null,631,null,"ERC/REC 12-07","x","x","x",1,15,44]
["BIH","14500-14620 and 15230-15350","X",null,null,null,null,"X",null,null,null,null,278,null,"ERC/REC 12-07","X","X",null,1,15,45]
["HRV","14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,20,null,null,"ERC/REC 12-07",null,null,null,0.6,9.9,22.7]
["CZE","14500-14620 and 15230-15350","X",null,null,"X",null,null,null,null,null,null,20,null,"ERC/REC 12-07"]
["CYP","14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,12,null,null,"ERC/REC 12-07",null,"X",null,0.45,null,38.17]
["DNK","14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,null,null,299,null,"ERC/REC 12-07",null,null,null,12]
["EST","14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,60,null,"ERC/REC 12-07",null,60,null,12,23,33,"- 5"]
["FIN","14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07"]
["FIN","14500-14620 and 15230-15350","X",null,null,null,null,"X",null,null,null,null,1950,null,"ITU-R F.636",null,"X",null,0.1,8.6999999999999993,10.9,-0.15]
["FRA","14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07"]
["GER","14500-14620 and 15230-15350","x",null,null,"x",null,null,null,null,null,10235,null,null,"ERC/REC 12-07",null,"x",null,2.25,14,54.5,null,"x"]
["GRC","14500-14620 and 15230-15350","X",null,null,null,null,"X",null,null,null,null,2863,null,"ERC/REC 12-07","X","X","X",0.5,15,75,0.5,"heavily used"]
["HUN","14500-14620 and 15230-15350"," ",null,null," ",null,null,null,null,null,null," ",null,"ERC/REC 12-07",null,null,null,null," "]
["HUN","14500-14620 and 15230-15350","X",null,null,"X",null,null,null,null,"15230-15350 MHz Non-Civil Digital P-P links",null,120,null,null,"X","X",null,null," ",null,null,"x",null,"non-civil usage"]
["ICE","14500-14620 and 15230-15350","X",null,null,"X",null,null,null,null,null,null,120,null,"ERC/REC 12-07",57,57,6,5,15,25,25]
["IRL","14500-14620 and 15230-15350"," X",null,null,null,null," X",null,null,null,null,1718,null,"ERC/REC 12-07\nNational Legislation: S.I. 370 of 2009"," X","X","X",1.7,17,53," 29"," X"]
["ITA","14500-14620 and 15230-15350","X",null,null,"X",null,"X",null,null,null,null,4070,null,"ERC/REC 12-07","X","X","X",7,16,33,0.15,"yes"]
["ITA","14500-14620 and 15230-15350","X",null,null,"X",null,"X",null,null,null,null,1562,null,"national",null,"X",null,null,null,null,null,"yes"]
["LVA","14500-14620 and 15230-15350","X",null,null,"X",null,null,null,null,null,null,48,null,"ERC/REC 12-07",null,"X",null,3,25,37,20]
["LTU","14500-14620 and 15230-15350","X",null,null,"X",null,null,null,null,null,null,262,null,"ERC/REC 12-07"]
["LUX","14500-14620 and 15230-15350","X",null,null,"X",null,"X","X",null,null,0,64,null,"ERC/REC 12-07",null,"X","X",1.4,"5-30",34.700000000000003,"N/A","NO","NO"]
["NLD","14500-14620 and 15230-15350","X",null,null,null,null,null,null,"X",null,null,116,null,"ERC/REC 12-07","x","x","x",7.71,14.7,34.9,20]
["NOR","14500-14620 and 15230-15350"]
["PRT","14500-14620 and 15230-15350","X",null,null,"X",null,"X",null,null,null,null,362,null,"ERC/REC 12-07","X","X",null,1,"15",37,5]
["SRB","14500-14620 and 15230-15350","X",null,null,null,null,"X",null,null,null,null,433,null,"ERC/REC 12-07","X","X","X",1.35,16.98,39.26,20]
["SVK","14500-14620 and 15230-15350","X",null,null,"X",null,"X",null,null,null,null,230,null,"ERC/REC 12-07","x","x",null,9.5,15,48,10]
["SVN","14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07",null,null,null,null,null,null,null,null,null,"Defence systems:","Land military systems (FS, MS)"]
["SWE","14500-14620 and 15230-15350","X",null,null,"X",null,null,null,null,null,null,2629,null,"Nat ch.plan(expdate 2016)",null,null,null,null,null,null,null,"Y"]
["CHE","14500-14620 and 15230-15350","X",null,null,"X",null,"X",null,null,null,null,263,null,"ERC/REC 12-07",110,153,null,10,14.6,37.1,"unchanged"]
["GBR","14500-14620 and 15230-15350","X",null,null,null,null,null,null,"X",null,2050,2050,null,"ERC/REC 12-07","X","X","X"]
["RUS","14500-14620 and 15230-15350\n(14500 - 15350)","X","X",null,null,null,"X","X",null,null,12,13320,null,"ERC/REC 12-07 e ITU-R F.636","X","X","X",8,20,30]
[null,null,{"$f":"COUNTA(C38:C70)","v":28},{"$f":"COUNTA(D38:D70)","v":1},0,15,0,15,4,2,null,{"$f":"SUM(L38:L70)","v":12329},{"$f":"SUM(M38:M70)","v":34505},{"$f":"SUM(N38:N70)","v":0},null,{"$f":"COUNTA(P38:P70)","v":16},{"$f":"COUNTA(Q38:Q70)","v":22},{"$f":"COUNTA(R38:R70)","v":10},{"$f":"MIN(S$38:S$70)","v":0.1},{"$f":"MIN(T$38:T$70)","v":8.6999999999999993},{"$f":"MIN(U$38:U$70)","v":10.9},{"$f":"COUNTA(V38:V70)","v":14},{"$f":"COUNTA(W38:W70)","v":9}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$38:S$70)","v":1.9750000000000001},{"$f":"MEDIAN(T$38:T$70)","v":15},{"$f":"MEDIAN(U$38:U$70)","v":37}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$38:S$70)","v":12},{"$f":"MAX(T$38:T$70)","v":25},{"$f":"MAX(U$38:U$70)","v":75}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$38:S$70,[1]TOT!$S$1)","v":11.899999999999999},{"$f":"PERCENTILE(T$38:T$70,[1]TOT!$S$1)","v":23.5},{"$f":"PERCENTILE(U$38:U$70,[1]TOT!$S$1)","v":54.5}]
["SVN","14613-14725 and 15033-15145","X",null,null,"X",null,"X",null,null,null,null,82,null,"ITU-R F.636-3 (Ch. 5,6,7,8)",null,"x",null,7,25,45,-10,null,"x"]
["SVN","14613-14725 and 15033-15145",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07",null,null,null,null,null,null,null,null,"x","Defence systems:","Land military systems (FS, MS)"]
[]
[null,null,{"$f":"COUNTA(C75:C76)","v":1},{"$f":"COUNTA(D75:D76)","v":0},0,1,0,1,0,0,null,{"$f":"SUM(L75:L76)","v":0},{"$f":"SUM(M75:M76)","v":82},{"$f":"SUM(N75:N76)","v":0},null,{"$f":"COUNTA(P75:P76)","v":0},{"$f":"COUNTA(Q75:Q76)","v":1},{"$f":"COUNTA(R75:R76)","v":0},{"$f":"PERCENTILE(S$75:S$76,[1]TOT!$S$1)","v":7},{"$f":"PERCENTILE(T$75:T$76,[1]TOT!$S$1)","v":25},{"$f":"PERCENTILE(U$75:U$76,[1]TOT!$S$1)","v":45}]

{"sheet":"17-17,7 GHz","index":17,"n_rows":15,"n_cols":25,"rows_kept":15,"cut":false,"hidden":false,"merged":[[4,11,4,12],[1,0,3,0],[1,1,3,1],[1,2,1,4],[1,5,1,10],[1,11,1,12],[1,15,1,20],[1,21,1,24],[2,5,2,6],[2,15,2,17],[2,18,2,20],[1,14,3,14]]}
["all empty but"]
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L6:M102)","v":66},null,{"$f":"SUBTOTAL(9,N6:N102)","v":0}]
["CZE","17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FS considered"]
["GRC","17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["ITA","17300-17700","X",null,null,"X",null,null,null,null,null,null,33,null,"national",null,"X"]
["LVA","17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HDFSS"]
["PRT","17300-17700",null,null,null,null,null,null,null,null,"FSS, HDFSS"]
["RUS","17300-17700","No","No"]
["SRB","17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["SVK","17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
[]
[null,null,{"$f":"COUNTA(C6:C13)","v":2},1,0,1,0,0,0,0,{"$f":"COUNTA(K6:K13)","v":1},{"$f":"SUM(L6:L13)","v":0},{"$f":"SUM(M6:M13)","v":33},{"$f":"SUM(N6:N13)","v":0},null,{"$f":"COUNTA(P6:P13)","v":0},{"$f":"COUNTA(Q6:Q13)","v":1},{"$f":"COUNTA(R6:R13)","v":0}]

{"sheet":"17-20,2 GHz","index":18,"n_rows":51,"n_cols":26,"rows_kept":51,"cut":false,"hidden":false,"merged":[[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[44,11,44,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[3,11,3,12],[0,14,2,14]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M101)","v":167500},null,{"$f":"SUBTOTAL(9,N5:N101)","v":0}]
["TELIASON","17700-19700","X",null,null,null,null,"X",null,null,null,null,3,null,"ERC/REC 12-03",null,null,3,9,null,11,null,"X",null,null,"NEC 900"]
["TELIASON","17700-19700","X",null,null,null,null,"X",null,null,null,null,23,null,null,null,null,23,3,null,14,0,null,null,null,"NERA Citylink"]
["TELIASON","17700-19700","X",null,null,null,null,"X",null,null,null,null,738,null,null,null,645,93,4,null,28,"+",null,null,null,"NEC NEO"]
["TELIASON","17700-19700","X",null,null,null,null,"X",null,null,null,null,1,null,null,null,null,1,null,9,null,"++",null,null,null,"Ericsson TN"]
["AUT","17700-19700","X",null,null,"X",null,"x",null,null,null,null,261,null,"ERC/REC 12-03",null,null,"x",1,10,19]
["BIH","17700-19700","X",null,null,null,null,"X",null,null,null,null,446,null,"ERC/REC 12-03","X","X","X",1,10,35,"+20"]
["HRV","17700-19700","X",null,null,null,null,"X",null,null,null,null,536,null,"ERC/REC 12-03",null,"x",null,0.4,10.199999999999999,24.6,10]
["CZE","17700-19700","X",null,null,"X",null,null,null,null,null,null,6883,null,"ERC/REC 12-03",null,null,null,null,null,null,null,"x"]
["CYP","17700-19700","X",null,null,null,null,"X","X",null,null,null,18,null,"ERC/REC 12-03","X","X"," ",1.62,null,9.99]
["DNK","17700-19700",null,"X",null,null,null,null,null,null,null,null,"No info",null,"ERC/REC 12-03"]
["DNK","17700-19700","X",null,null,null,null,null,null,null,null,null,759]
["EST","17700-19700",null,null,null,null,null,null,null,null,null,null,585,null,"ERC/REC 12-03",null,585,null,10,21,43,"+25"]
["FIN","17700-19700","X",null,null,null,null,"X",null,null,null,null,2650,null,"ERC/REC 12-03",null,"X","X",0.1,8.6999999999999993,32.5,0.3,"x",null,"Local congestion"]
["FRA","17700-19700","X",null,null,"X",null,"X",null,null,null,null,4399,null,"ERC/REC 12-03",237,2787,1375,0.16,"4<x>25",46,"+ 8 %","X"]
["FRA","17700-19700",null,null,null,null,null,null,null,null,null,null,null,null,"IUT-RF 595-8"]
["GER","17700-19700","x",null,null,"x",null,null,null,null,null,6162,null,null,"ERC/REC 12-03",null,"x",null,0.25,9,38.4,15]
["GRC","17700-19700","X",null,null,null,null,"X",null,null,null,null,2446,null,"ERC/REC 12-03","X","X","X","0.3",8,28,0.35,"heavily used"]
["HUN","17700-19700",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-03"]
["HUN","17700-19700","X",null,null,"X",null,null,null,null,"Non-Civil P-P links",null,null,null,"ERC/DEC/(00)07",null,null,null,null,null,null,null,"x",null,"Development of high capacity P-P Non-Civil system is foreseen."]
["ICE","17700-19700","X",null,null,"X",null,null,null,null,null,null,60,null,"ERC/REC 12-03",40,10,10,10,15,20,25]
["IRL","17700-19700"," X",null,null,null,null," X",null,null,null,null,686,null,"ERC/REC 12-03\nNational Legislation: S.I. 370 of 2009",null," X","X",0.3,9,45," 28"," X"]
["ITA","17700-19700","X","X",null,"X",null,"X",null,null,null,null,{"$f":"14300+1512","v":15812},null,"ERC/REC 12-03","X","X","X",0.3,6,12,0.25,"highly"]
["ITA","17700-19700","X",null,null,null,null,"X","X",null,null,71,35,null,null,null,"X","X",1.3,4,7.5,0.25]
["LVA","17700-19700","X",null,null,"x",null,null,null,null,null,null,390,null,"ERC/REC 12-03",null,null,"X",1,20,43,20]
["LTU","17700-19700","X",null,null,"X",null,null,null,null,null,null,490,null,"ERC/REC 12-03"]
["LUX","17700-19700","X",null,null,"X",null,"X",null,null,null,0,47,null,"ERC/REC 12-03",null,null,"X",4.8,"4-25",24.1,"N/A","NO","NO"]
["LUX","17700-19700",null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["NLD","17700-19700","X",null,null,null,null,null,null,"X",null,null,1020,null,"ERC/REC 12-03",null,"x","x",7.7,5.27,34.9,20]
["NLD","17700-19700","X",null,null,null,null,null,null,"X",null,null,43,null,"F-5958-8 Annex 8",null,"x","x",5.63,13.11,18.649999999999999,0]
["NOR","17700-19700",null,"X",null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-03"]
["NOR","17700-19700","X",null,null,null,null,null,null,"X",null,null,387,null,null,null,null,"x",0.5,10.199999999999999,44.8]
["PRT","17700-19700","X",null,null,"X",null,"X",null,null,"FSS",null,131,null,"ITU-R F.595","X",null,null,2,"10",29,10]
["PRT","17700-19700","X",null,null,"X",null,"X",null,null,"FSS",null,1087,null,"ERC/REC 12-03",null,"X","X",0,"7",35,20]
["RUS","17700-19700","X","X",null,null,null,null,null,null,null,null,24277,null,"ERC/REC 12-03 and ITU-R F.595-9 ","X","X","X",5,12,20]
["SRB","17700-19700","X",null,null,null,null,"X",null,null,null,null,459,null,"ERC/REC 12-03 and ITU-R F.595-9 ","X","X","X",0.91,10.029999999999999,35.159999999999997,100]
["SVK","17700-19700","X",null,null,"X",null,"X",null,null,null,null,2170,null,"ERC/REC 12-03","x","x","x",1,10,38,20]
["SVN","17700-19700","X",null,null,"X",null,"X",null,null,null,null,361,null,"ERC/REC 12-03",null,null,"x",5,15,35,20,"x**",null,"congested in urban/sub urban regions"]
["SVN","17700-19700",null,"X",null,"X",null,"X",null,null,null,null,300,null,"ERC/REC 12-03",null,"x","x",5,15,35,0,"x**",null,"congested in urban/sub urban regions"]
["SWE","17700-19700","X",null,null,"X",null,null,null,null,null,null,2242,null,"ERC/REC 12-03",null,null,null,null,null,null,"Y","N"]
["CHE","17700-19700","X",null,null,"X",null,"X",null,null,null,null,332,null,"ERC/REC 12-03",24,155,153,3,9.1999999999999993,26.1,"growth",null,null,"heavily used by FSS"]
["GBR","17700-19700","X",null,null,null,null,null,null,"X",null,7440,null,null,"ERC/REC 12-03","X","X","X"]
["GBR","17700-19700",null,null,null,null,null,null,null,null,null,null,null,null,"ITU-R F.595"]
[]
[null,null,{"$f":"COUNTA(C5:C46)","v":34},5,0,17,0,22,2,5,{"$f":"COUNTA(K5:K46)","v":3},{"$f":"SUM(L5:L46)","v":13673},{"$f":"SUM(M5:M46)","v":70077},{"$f":"SUM(N5:N46)","v":0},null,{"$f":"COUNTA(P5:P46)","v":12},{"$f":"COUNTA(Q5:Q46)","v":22},{"$f":"COUNTA(R5:R46)","v":27},{"$f":"MIN(S$5:S$46)","v":0},{"$f":"MIN(T$5:T$46)","v":4},{"$f":"MIN(U$5:U$46)","v":7.5},{"$f":"COUNTA(V5:V46)","v":26}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$46)","v":1.46},{"$f":"MEDIAN(T$5:T$46)","v":10},{"$f":"MEDIAN(U$5:U$46)","v":29}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$46)","v":10},{"$f":"MAX(T$5:T$46)","v":21},{"$f":"MAX(U$5:U$46)","v":46}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$46,[1]TOT!$S$1)","v":9.6499999999999986},{"$f":"PERCENTILE(T$5:T$46,[1]TOT!$S$1)","v":19.749999999999996},{"$f":"PERCENTILE(U$5:U$46,[1]TOT!$S$1)","v":44.92}]

{"sheet":"21,2-22 GHz","index":19,"n_rows":21,"n_cols":25,"rows_kept":21,"cut":false,"hidden":false,"merged":[[4,11,4,12],[1,0,3,0],[1,1,3,1],[1,2,1,4],[1,5,1,10],[1,11,1,12],[1,15,1,20],[1,21,1,24],[2,5,2,6],[2,15,2,17],[2,18,2,20],[1,14,3,14]]}
["all empty but"]
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L6:M101)","v":782},null,{"$f":"SUBTOTAL(9,N6:N101)","v":0}]
["AUT","21200-22000","X",null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["BIH","21200-22000","X",null,null,null,null,"X",null,null,null,null,256,null,null,"X","X","X","0.5",5,20,null,null,null,"21200-22000 MHz: Planned leaving of band and full harmonization according to T/R 13-02 Annexes A1, A2, A3"]
["CYP","21200-22000","X",null,null,null,null,"X",null,null,null,null,97,null,null,"X","X"," ",0.2,null,18.27,null,"X"]
["GRC","21200-22000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Use"]
["HUN","21200-22000","X",null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,40,null,null,"X"]
["ITA","21200-22000","X",null,null,null,null,"X",null,null,null,26,7,null,null,null,"X",null,0.19,2.44,7.25]
["LVA","21200-22000","X",null,null,"x",null,null,null,null,null,2,null,null,"national plan","X",null,null,3,5,8,100]
["LTU","21200-22000","X",null,null,"X",null,null,null,null,null,0,0,null,"local"]
["PRT","21200-22000",null,null,null,null,null,null,null,null,"SRR"]
["SRB","21200-22000","X",null,null,null,null,null,"X",null,null,3,null,null,"ITU-R F.637-3 annex 5 ","X",null,null,3.11,4.9800000000000004,7.15]
["SVK","21200-22000","X",null,null,"X",null,null,"X",null,null,0,null,null,"ITU-R F.637",null,null,null,null,null,null,null,null,null,"currently no links"]
[]
[null,null,{"$f":"COUNTA(C6:C16)","v":9},0,0,3,0,3,4,0,{"$f":"COUNTA(K6:K16)","v":2},{"$f":"SUM(L6:L16)","v":31},{"$f":"SUM(M6:M16)","v":360},{"$f":"SUM(N6:N16)","v":0},null,{"$f":"COUNTA(P6:P16)","v":4},{"$f":"COUNTA(Q6:Q16)","v":3},{"$f":"COUNTA(R6:R16)","v":2},{"$f":"MIN(S$5:S$16)","v":0.19},{"$f":"MIN(T$5:T$16)","v":2.44},{"$f":"MIN(U$5:U$16)","v":7.15}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$16)","v":1.5999999999999999},{"$f":"MEDIAN(T$5:T$16)","v":5},{"$f":"MEDIAN(U$5:U$16)","v":8}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$16)","v":3.11},{"$f":"MAX(T$5:T$16)","v":40},{"$f":"MAX(U$5:U$16)","v":20}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$16,[1]TOT!$S$1)","v":3.0934999999999997},{"$f":"PERCENTILE(T$5:T$16,[1]TOT!$S$1)","v":32.999999999999993},{"$f":"PERCENTILE(U$5:U$16,[1]TOT!$S$1)","v":19.654}]

{"sheet":"22-23,6 GHz","index":20,"n_rows":47,"n_cols":26,"rows_kept":47,"cut":false,"hidden":false,"merged":[[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[1,11,2,11],[1,12,2,12],[0,15,0,20],[0,21,0,24],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,1,6],[1,7,2,7],[1,8,2,8],[1,9,2,9],[1,10,2,10],[0,14,2,14],[1,13,2,13],[1,18,1,20],[1,21,2,21],[1,22,2,22],[1,23,2,23],[1,24,2,24],[22,7,23,7],[22,8,23,8],[22,9,23,9],[22,10,23,10],[1,15,1,17],[22,11,23,11],[22,12,23,12],[22,13,23,13],[41,11,41,12],[3,11,3,12],[22,2,23,2],[22,3,23,3],[22,4,23,4],[22,5,23,5],[22,6,23,6]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,"Link by link","Block","Unlicensed","FWA",null,"Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"Capacity",null,null,"Hop lenght (km)",null,null,"Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
[null,null,null,null,null,"P-P","P-MP",null,null,null,null,null,null,null,null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX"]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M101)","v":196462},null,{"$f":"SUBTOTAL(9,N5:N101)","v":0}]
["TELIASON","22000-22600 and 23000-23600","X",null,null,null,null,"X",null,null,null,null,506,null,"T/R 13-02 Annexes A1, A2, A3",303,203,null,1,null,18,"-",null,null,null,"Eric sson ML"]
["TELIASON","22000-22600 and 23000-23600","X",null,null,null,null,"X",null,null,null,null,338,null,null,null,316,22,3,null,17,"+",null,null,null,"NEC NEO"]
["AUT","22000-22600 and 23000-23600","X",null,null,"X",null,"X",null,null,null,null,2885,null,"T/R 13-02 Annexes A1, A2, A3","x","x","x",1,10,20]
["BIH","22000-22600 and 23000-23600","X",null,null,null,null,"X",null,null,null,null,421,null,"T/R 13-02 Annexes A1, A2, A3","X","X","X","0.5",5,20,"+20"]
["HRV","22000-22600 and 23000-23600","X",null,null,null,null,"X",null,null,null,null,1220,null,"T/R 13-02 Annexes A1, A2, A3",null,"x",null,0.18,5.5,21.1,10]
["CZE","22000-22600 and 23000-23600","X",null,null,"X",null,null,null,null,null,null,3707,null,"T/R 13-02 Annexes A1, A2, A3",null,null,null,null,null,null,5]
["CYP","22000-22600 and 23000-23600","X",null,null,null,null,"X",null,null,null,null,738,null,"T/R 13-02 Annexes A1, A2, A3","X","X"," ",0.25,null,15.16,null,"X"]
["DNK","22000-22600 and 23000-23600",null,"X",null,null,null,null,null,null,null,null,"No info",null,"T/R 13-02 Annexes A1, A2, A3"]
["DNK","22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,null,650]
["EST","22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,788,null,"T/R 13-02 Annexes A1, A2, A3",null,788,null,3,14,24,"+25"]
["FIN","22000-22600 and 23000-23600","X",null,null,null,null,"X",null,null,null,null,2770,null,"T/R 13-02 Annexes A1, A2, A3",null,"X","X",0.1,4.5999999999999996,19,0.15,"x",null,"Local congestion"]
["FRA","22000-22600 and 23000-23600","X","X",null,"X",null,"X",null,null,null,null,12195,null,"T/R 13-02 Annexes A1, A2, A3",4614,7498,83,0.1,"3<x>20",32,"+ 9 %"]
["FRA","22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,"IUT-RF 637-3"]
["GER","22000-22600 and 23000-23600","x",null,null,"x",null,null,null,null,null,19401,null,null,"ERC/REC 13-02 ",null,"x",null,0.13,8,51.1]
["GRC","22000-23600","X",null,null,null,null,"X",null,null,null,null,1724,null,"T/R 13-02 Annex A","X","X","X","0.04",4,16,0.4]
["HUN","22000-22600 and 23000-23600","X",null,null,"X",null,null,null,null,"22442-22600 MHz Emergency Services Digital P-P links",null,40,null,"T/R 13-02 Annexes A1, A2, A3","X","X",null,null,null,null,null,"x"]
["HUN","22000-22600 and 23000-23600","X",null,null,"X",null,null,null,null,"23450-23600 MHz Emergency services Digital P-P links",null,3512,null,"T/R 13-02 Annexes A1, A2, A3","X","X",null,null,null,null,null,"x"]
["ICE","22000-22600 and 23000-23600","X",null,null,"x",null,null,null,null,null,null,18,null,"T/R 13-02 Annexes A1, A2, A3",5,11,2,1,6,25,25]
["IRL","22000-22600 and 23000-23600"," X",null,null,null,null," X",null,null,null,null,2178,null,"T/R 13-02 Annexes A1, A2, A3"," X","X","X",0.2,6.7,24," 36"," X"]
["IRL","22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["ITA","22000-22600 and 23000-23600","X","X",null,"X",null,"X",null,null,null,2,{"$f":"10970+1101","v":12071},null,"T/R 13-02 Annexes A1, A2, A3","X","X","X",2.1800000000000002,2.95,3.17,0.25,"yes"]
["LVA","22000-22600 and 23000-23600","X",null,null,"X",null,null,null,null,null,null,592,null,"T/R 13-02 Annexes A1, A2, A3",null,null,"X",0.15,15,25,30]
["LTU","22000-22600 and 23000-23600","X",null,null,"X",null,null,null,null,null,null,1362,null,"T/R 13-02 Annexes A1, A2, A3"]
["LUX","22000-22600 and 23000-23600","X",null,null,"X",null,"X","X",null,null,1,243,null,"T/R 13-02 Annexes A1, A2, A3",null,"X",null,0.3,"3-20",15,"N/A","NO","NO"]
["LUX","22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["NLD","22000-22600 and 23000-23600","X",null,null,null,null,null,null,"X",null,null,1450,null,"T/R 13-02 Annexes A1, A2, A3","x","x","x",3,7.65,14.78,30]
["NOR","22000-22600 and 23000-23600",null,"X",null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annexes A1, A2, A3"]
["NOR","22000-22600 and 23000-23600","X",null,null,null,null,null,null,"X",null,2,64,null,null,null,null,"x",0.3,5.7,25.4]
["PRT","22000-22600 and 23000-23600","X",null,null,"X",null,"X",null,null,"SRR",null,10,null,"Report 936-2 Annex 6","X",null,null,1,"5",12,-100]
["PRT","22000-22600 and 23000-23600","X",null,null,"X",null,"X",null,null,"SRR",null,908,null,"T/R 13-02 Annexes A1","X","X","X",null,"5",12,10]
["RUS","21200-23600","X","X",null,null,null,null,null,null,null,null,16816,null,"F.637 ITU-R","X","X","X",2,4,8]
["SRB","22000-22600 and 23000-23600","X",null,null,null,null,"X",null,null,null,null,1288,null,"T/R 13-02 Annexes A1","X","X","X",0.14000000000000001,4.74,24.41,100]
["SVK","22000-22600 and 23000-23600","X",null,null,"X",null,"X",null,null,null,null,1582,null,"T/R 13-02 Annex A1","x","x","x",0.5,5,13,10]
["SVN","22000-22600 and 23000-23600","X",null,null,"X",null,"X",null,null,null,null,767,null,"T/R 13-02 Annex A1",null,"x",null,3,7,10,5,"x**",null,"congested in urban/sub urban regions"]
["SVN","22000-22600 and 23000-23600","X",null,null,"X",null,"X",null,null,null,null,10,null,"T/R 13-02 Annex A1",null,null,"x",2,4,5,20,"x**",null,"congested in urban/sub urban regions"]
["SWE","22000-22600 and 23000-23600","X",null,null,"X",null,null,null,null,null,null,1322,null,"T/R 13-02 Annexes A1, A2, A3",null,null,null,null,null,null,null,"Y"]
["CHE","22000-22600 and 23000-23600","X",null,null,"X",null,"X",null,null,null,null,1900,null,"T/R 13-02 Annexes A1, A2, A3",787,1113,null,5,7.4,29.9,"unchanged","city areas congested, HIGH/LOW situation",null,"problem: SRR"]
["GBR","22000-22600 and 23000-23600","X",null,null,null,null,null,null,"X",null,4750,null,null,"T/R 13-02 ","X","X","X"]
[]
[null,null,{"$f":"COUNTA(C5:C42)","v":32},5,0,18,0,19,1,4,{"$f":"COUNTA(K5:K42)","v":4},{"$f":"SUM(L5:L42)","v":24156},{"$f":"SUM(M5:M42)","v":74075},{"$f":"SUM(N5:N42)","v":0},null,{"$f":"COUNTA(P5:P42)","v":19},{"$f":"COUNTA(Q5:Q42)","v":25},{"$f":"COUNTA(R5:R42)","v":19},{"$f":"MIN(S$5:S$42)","v":0.1},{"$f":"MIN(T$5:T$42)","v":2.95},{"$f":"MIN(U$5:U$42)","v":3.17},{"$f":"COUNTA(V5:V42)","v":22},{"$f":"COUNTA(W5:W42)","v":11}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$42)","v":1},{"$f":"MEDIAN(T$5:T$42)","v":5.7},{"$f":"MEDIAN(U$5:U$42)","v":18.5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$42)","v":5},{"$f":"MAX(T$5:T$42)","v":15},{"$f":"MAX(U$5:U$42)","v":51.1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$42,[1]TOT!$S$1)","v":3},{"$f":"PERCENTILE(T$5:T$42,[1]TOT!$S$1)","v":14.099999999999998},{"$f":"PERCENTILE(U$5:U$42,[1]TOT!$S$1)","v":31.475000000000001}]

{"sheet":"22,6-23 GHz","index":21,"n_rows":28,"n_cols":25,"rows_kept":28,"cut":false,"hidden":false,"merged":[[4,11,4,12],[1,0,3,0],[1,1,3,1],[1,2,1,4],[1,5,1,10],[1,11,1,12],[1,15,1,20],[1,21,1,24],[2,5,2,6],[2,15,2,17],[2,18,2,20],[1,14,3,14]]}
["all empty but"]
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L6:M101)","v":518},null,{"$f":"SUBTOTAL(9,N6:N101)","v":0}]
["CZE","22600-22700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENG/OB"]
["CZE","22700-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no utilisation"]
["CYP","22600-23000","X",null,null,null,null,"X",null,null,null,37,null,null,"National","X","X"," ",0.2,null,18.14,null,null,"X"]
["DNK","22600-23000","X",null,null,null,null,null,null,null,null,null,1]
["FRA","22600-23000","X",null,null,"X",null,"X",null,null,null,null,124,null,null,124,null,null,0.1,10,32,"+ 1%"]
["GRC","22600-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,"No current FS use.\nAllocation for analogue links. SAP/SAB, ENG/OB"]
["HUN","22600-23000","X",null,null,null,null,null,"X",null,null,1,null,null,null,null,null,null,null,40,null,null,"x"]
["ITA","22600-23000","x",null,null,null,null,"X",null,null,null,1,null,null,null,null,"x",null,null,0.19]
["LVA","22600-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAP/SAB "]
["LTU","22600-23000","X",null,null,"X",null,null,"X",null,null,1,null,null,"local"]
["PRT","22600-23000","X",null,null,"X",null,"?",null,null,"SRR",null,null,null,"T/R 13-02 Annexes A2, A3",null,null,null,null,null,null,"no use at the moment"]
["SRB","22600-23000","X",null,null,null,null,null,"X",null,null,94,null,null,"ITU-R F.637-3 annex 5 ","X",null,null,0.21,2.5,11.87]
["SVK","22600-23000","x",null,null,"X",null,null,"X",null,null,0,null,null,"ITU-R F.637",null,null,null,null,null,null,null,null,null,"currently no links"]
["SVN","22600-23000","x",null,null,"X",null,"X",null,null,null,null,"planned",null,"T/R 13-02 Annex A2","x","x"]
["SVN","22600-23000",null,null,null,"X",null,null,"X","X",null,"planned",null,null,"T/R 13-02 Annex A3","x","x"]
[]
[null,null,{"$f":"COUNTA(C6:C20)","v":10},0,0,6,0,5,5,1,{"$f":"COUNTA(K6:K20)","v":1},{"$f":"SUM(L6:L20)","v":134},{"$f":"SUM(M6:M20)","v":125},{"$f":"SUM(N6:N20)","v":0},null,{"$f":"COUNTA(P6:P20)","v":5},{"$f":"COUNTA(Q6:Q20)","v":4},{"$f":"COUNTA(R6:R20)","v":1},{"$f":"PERCENTILE(S$6:S$20,[1]TOT!$S$1)","v":0.20899999999999999},{"$f":"PERCENTILE(T$6:T$20,[1]TOT!$S$1)","v":35.499999999999986},{"$f":"PERCENTILE(U$6:U$20,[1]TOT!$S$1)","v":30.613999999999997}]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"original value","3<x>20"]

{"sheet":"24,25-24,5 GHz","index":22,"n_rows":18,"n_cols":25,"rows_kept":18,"cut":false,"hidden":false,"merged":[[1,0,3,0],[1,1,3,1],[1,2,1,4],[1,5,1,10],[1,11,1,12],[11,1,12,1],[1,15,1,20],[1,21,1,24],[2,5,2,6],[2,15,2,17],[2,18,2,20],[4,11,4,12],[1,14,3,14]]}
["all empty but"]
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L6:M102)","v":104},null,{"$f":"SUBTOTAL(9,N6:N102)","v":70}]
["CZE","24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAB"]
["DNK","24250-24500","X",null,null,null,null,null,null,null,null,null,1]
["GRC","24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,"ERC REP 38",null,null,null,null,null,null,"-",null,null,"No current use.\nAllocation for analogue links. SAP/SAB, ENG/OB"]
["HUN","24250-24500","X","X",null,"X","X",null,null,null,null,null,41,31,null,"X","X","X",null,7,null,0.25,"x",null,"ù"]
["LVA","24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAB/SAP, SRR"]
["LTU","24250-24500","X",null,null,"X",null,null,null,null,null,0,0,null,"local"]
["LUX","24250-24500",null,"X",null,null,"X","X","X",null,null,null,null,4,"Nat. freq. plan",null,null,null,null,null,null,"N/A","NO","NO"]
["LUX",null,"X",null,null,"X",null,"X","X",null,null,0,10,null,"Nat. freq. plan",null,"X",null,null,"2-15",null,"N/A","NO","NO"]
["PRT","24250-24500",null,null,null,null,null,null,null,null,"SRR, SRD"]
["RUS","24250-24500","No","No",null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["SVK","24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
[]
[null,null,{"$f":"COUNTA(C6:C16)","v":5},{"$f":"COUNTA(D6:D16)","v":3},0,3,2,2,2,0,{"$f":"COUNTA(K6:K16)","v":1},{"$f":"SUM(L6:L16)","v":0},{"$f":"SUM(M6:M16)","v":52},{"$f":"SUM(N6:N16)","v":35},null,{"$f":"COUNTA(P6:P16)","v":1},{"$f":"COUNTA(Q6:Q16)","v":2},{"$f":"COUNTA(R6:R16)","v":1}]

{"sheet":"24,5-26,5 GHz","index":23,"n_rows":70,"n_cols":26,"rows_kept":70,"cut":false,"hidden":false,"merged":[[3,11,3,12],[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[0,14,2,14],[30,15,31,15],[30,16,31,16],[30,17,31,17],[30,18,31,18],[30,19,31,19],[32,15,33,15],[32,16,33,16],[32,17,33,17],[32,18,33,18],[32,19,33,19],[34,20,35,20],[30,21,31,21],[30,22,31,22],[30,23,31,23],[30,24,31,24],[32,20,33,20],[30,20,31,20],[34,21,35,21],[34,22,35,22],[34,23,35,23],[34,24,35,24],[32,21,33,21],[32,22,33,22],[32,23,33,23],[32,24,33,24],[34,15,35,15],[34,16,35,16],[34,17,35,17],[34,18,35,18],[34,19,35,19]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M102)","v":74316},null,{"$f":"SUBTOTAL(9,N5:N102)","v":3292}]
["TELIASON","24500-26500",null,"X",null,null,null,"X",null,null,null,null,161,null,"T/R 13-02 Annex B",99,18,44,2,null,10,"-",null,null,null,"Eric sson ML"]
["TELIASON","24500-26500",null,"X",null,null,null,null,null,null,null,null,629,null,null,null,574,55,1,null,12,"+",null,null,null,"NEC NEO"]
["AUT","24500-26500","X",null,null,"X",null,"X",null,null,null,null,2365,null,"T/R 13-02 Annex B","x","x","x",1,6,24]
["AUT","24500-26500"]
["BIH","24500-26500","X","X",null,null,null,"X",null,null,null,null,3,null,"T/R 13-02 Annex B","X","X","X",1,4,6,"+35",null,null,"24500-26500, 27500-29500 MHz: Shared band between P-P links and FWA. Actually, block assignments for P-P links in process. We still do not have active implemented FWA systems."]
["BIH","24500-26500",null,"X",null,"X","X"]
["HRV","24500-26500",null,"X",null,null,"X",null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["HRV","24500-26500"]
["CZE","24500-24745/25500-25753",null,"X",null,null,"X",null,null,null,null,null,null,133,"T/R 13-02 Annex B",null,null,null,null,null,null,10]
["CZE","24745-25500/25753-26500","X",null,null,"X",null,null,null,null,null,null,4537,null,null,null,null,null,null,null,null,10]
["CYP","24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["CYP","24500-26500"]
["DNK","24500-26500",null,"X",null,null,null,null,null,null,null,null,null,"No info","T/R 13-02 Annex B"]
["DNK","24500-26500","X",null,null,null,null,null,null,null,null,null,null,135]
["EST","24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["EST","24500-26500"]
["FIN","24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["FIN","24500-26500"]
["FRA","24500-26500","X","X",null,"X","X","X",null,null,null,null,215,75,"T/R 13-02 Annex B",null,88,127,0.12,"3<x>20",15,"+ 3 %"]
["FRA","24500-26500"]
["GER","24500-26500","x",null,null,"x","x",null,null,null,null,15880,null,null,"ERC/REC 13-02 ",null,"x",null,0.1,4,10.9]
["GER","24500-26500",null,"x",null,null,null,null,null,null,null,null,null,836]
["GRC","24500-26500",null,"X",null,"X","X",null,null,null,null,null,null,null,"ERC/REC 13-02","-",null,null,null,null,null,"-",null,null,"5 issued licenses"]
["HUN","24500-26500","X","X",null,"X","X",null,null,null,null,null,83,31,"T/R 13-02 Annex B","X","X","X",null,7,null,0.25,"x",null,"PMP systems"]
["HUN","24500-26500"]
["ICE","24500-26500","X",null,null,"x",null,null,null,null,null,null,2,null,"T/R 13-02 Annex B",null,null,2,12,15,18,10]
["IRL","24500-26500"," X",null,null,"X",null," X",null,null,null,null,636,null,"T/R 13-02 Annex B"," X","X","X",0.05,5,17," 43"," X"]
["IRL","24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["IRL","24500-26500",null," X",null,null,null," X",null,null,null,null,null,null," National Legislation: S.I. 762 of 2007"]
["IRL","24500-26500",null,null,null,null,null,null,null,null,null,null,null,null," "]
["IRL","24500-26500","X",null,null,null,"X",null,null,null,null,null,null,15,"National Legislation: S.I. 79 of 2003",null,null,null,null,null,null,55]
["IRL","24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 530 of 2003"]
["ITA","24500-26500",null,"X",null,null,"X","X",null,null,null,null,null,"not known","T/R 13-02 Annex B",null,null,null,null,null,null,0.15,"not yet"]
["ITA","24500-26500"]
["LVA","24500-26500","X",null,null,"x",null,null,null,null,null,null,6,null,"T/R 13-02 Annex B",null,null,"X",1.4,5,6]
["LVA","24500-26500",null,"X",null,null,"X",null,null,null,null,null,null,52,null,null,"X",null,null,5,null,50]
["LTU","24500-26500","X",null,null,"X",null,null,null,null,null,0,0,null,"T/R 13-02 Annex B"]
["LTU","24500-26500",null,"X",null,null,"X",null,null,null,null,null,null,84,"T/R 13-02 Annex B",null,null,null,null,null,null,30]
["LUX","24500-26500",null,"X",null,null,"X","X","X",null,null,null,null,4,"T/R 13-02 Annex B",null,null,null,null,null,null,"N/A","NO","NO"]
["LUX","24500-26500","X",null,null,"X",null,"X","X",null,null,0,10,null,"Nat. freq. plan",null,"X",null,null,"2-15",null,"N/A","NO","NO"]
["NLD","24500-26500","x",null,null,null,null,null,null,"X",null,null,908,null,"T/R 13-02 Annex B","x","x","x",2.5499999999999998,6.42,14.52,30]
["NLD","24500-26500",null,null,null,null,"x",null,null,"X",null,null,null,90,"T/R 13-02 Annex B",null,null,null,null,null,null,10]
["NOR","24500-26500",null,"x",null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annex B"]
["NOR","24500-26500","x",null,null,null,null,null,null,"X",null,3,65,null,null,null,"x","x",0.5,4.8,21.1]
["PRT","24500-26500",null,"X",null,null,"X","X",null,null,"SRR, SRD, Military (25.25-25.492 GHz and 26.25-27.5 GHz)",null,null,125,"T/R 13-02 Annex B","X","X",null,null,"5",null,0]
["PRT","24500-26500"]
["RUS","24500-26500","X","X",null,null,"X","X",null,null,null,null,447,null,"T/R 13-02 Annex B","X","X","X",2,4,8]
["RUS","24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["SRB","24500-26500","X",null,null,null,null,"X",null,null,null,null,660,null,"T/R 13-02 Annex B","X","X","X",0.6,2.21,12.5,100]
["SRB","24500-26500",null,"X",null,null,"X",null,null,null,null,null,null,4]
["SVK","24500-26500","X",null,null,"X",null,"X",null,null,null,null,1230,null,"T/R 13-02 Annex B","x","x","x",0.1,3.5,8,20]
["SVK","24500-26500",null,"X",null,null,"X",null,null,null,null,null,null,40,null,"x","x",null,null,null,null,10]
["SVN","24500-26500","X",null,null,"X",null,"X",null,null,null,null,109,null,"T/R 13-02 Annex B (25.165-25.557 GHz/>26.173 GHz)",null,"x",null,3,6,8,100,null,null,null,"used instead of the congested 23 GHz band"]
["SVN","24500-26500","X",null,null,null,"X","X",null,null,null,null,null,22,"T/R13-02 AnnexB (25.053-25.165GHz/26.061-26.173GHz)",null,"x",null,null,null,null,-5]
["SVN","24500-26500",null,"X",null,null,"X",null,null,null,"BWA",null,null,"planned","T/R13-02 Annex B (24.549–25.053GHz/25.557–26.061GHz)",null,"x","x",1,3,5,null,null,null,"BWA"]
["SWE","24500-26500",null,"X",null,"X","X","X",null,null,null,null,5601,null,"T/R 13-02 Annex B",null,null,null,null,null,null,"Y"]
["SWE","24500-26500","X",null,null,"X",null,null,null,null,null,null,null,null," ERC / REC / (00) 05",null,null,null,null,null,null,null,"N"]
["CHE","24500-26500","X",null,null,"X",null,"X",null,null,null,null,38,null,"T/R 13-02 Annex B",null,null,38,2,2.9,5.9,"growth",null,null,"problem: SRR"]
["CHE","24500-26500"]
["GBR","24500-26500","X",null,null,null,null,null,null,"X",null,3570,null,null,"T/R 13-02","X","X","X"]
["GBR","24500-26500"]
[]
[null,null,{"$f":"COUNTA(C5:C65)","v":23},23,0,17,20,17,2,5,{"$f":"COUNTA(K5:K65)","v":2},{"$f":"SUM(L5:L65)","v":19453},{"$f":"SUM(M5:M65)","v":17705},{"$f":"SUM(N5:N65)","v":1646},null,{"$f":"COUNTA(P5:P65)","v":13},{"$f":"COUNTA(Q5:Q65)","v":21},{"$f":"COUNTA(R5:R65)","v":17},{"$f":"MIN(S$5:S$65)","v":0.05},{"$f":"MIN(T$5:T$65)","v":2.21},{"$f":"MIN(U$5:U$65)","v":5},{"$f":"COUNTA(V5:V65)","v":26},{"$f":"COUNTA(W5:W65)","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$65)","v":1},{"$f":"MEDIAN(T$5:T$65)","v":4.9000000000000004},{"$f":"MEDIAN(U$5:U$65)","v":10.9}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$65)","v":12},{"$f":"MAX(T$5:T$65)","v":15},{"$f":"MAX(U$5:U$65)","v":24}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$65,[1]TOT!$S$1)","v":4.7999999999999936},{"$f":"PERCENTILE(T$5:T$65,[1]TOT!$S$1)","v":9},{"$f":"PERCENTILE(U$5:U$65,[1]TOT!$S$1)","v":21.68}]

{"sheet":"26,5-27,5 GHz","index":24,"n_rows":16,"n_cols":25,"rows_kept":16,"cut":false,"hidden":false,"merged":[[1,0,3,0],[1,1,3,1],[1,2,1,4],[1,5,1,10],[1,11,1,12],[5,1,6,1],[1,15,1,20],[1,21,1,24],[2,5,2,6],[2,15,2,17],[2,18,2,20],[4,11,4,12],[1,14,3,14]]}
["all empty but"]
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L6:M102)","v":52},null,{"$f":"SUBTOTAL(9,N6:N102)","v":0}]
["CZE","26500-27500",null,null,null,null,null,null,null,null,"MD"]
["CZE"]
["GRC","26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["HUN","26500-27500",null,null,null,"X",null,null,null,null,"Land military systems. P-P links Harmonized NATO band type 2.(planned)",null,null,null,null,null,null,null,null,null,null,null,"X"]
["LVA","26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band"]
["PRT","26500-27500",null,null,null,null,null,null,null,null,"SRR, SRD, Military (26.25-27.5 GHz)"]
["RUS","26500-27500","X","X",null,null,"X","X",null,null,null,null,26,null,"F.748 ITU-R","X","X","X",2,4,8]
["SRB","26500-27500",null,null,null,null,null,null,null,"X"]
["SVK","26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
[]
[null,null,{"$f":"COUNTA(C6:C14)","v":1},{"$f":"COUNTA(D6:D14)","v":1},0,1,1,1,0,1,{"$f":"COUNTA(K6:K14)","v":3},{"$f":"SUM(L6:L14)","v":0},{"$f":"SUM(M6:M14)","v":26},{"$f":"SUM(N6:N14)","v":0},null,{"$f":"COUNTA(P6:P14)","v":1},{"$f":"COUNTA(Q6:Q14)","v":1},{"$f":"COUNTA(R6:R14)","v":1},{"$f":"PERCENTILE(S$6:S$14,[1]TOT!$S$1)","v":2},{"$f":"PERCENTILE(T$6:T$14,[1]TOT!$S$1)","v":4},{"$f":"PERCENTILE(U$6:U$14,[1]TOT!$S$1)","v":8}]

{"sheet":"27,5-29,5 GHz","index":25,"n_rows":63,"n_cols":26,"rows_kept":63,"cut":false,"hidden":false,"merged":[[3,11,3,12],[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[0,14,2,14],[31,1,32,1],[4,1,5,1],[6,1,7,1],[8,1,9,1],[10,1,11,1],[14,1,15,1],[16,1,17,1],[18,1,19,1],[20,1,21,1],[22,1,23,1],[26,1,27,1],[29,1,30,1],[56,1,57,1],[33,1,34,1],[35,1,36,1],[37,1,38,1],[39,1,40,1],[41,1,42,1],[43,1,44,1],[45,1,46,1],[47,1,48,1],[49,1,50,1],[51,1,52,1],[54,1,55,1]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M102)","v":4942},null,{"$f":"SUBTOTAL(9,N5:N102)","v":366}]
["TELIASON","27500-29500",null,"X",null,null,null,"X",null,null,null,null,6,null,"T/R 13-02 Annex C",null,null,6,1,null,4,"++",null,null,null,"Ericsson TN"]
["TELIASON"]
["AUT","27500-29500","X",null,null,"X",null,"X",null,null,null,null,156,null,"T/R 13-02 Annex C",null,null,"x",1,2,4]
["AUT"]
["BIH","27500-29500","X","X",null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,"+5",null,null,"24500-26500, 27500-29500 MHz: Shared band between P-P links and FWA. Actually, block assignments for P-P links in process. We still do not have active implemented FWA "]
["BIH",null,null,"X",null,"X","X"]
["HRV","27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["HRV"]
["CZE","27500-29050",null,"X",null,null,"X",null,null,null,null,null,null,41,"T/R 13-02 Annex C"]
["CZE","28050-29500","X","X",null,"X","X",null,null,null,null,null,189]
["CYP","27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["CYP"]
["DNK","27500-29500","X",null,null,null,null,null,null,null,null,null,null,18,"T/R 13-02 Annex C"]
["DNK"]
["EST","27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["EST"]
["FIN","27500-29500","X",null,null,null,null,"X",null,null,null,null,380,null,"T/R 13-02 Annex C",null,"X","X",0.1,1.1000000000000001,7.2,0.9,"x",null,"Local congestion"]
["FIN"]
["FRA","27500-29500","X",null,null,"X",null,"X",null,null,null,null,null,null,"T/R 13-02 Annex C"]
["FRA"]
["GER","27500-29500",null,"x",null,"x","x",null,null,null,null,1424,null,29,"ERC/REC 13-02 ",null,null,null,0.18,3,13.3]
["GRC","27500-29500",null,null,null,"X","X",null,null,null,null,null,null,null,"ECC/DEC/(05)01","no current use",null,null,null,null,null,"-",null,null,"27828,5-27940,5 and 27940,5-28444,5 MHz paired with 28948,5-29452,5 new row by EETT allocated to digital P-P and P-MP links"]
["HUN","27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["HUN"]
["ICE","27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["IRL","27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["IRL"]
["ITA","27500-29500",null,"X",null,null,"X","X",null,null,null,null,null,"not known","T/R 13-02 Annex C",null,null,null,null,null,null,0.15,"not yet"]
["ITA"]
["LVA","27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["LVA",null,null,"X",null,null,"X",null,null,null,null,null,null,51,null,null,null,"X",null,null,null,50]
["LTU","27500-29500","X",null,null,"X",null,null,null,null,null,null,20,null,"T/R 13-02 Annex C",null,20]
["LTU",null,null,"X",null,null,"X",null,"X",null,null,null,null,8,"54MHz/3,2MHz",null,null,null,null,null,null,0,null,null,"LMDS (do not comply T/R 13-02)"]
["LUX","27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["LUX",null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["NLD","27500-29500","X",null,null,null,null,null,null,"X",null,null,185,null,"T/R 13-02 Annex C",null,null,"x",2.52,4.21,6.8730000000000002,30]
["NLD"]
["NOR","27500-29500",null,"X",null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annex C"]
["NOR",null,"X",null,null,null,null,null,null,"X",null,null,0]
["PRT","27500-29500",null,"X",null,null,"X",null,null,null,"FSS, HDFSS",null,null,21,"T/R 13-02 Annex C",null,"X",null,null,"5",null,0]
["PRT"]
["RUS","27500-29500","X","X",null,null,"X","X",null,null,null,null,1,null,"T/R 13-02 Annex C","X","X","X",2,4,8]
["RUS",null,null,null,null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["SRB","27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["SRB"]
["SVK","27500-29500","X",null,null,"X",null,"X",null,null,null,null,110,null,"T/R 13-02 Annex C","x","x","x",0.2,2.5,4.5,10]
["SVK",null,null,"X",null,null,"X",null,null,null,null,null,null,15,null,"x","x",null,null,null,null,10]
["SVN","27500-29500","X",null,null,"X",null,"X",null,null,null,null,"planned",null,"T/R 13-02 Annex C (27.8285 – 27.9405 GHz/28.8365 – 28.9485 GHz)",null,"x",null,0.5,3,5]
["SVN",null,null,"X",null,null,"X",null,null,null,null,null,null,"planned","T/R13-02 Annex C (27.9405 – 28.4445 GHz/28.9485 – 29.4525 GHz)",null,"x","x",0.3,2,4]
["SWE",null,null,"X",null,"X","X","X",null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,"Y"]
["CHE","27500-29500","X",null,null,"X",null,"X",null,null,null,null,"starts now",null,"T/R 13-02 Annex C",null,null,null,null,null,null,"growth"]
["CHE"]
["GBR","27500-29500"]
["GBR"]
[]
[null,null,{"$f":"COUNTA(C5:C58)","v":13},15,0,11,13,10,1,3,{"$f":"COUNTA(K5:K58)","v":1},{"$f":"SUM(L5:L58)","v":1424},{"$f":"SUM(M5:M58)","v":1047},{"$f":"SUM(N5:N58)","v":183},null,{"$f":"COUNTA(P5:P58)","v":4},{"$f":"COUNTA(Q5:Q58)","v":8},{"$f":"COUNTA(R5:R58)","v":8},{"$f":"MIN(S$5:S$58)","v":0.1},{"$f":"MIN(T$5:T$58)","v":1.1000000000000001},{"$f":"MIN(U$5:U$58)","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$58)","v":0.5},{"$f":"MEDIAN(T$5:T$58)","v":2.75},{"$f":"MEDIAN(U$5:U$58)","v":5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$58)","v":2.52},{"$f":"MAX(T$5:T$58)","v":4.21},{"$f":"MAX(U$5:U$58)","v":13.3}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$58,[1]TOT!$S$1)","v":2.3119999999999998},{"$f":"PERCENTILE(T$5:T$58,[1]TOT!$S$1)","v":4.1364999999999998},{"$f":"PERCENTILE(U$5:U$58,[1]TOT!$S$1)","v":11.179999999999998}]

{"sheet":"31-31,3 GHz","index":26,"n_rows":17,"n_cols":25,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,0,3,0],[1,1,3,1],[1,2,1,4],[1,5,1,10],[1,11,1,12],[10,1,11,1],[1,15,1,20],[1,21,1,24],[2,5,2,6],[2,15,2,17],[2,18,2,20],[4,11,4,12],[1,14,3,14]]}
["all empty but"]
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L6:M101)","v":0},null,{"$f":"SUBTOTAL(9,N6:N101)","v":0}]
["CZE","31000-31300","X",null,null,"X",null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,5]
["GER","31000-31300",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,"x",null,null,null,null,null,null,null,"not open"]
["HUN","31000-31300","X",null,null,"X",null,null,null,null,null,null,null,null,"ECC/REC/(02)02","X","X","X",null,5,null,null,"x",null,"FDD mode PP systems"]
["LVA","31000-31300","?",null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,null,null,null,"Fixed links, FWA"]
["LTU","31000-31300","X",null,null,"X",null,null,null,null,null,0,0,null,"ECC/REC/(02)02"]
["LUX","31000-31300","X",null,null,"X",null,"X",null,null,null,0,0,null,"ECC/REC/(02)02",null,null,null,null,null,null,"N/A","NO","NO"]
["LUX",null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["PRT","31000-31300",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,"Planned"]
["RUS","31000-31300","No","No",null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02"]
["GBR","31000-31300","X",null,null,null,null,null,null,null,"X",null,null,null,"national arrangement"]
[]
[null,null,{"$f":"COUNTA(C6:C15)","v":7},{"$f":"COUNTA(D6:D15)","v":1},0,4,0,1,0,0,{"$f":"COUNTA(K6:K15)","v":1},{"$f":"SUM(L6:L15)","v":0},{"$f":"SUM(M6:M15)","v":0},{"$f":"SUM(N6:N15)","v":0},null,{"$f":"COUNTA(P6:P15)","v":1},{"$f":"COUNTA(Q6:Q15)","v":2},{"$f":"COUNTA(R6:R15)","v":1}]

{"sheet":"31,8-33,4 GHz","index":27,"n_rows":44,"n_cols":26,"rows_kept":44,"cut":false,"hidden":false,"merged":[[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[35,1,36,1],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[3,11,3,12],[0,14,2,14],[16,1,17,1],[23,1,24,1],[26,1,27,1],[29,1,30,1],[33,1,34,1]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M102)","v":10354},null,{"$f":"SUBTOTAL(9,N5:N102)","v":0}]
["TELIASON","31800-33400","X",null,null,null,null,"X",null,null,null,null,1085,null,"ERC/REC/(01)02",null,996,89,0.2,null,8.6999999999999993,"+",null,null,null,"NEC NEO"]
["AUT","31800-33400"]
["BIH","31800-33400"]
["HRV","31800-33400"]
["CZE","31800-33400","X",null,null,"X",null,null,null,null,null,null,50,null,"ERC/REC/(01)02",null,null,null,null,null,null,50]
["CYP","31800-33400"]
["DNK","31800-33400",null,"X",null,null,null,null,null,null,null,null,"No info",null,"ERC/REC/(01)02"]
["EST","31800-33400"]
["FIN","31800-33400","X",null,null,null,null,"X",null,null,null,null,1,null,"ERC/REC/(01)02",null,"X","X",null,null,null,100]
["FRA","31800-33400","X","X",null,"X",null,"X",null,null,null,null,null,null,"ERC/REC/(01)02"]
["GER","31800-33400","x",null,null,"x",null,null,null,null,null,1466,null,null,"ERC/REC/(01)02",null,"x",null,0.1,2.2999999999999998,6.8,20]
["GRC","31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["HUN","31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,"x"]
["HUN",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(04)06",null,null,null,null,null,null,null,"x"]
["ICE","31800-33400"]
["IRL","31800-33400"]
["ITA","31800-33400"]
["LVA","31800-33400",null,"X",null,"X",null,null,null,null,null,null,43,null,"ERC/REC/(01)02",null,null,"X",0.2,3,4.5999999999999996,100]
["LTU","31800-33400","X",null,null,"X",null,null,null,null,null,null,28,null,"ERC/REC/(01)02"]
["LUX","31800-33400","X",null,null,"X",null,"X",null,null,null,0,0,null,"ERC/REC/(01)02",null,null,null,null,null,null,"N/A","NO","NO"]
["LUX",null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan "]
["NLD","31800-33400","X",null,null,null,null,null,null,"X",null,null,515,null,"ERC/REC/(01)02","x","x","x",0.253,3.57,6.27,30]
["NOR","31800-33400",null,"X",null,null,null,null,null,"X",null,null,null,null,"ERC/REC/(01)02"]
["NOR",null,"X",null,null,null,null,null,null,"X",null,null,0]
["PRT","31800-33400","X",null,null,"X","X",null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,null,null,"Not used at the moment."]
["RUS","31800-33400","No","No",null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02"]
["RUS",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(04)06"]
["SRB","31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,null,null,"it have not been used yet"]
["SVK","31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,100,null,null,"operation expected"]
["SVN","31800-33400","x",null,null,"X",null,"X",null,null,null,null,"planned Upper part",null,"ERC/REC/(01)02",null,"x","x",0.2,2,4]
["SVN",null,null,"x",null,null,"X",null,null,null,"BWA",null,"planned Lower part",null,"ERC/REC/(01)02/ ECC/REC/(04)06",null,"x","x",0.2,1,3,null,null,null,"BWA"]
["SWE","31800-33400",null,null,null,null,null,null,null,null,null,null,1887,null,"ERC/REC/(01)02"]
["SWE",null,"X",null,null,"X",null,null,null,null,null,null,null,null,"ECC/REC/(04)06",null,null,null,null,null,null,"Y","N"]
["CHE","31800-33400","X",null,null,"X",null,"X",null,null,null,null,102,null,"ERC/REC/(01)02",null,69,33,0.5,2.2999999999999998,4.5999999999999996,"growth"]
["GBR","31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it have not been used yet"]
[]
[null,null,{"$f":"COUNTA(C5:C39)","v":14},6,0,10,2,6,0,3,{"$f":"COUNTA(K5:K39)","v":1},{"$f":"SUM(L5:L39)","v":1466},{"$f":"SUM(M5:M39)","v":3711},{"$f":"SUM(N5:N39)","v":0},null,{"$f":"COUNTA(P5:P39)","v":1},{"$f":"COUNTA(Q5:Q39)","v":7},{"$f":"COUNTA(R5:R39)","v":7},{"$f":"MIN(S$5:S$39)","v":0.1},{"$f":"MIN(T$5:T$39)","v":1},{"$f":"MIN(U$5:U$39)","v":3},{"$f":"COUNTA(V5:V39)","v":10},{"$f":"COUNTA(W5:W39)","v":4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$39)","v":0.2},{"$f":"MEDIAN(T$5:T$39)","v":2.2999999999999998},{"$f":"MEDIAN(U$5:U$39)","v":4.5999999999999996}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$39)","v":0.5},{"$f":"MAX(T$5:T$39)","v":3.57},{"$f":"MAX(U$5:U$39)","v":8.6999999999999993}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$39,[1]TOT!$S$1)","v":0.42589999999999983},{"$f":"PERCENTILE(T$5:T$39,[1]TOT!$S$1)","v":3.4274999999999998},{"$f":"PERCENTILE(U$5:U$39,[1]TOT!$S$1)","v":8.129999999999999}]

{"sheet":"36-37 GHz","index":28,"n_rows":7,"n_cols":25,"rows_kept":7,"cut":false,"hidden":false,"merged":[[3,11,3,12],[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[0,14,2,14]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M101)","v":264},null,{"$f":"SUBTOTAL(9,N5:N101)","v":0}]
["RUS","36000-37000","X","X",null,null,null,"X",null,null,null,null,132,null,"F.749 ITU-R","X","X","X",0.1,3,5]
[]
[null,null,{"$f":"COUNTA(C5)","v":1},1,0,0,0,1,0,0,{"$f":"COUNTA(K5)","v":0},{"$f":"SUM(L5)","v":0},{"$f":"SUM(M5)","v":132},{"$f":"SUM(N5)","v":0},null,{"$f":"COUNTA(P5)","v":1},{"$f":"COUNTA(Q5)","v":1},{"$f":"COUNTA(R5)","v":1},{"$f":"PERCENTILE(S$5:S$6,[1]TOT!$S$1)","v":0.1},{"$f":"PERCENTILE(T$5:T$6,[1]TOT!$S$1)","v":3},{"$f":"PERCENTILE(U$5:U$6,[1]TOT!$S$1)","v":5}]

{"sheet":"37-39,5 GHz","index":29,"n_rows":47,"n_cols":26,"rows_kept":47,"cut":false,"hidden":false,"merged":[[3,11,3,12],[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[0,14,2,14],[20,8,21,8],[20,9,21,9],[20,10,21,10],[10,1,11,1],[17,1,18,1],[20,1,21,1],[20,2,21,2],[20,3,21,3],[20,4,21,4],[41,11,41,12],[20,24,21,24],[25,1,26,1],[28,1,29,1],[32,1,33,1],[36,1,37,1],[38,1,39,1],[20,11,21,11],[20,12,21,12],[20,13,21,13],[20,21,21,21],[20,22,21,22],[20,23,21,23],[20,5,21,5],[20,6,21,6],[20,7,21,7]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M102)","v":239846},null,{"$f":"SUBTOTAL(9,N5:N102)","v":0}]
["TELIASON","37000-39500","X",null,null,null,null,"X",null,null,null,null,173,null,"T/R 12-01",95,78,null,0.1,null,5.4,0,null,null,null,"Ericsson ML"]
["AUT","37000-39500","X",null,null,"X",null,"X",null,null,null,null,5273,null,"T/R 12-01","x","x","x",1,5,17]
["BIH","37000-39500","X",null,null,null,null,"X",null,null,null,1,23,null,"T/R 12-01","X",null,null,"0.1",1,5,"+5"]
["HRV","37000-39500","X",null,null,null,null,"X",null,null,null,null,335,null,"T/R 12-01",null,"x",null,7.0000000000000007E-2,0.42,4.9000000000000004,20]
["CZE","37000-39500","X",null,null,"X",null,null,null,null,null,null,5603,null,"T/R 12-01",null,null,null,null,null,null,5]
["CYP","37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 12-01"]
["DNK","37000-39500","X",null,null,null,null,null,null,null,null,null,158,null,"T/R 12-01"]
["DNK",null,null,"X",null,null,null,null,null,null,null,null,"No info"]
["EST","37000-39500",null,null,null,null,null,null,null,null,null,null,232,null,"T/R 12-01",169,63,null,0.7,5,10,"+10"]
["FIN","37000-39500","X",null,null,null,null,"X",null,null,null,null,45,null,"T/R 12-01",null,"X","X",0.2,1.7,6.1,0.1]
["FRA","37000-39500","X","X",null,"X",null,"X",null,null,null,null,8304,null,"T/R 12-01",2223,6057,24,0.1,"0<x>6",15,"+8%"]
["GER","37000-39500","x",null,null,"x",null,null,null,null,null,30594,null,null,"ERC/REC 12-01 ",null,"x",null,0.02,2.2999999999999998,13.2]
["GRC","37000-39500","X",null,null,null,null,"X",null,null,null,null,984,null,"T/R 12-01",null,"X","X","0.05","1.5","6.8",0.2]
["HUN","37000-39500","X",null,null,"X",null,null,null,null,null,null,6454,null,"T/R 12-01","X","X","X",null,4]
["HUN",null,null,null,null,null,null,null,null,null,"37926-38178 and 39186-39500 MHz Non-Civil P-P links.   39186-39500 MHz Emergency services. 37-39.5 GHz NJFA military requirement for existing and future fixed systems.",null,100,null,"ERC/DEC/(00)02","X","X","X"]
["ICE","37000-39500","X",null,null,"X",null,null,null,null,null,null,1,null,"T/R 12-01",1,null,null,null,5]
["IRL","37000-39500"," X",null,null,null,null,"X",null,null,null,null,2924,null,"T/R 12-01"," X","X","X",1.6E-2,1.9,10.7," 31"," X"]
["IRL",null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["ITA","37000-39500","X","X",null,"X",null,"X",null,null,null,null,10412,null,"T/R 12-01","X","X","X",null,"0,8/10",null,0.25,"yes"]
["LVA","37000-39500","X",null,null,"X",null,null,null,null,null,null,27,null,"T/R 12-01",null,null,"X",0.2,3,4.7,20]
["LTU","37000-39500","X",null,null,"X",null,null,null,null,null,null,268,null,"T/R 12-01",null,268]
["LUX","37000-39500","X",null,null,"X",null,"X","X",null,null,1,110,null,"T/R 12-01",null,"X",null,0.13,"1-6",5.4,"N/A","NO","NO"]
["LUX",null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["NLD","37000-39500","X",null,null,null,null,null,null,"X",null,null,6377,null,"T/R 12-01","x","x","x",0.05,2.15,10.266,30]
["NOR","37000-39500",null,"x",null,null,null,null,null,"X",null,null,null,null,"T/R 12-01 Annex A"]
["NOR",null,"X",null,null,null,null,null,null,"X",null,null,64,null,null,null,null,"x",0.1,3.6,16.399999999999999]
["NOR","39500-40500"]
["PRT","37000-39500","X",null,null,"X",null,"X",null,null,"FS",null,617,null,"T/R 12-01","X","X","X",0,"2",6,5]
["RUS","37000-39500","X","X",null,null,null,"X",null,null,null,null,16865,null,"T/R 12-01","X","X","X",0.1,3,5]
["RUS",null,null,null,null,null,null,null,null,null,null,null,null,null,"F.749 ITU-R"]
["SRB","37000-39500","X",null,null,null,null,"X",null,null,null,null,426,null,"T/R 12-01","X","X","X",0.16,1.4,4.8600000000000003,300]
["SVK","37000-39500","X",null,null,"X",null,"X",null,null,null,null,1600,null,"T/R 12-01","x","x","x",0.1,2,9,20]
["SVN","37000-39500","X",null,null,"X",null,"X",null,null,null,null,580,null,"T/R 12-01",null,"x",null,0.1,2,4,30,"x***",null,null,"HI/LO problem"]
["SVN",null,"X",null,null,"X",null,"X"]
["SWE","37000-39500",null,null,null,null,null,null,null,null,null,null,6188,null,"T/R 12-01"]
["SWE",null,"X",null,null,"X",null,null,null,null,null,null,null,null,"T/R 12-01",null,null,null,null,null,null,"Y","N"]
["CHE","37000-39500","X",null,null,"X",null,"X",null,null,null,null,3134,null,"T/R 12-01",1248,1886,null,1,2.6,7.9,"unchanged","city areas congested, HIGH/LOW situation"]
["GBR","37000-39500","X",null,null,null,null,null,null,"X",null,12050,null,null,"T/R 12-01","X","X","X"]
[]
[null,null,{"$f":"COUNTA(C5:C42)","v":28},5,0,16,0,17,1,4,{"$f":"COUNTA(K5:K42)","v":2},{"$f":"SUM(L5:L42)","v":42646},{"$f":"SUM(M5:M42)","v":77277},{"$f":"SUM(N5:N42)","v":0},null,{"$f":"COUNTA(P5:P42)","v":17},{"$f":"COUNTA(Q5:Q42)","v":22},{"$f":"COUNTA(R5:R42)","v":16},{"$f":"MIN(S$5:S$42)","v":0},{"$f":"MIN(T$5:T$42)","v":0.42},{"$f":"MIN(U$5:U$42)","v":4},{"$f":"COUNTA(V5:V42)","v":19},{"$f":"COUNTA(W5:W42)","v":6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MEDIAN(S$5:S$42)","v":0.1},{"$f":"MEDIAN(T$5:T$42)","v":2.2999999999999998},{"$f":"MEDIAN(U$5:U$42)","v":6.1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(S$5:S$42)","v":1},{"$f":"MAX(T$5:T$42)","v":5},{"$f":"MAX(U$5:U$42)","v":17}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PERCENTILE(S$5:S$42,[1]TOT!$S$1)","v":1},{"$f":"PERCENTILE(T$5:T$42,[1]TOT!$S$1)","v":5},{"$f":"PERCENTILE(U$5:U$42,[1]TOT!$S$1)","v":16.459999999999997}]

{"sheet":"39,5-40,5 GHz","index":30,"n_rows":3,"n_cols":1,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["all empty"]
[]
["LVA indicated \"FSS earth stations\" in the notes"]

{"sheet":"40,5-43,5 GHz","index":31,"n_rows":36,"n_cols":25,"rows_kept":36,"cut":false,"hidden":false,"merged":[[0,0,2,0],[0,1,2,1],[0,2,0,4],[0,5,0,10],[0,11,0,12],[24,1,25,1],[30,1,31,1],[0,15,0,20],[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[3,11,3,12],[0,14,2,14]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M101)","v":146},null,{"$f":"SUBTOTAL(9,N5:N101)","v":6}]
["TELIASON","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["AUT","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["BIH","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["HRV","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["CZE","40500-43500","X",null,null,"X",null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"yes",null,null,"P-P and P-MP planned"]
["CYP","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["DNK","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["EST","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["FIN","40500-43500","X",null,null,null,null,"X",null,null,null,null,null,null,"ECC/REC/(01)04",null,"X","X",null,null,null,null,null,null,"Opens 2011"]
["FRA","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["GER","40500-43500","x",null,null,"x",null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,"x",null,null,null,null,null,null,"will be opened 2011"]
["GRC","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Use"]
["HUN","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["ICE","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["IRL","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["ITA","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["LVA","40500-43500",null,"X",null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,null,null,null,"MWS (MVDS)"]
["LTU","40500-43500",null,"X",null,null,"X",null,null,null,null,null,null,0,"ECC/REC/(01)04"]
["LUX","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["NLD","40500-43500","X",null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,100]
["NOR","40500-43500",null,"X",null,null,null,null,null,"X",null,null,null,null,"ECC/REC/(01)04 Annex A"]
["NOR",null,"X",null,null,null,null,null,null,"X",null,null,0]
["PRT","40500-43500",null,null,null,null,null,null,null,null,"MWS, MVDS",null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"Planned "]
["RUS","40500-43500","X","X",null,null,"X","X",null,null,null,null,73,null,"ECC/REC/(01)04","X","X","X",0.1,3,5]
["SRB","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["SVK","40500-43500",null,"X",null,null,"X",null,"X",null,null,null,null,3,"ECC/REC/(01)04",null,"x"]
["SVN","40500-43500",null,"X",null,null,"X",null,null,null,"MWS",null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"planned Upper part",null,null,"MWS"]
["SVN",null,"X",null,null,"X",null,"X",null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"planned Lower part (only small part)"]
["SWE","40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04\n(New ITU-R Rec under dev.)",null,null,null,null,null,null,"Y","N",null,"Blockassignments?"]
["CHE","40500-43500","X",null,null,"X",null,"X",null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"growth. Starts now"]
[]
[null,null,{"$f":"COUNTA(C5:C34)","v":8},6,0,4,4,4,1,2,{"$f":"COUNTA(K5:K34)","v":2},{"$f":"SUM(L5:L34)","v":0},{"$f":"SUM(M5:M34)","v":73},{"$f":"SUM(N5:N34)","v":3},null,{"$f":"COUNTA(P5:P34)","v":1},{"$f":"COUNTA(Q5:Q34)","v":3},{"$f":"COUNTA(R5:R34)","v":3},{"$f":"PERCENTILE(S$5:S$34,[1]TOT!$S$1)","v":0.1},{"$f":"PERCENTILE(T$5:T$34,[1]TOT!$S$1)","v":3},{"$f":"PERCENTILE(U$5:U$34,[1]TOT!$S$1)","v":5},{"$f":"COUNTA(V5:V34)","v":8},{"$f":"COUNTA(W5:W34)","v":1},{"$f":"COUNTA(X5:X34)","v":0},{"$f":"COUNTA(Y5:Y34)","v":7}]

{"sheet":"above 43,5 GHz","index":32,"n_rows":123,"n_cols":27,"rows_kept":123,"cut":false,"hidden":false,"merged":[[0,21,0,24],[1,5,1,6],[1,15,1,17],[1,18,1,20],[3,11,3,12],[0,0,2,0],[0,11,0,12],[0,14,2,14],[0,15,0,20]]}
["Country","Frequency band (MHz)","Licensing regime",null,null,"Application",null,null,null,null,null,"Number of P-P links",null,"Number of BS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends in the next 5 years"]
[null,null,null,null,null,"FWA",null,null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop lenght (km)"]
[null,null,"Link by link","Block","Unlicensed","P-P","P-MP","Network Infrastructure","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","congested","planned relocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["TOTAL",null,null,null,null,null,null,null,null,null,null,{"$f":"SUBTOTAL(9,L5:M129)","v":3310},null,{"$f":"SUBTOTAL(9,N5:N134)","v":0}]
["CZE","47200-48500","X",null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["LVA","47200-48500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAP/SAB, HAPS "]
["POR","47200-48500",null,null,null,null,null,null,null,null,"HDFSS (47.5-47.9 GHz)"]
["RUS","47200-48500"]
[null,null,{"$f":"COUNTA(C5:C8)","v":1},{"$f":"COUNTA(D5:D8)","v":0},0,1,0,0,0,0,null,{"$f":"SUM(L5:L8)","v":0},{"$f":"SUM(M5:M8)","v":0},{"$f":"SUM(N5:N8)","v":0},null,{"$f":"COUNTA(P5:P8)","v":0},{"$f":"COUNTA(Q5:Q8)","v":0},{"$f":"COUNTA(R5:R8)","v":0}]
["CZE","48500-50200","X",null,null,"X",null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["HUN","48500-50200",null,null,null,"X",null,null,null,null,"Non-Civil Digital P-P links",null,null,null,"ERC/REC 12-10"]
["LVA","48500-50200","X",null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"Fixed links"]
["LTU","48500-50200","X",null,null,"X",null,null,null,null,null,0,0,null,"ERC/REC 12-10"]
["LUX","48500-50200","X",null,null,"X",null,"X",null,null,null,0,0,null,"ERC/REC 12-10",null,null,null,null,null,null,"N/A","NO","NO"]
["NOR","48500-50200","X","X",null,null,null,null,null,"X",null,null,0,null,"ERC/REC 12-10"]
["POR","48500-50200",null,null,null,null,null,null,null,null,"HDFSS (48.2-48.54 GHz and 49.44-50.2 GHz)",null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,"Planned"]
["RUS","48500-50200",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10"]
["SRB","48500-50200",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["SVN","48500-50200",null,null,null,null,null,null,null,null,null,null,"planned",null,"ERC/REC 12-10"]
[null,null,{"$f":"COUNTA(C10:C19)","v":5},{"$f":"COUNTA(D10:D19)","v":1},0,4,0,1,0,1,null,{"$f":"SUM(L10:L19)","v":0},{"$f":"SUM(M10:M19)","v":0},{"$f":"SUM(N10:N19)","v":0},null,{"$f":"COUNTA(P10:P19)","v":0},{"$f":"COUNTA(Q10:Q19)","v":0},{"$f":"COUNTA(R10:R19)","v":0}]
["CZE","50400-51400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["DNK","50400-51400","X",null,null,null,null,null,null,null,null,null,1]
["LVA","50400-51400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Future satellite and terrestrial applications"]
["POR","50400-51400",null,null,null,null,null,null,null,"X"]
["RUS","50400-51400"]
["CZE","51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["GER","51400-52600","x",null,null,"x",null,null,null,null,null,null,null,0,"ERC/REC 12-11",null,"x"]
["HUN","51400-52600","X",null,null,"X",null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,null,null,"30 original value"]
["LVA","51400-52600","X",null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"Fixed links"]
["LTU","51400-52600","X",null,null,"X",null,null,null,null,null,0,0,null,"ERC/REC 12-11"]
["LUX","51400-52600","X",null,null,"X",null,"X",null,null,null,0,0,null,"ERC/REC 12-11",null,null,null,null,null,null,"N/A","NO","NO"]
["POR","51400-52600",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,"Planned"]
["RUS","51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11"]
["SRB","51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["SVN","51400-52600","X",null,null,"X",null,"X",null,null,null,null,"planned",null,"ERC/REC 12-11",null,"x","x",0.1,2,4]
["CHE","51400-52600",null,"X",null,"X",null,"X",null,null,null,null,837,null,"ERC/REC 12-11",193,644,null,0.15,0.8,2.8,"growth"]
["GBR","51400-52600","X",null,null,null,null,null,null,null,null,0,null,null,"ERC/REC 12-11"]
[null,null,{"$f":"COUNTA(C21:C37)","v":8},{"$f":"COUNTA(D21:D37)","v":1},0,6,0,3,0,2,null,{"$f":"SUM(L21:L37)","v":0},{"$f":"SUM(M21:M37)","v":838},{"$f":"SUM(N21:N37)","v":0},null,{"$f":"COUNTA(P21:P37)","v":1},{"$f":"COUNTA(Q21:Q37)","v":3},{"$f":"COUNTA(R21:R37)","v":1},{"$f":"PERCENTILE(S$21:S$37,[1]TOT!$S$1)","v":0.14749999999999999},{"$f":"PERCENTILE(T$21:T$37,[1]TOT!$S$1)","v":1.94},{"$f":"PERCENTILE(U$21:U$37,[1]TOT!$S$1)","v":3.94}]
["RUS","55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12"]
["CZE","55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["GER","55780-57000",null,null,null,null,null,null,null,null,null,null,null,0,"ERC/REC 12-12",null,"x",null,null,null,null,null,null,null,"not open"]
["GRC","55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12 Annex 3",null,null,null,null,null,null,"Maximum PFD=-26dBW/MHz",null,null,"No current use. Allocation for digital P-P links"]
["HUN","55780-57000","X",null,null,"X",null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,30]
["LVA","55780-57000","X",null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"Fixed links"]
["LUX","55780-57000","X",null,null,"X",null,"X",null,null,null,0,0,null,"ERC/REC 12-12",null,null,null,null,null,null,"N/A","NO","NO"]
["NOR","55780-57000","X","X",null,null,null,null,null,"X",null,null,0,null,"ERC/REC 12-09"]
["POR","55780-57000",null,null,null,null,null,null,null,null,"EESS",null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,"Planned"]
["SRB","55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["SWE","55780-57000",null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,"N"]
["SVN","55780-57000",null,null,null,null,null,null,null,null,null,null,"planned",null,"ERC/REC 12-12"]
["CHE","55780-57000",null,"X",null,"X",null,"X",null,null,null,null,0,null,"ERC/REC 12-12",null,null,null,null,null,null,"no equipment available"]
["GBR","55780-57000","X",null,null,null,null,null,null,null,null,0,null,null,"ERC/REC 12-12"]
[null,null,{"$f":"COUNTA(C39:C52)","v":5},{"$f":"COUNTA(D39:D52)","v":2},1,4,0,2,0,1,null,{"$f":"SUM(L39:L52)","v":0},{"$f":"SUM(M39:M52)","v":0},{"$f":"SUM(N39:N52)","v":0},null,{"$f":"COUNTA(P39:P52)","v":0},{"$f":"COUNTA(Q39:Q52)","v":1},{"$f":"COUNTA(R39:R52)","v":0}]
["CHE","57000-58000",null,"X",null,"X",null,"X",null,null,null,null,292,null,"ECC/REC/(09)01",292,null,null,0.1,0.3,2.2000000000000002,"reduction"]
["CZE","57000-59000","X",null,null,"X",null,null,null,null,null,null,3,null,"ECC/REC/(09)01",null,null,null,null,null,null,"yes"]
["GRC","57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-09 Annex A",null,null,null,null,null,null,"Radio Frequency Rights of Use not required. Maximum EIRP=15dBW",null,null,"No current use. Allocation for digital P-P links"]
["HUN","57000-59000","X",null,null,"X","X",null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,null,null,"25 original"]
["IRL","57000-59000","X",null,null,null,null," X",null,null,null,null,1,null,"ECC/REC/(09)01\nNational Legislation: S.I. 370 of 2009"," X",null,null,1.4,1.4,1.4," 0"]
["LVA","57000-59000",null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"SRD, Fixed links, FWA"]
["LUX","57000-59000","X",null,null,"X",null,"X",null,null,null,0,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"N/A","NO","NO"]
["POR","57000-59000","?","?",null,"X","X","X",null,null,"EESS, SRD",null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"No use at the moment."]
["RUS","57000-59000","X","X",null,null,null,"X",null,null,null,null,420,null,"ECC/REC/(09)01","X","X",null,0.1,1,2]
["RUS","57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,"F.1497 ITU-R"]
["SRB","57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["SWE","57000-59000",null,null,"X","X",null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Y","N",null,"Exemption"]
["SVN","57000-59000",null,null,"X","X",null,null,null,null,null,null,"N/A",null,"ECC/REC/(09)01",null,null,"x",null,1,null,"N/A"]
["GBR","57000-59000",null,null,"X",null,null,null,null,"X",null,null,null,null,"no channel plan"]
["NOR","57000-64000","X","X",null,null,null,null,null,"X",null,null,1,null,"ECC/REC/(09)01",null,null,1,null,0.4]
["GER","57100-58900",null,null,"x","x",null,null,null,null,null,null,null,null,"ECC/REC/(09)01","x"]
[null,null,{"$f":"COUNTA(C54:C69)","v":7},{"$f":"COUNTA(D54:D69)","v":4},5,8,2,5,0,2,null,{"$f":"SUM(L54:L69)","v":0},{"$f":"SUM(M54:M69)","v":717},{"$f":"SUM(N54:N69)","v":0},null,{"$f":"COUNTA(P54:P69)","v":4},{"$f":"COUNTA(Q54:Q69)","v":1},{"$f":"COUNTA(R54:R69)","v":2},{"$f":"PERCENTILE(S$54:S$69,[1]TOT!$S$1)","v":1.2699999999999998},{"$f":"PERCENTILE(T$54:T$69,[1]TOT!$S$1)","v":1.3199999999999998},{"$f":"PERCENTILE(U$54:U$69,[1]TOT!$S$1)","v":2.1800000000000002}]
["CHE","58000-63000",null,null,"X",null,null,null,null,null,null,null,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"no equipment available"]
["GER","59000-63000",null,null,"x","x",null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,"x"]
["CZE","59000-64000",null,null,null,null,null,null,null,null,"MD shared",null,null,null,"ECC/REC/(09)01"]
["HUN","59000-64000",null,null,null,null,null,null,null,null,"59000-61000 MHz Harmonized NATO band type 2. (planned for P-P)",null,null,null,"ECC/REC/(09)01"]
["LVA","59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"SRD,  Military band 59-61 GHz"]
["LUX","59000-64000","X",null,null,"X",null,"X",null,null,null,0,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"N/A","NO","NO"]
["POR","59000-64000",null,null,null,null,null,null,null,null,"SRD, ISM, Military (59-61 GHz)",null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Planned"]
["RUS","59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01"]
["SRB","59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["SWE","59000-64000",null,null,"X","X",null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Y","N",null,"Exemption"]
["GBR","59000-64000",null,null,"X",null,null,null,null,"X",null,null,null,null,"no channel plan"]
[null,null,{"$f":"COUNTA(C71:C81)","v":1},{"$f":"COUNTA(D71:D81)","v":0},4,3,0,1,0,1,null,{"$f":"SUM(L71:L81)","v":0},{"$f":"SUM(M71:M81)","v":0},{"$f":"SUM(N71:N81)","v":0},null,{"$f":"COUNTA(P71:P81)","v":0},{"$f":"COUNTA(Q71:Q81)","v":0},{"$f":"COUNTA(R71:R81)","v":1}]
["GER","64000-66000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)02",null,null,"x",null,null,null,null,null,null,"not open"]
["GRC","64000-66000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)02",null,null,null,null,null,null,null,null,null,"No current use. Allocation for digital P-P links"]
["HUN","64000-66000",null,null,null,"X",null,null,null,null,"Reserved for Civil and Non-Civil P-P links",null,null,null,"ECC/REC/(05)02"]
["LVA","64000-66000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)02",null,null,null,null,null,null,null,null,null,"SRD"]
["LTU","64000-66000",null,null,"X","X",null,null,null,null,null,0,0,null,"ECC/REC/(05)02"]
["LUX","64000-66000","X",null,null,"X",null,"X",null,null,null,0,0,null,"ECC/REC/(05)02",null,null,null,null,null,null,"N/A","NO","NO"]
["POR","64000-66000",null,null,null,null,null,null,null,"X",null,null,null,null,"ECC/REC/(05)02",null,null,null,null,null,null,"Planned"]
["RUS","64000-66000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)02"]
["SRB","64000-66000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)02",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["SVN","64000-66000","X",null,null,"X",null,"X",null,null,null,null,"planned",null,"ECC/REC/(05)02",null,null,"x"]
["CHE","64000-66000","X",null,null,"X",null,null,null,null,null,null,0,null,"ECC/REC/(05)02",null,null,null,null,null,null,"no equipment available"]
["GBR","64000-66000","X",null,null,null,null,null,null,"X",null,null,1,null,"no channel plan",null,null,"X"]
[null,null,{"$f":"COUNTA(C83:C94)","v":4},{"$f":"COUNTA(D83:D94)","v":0},1,5,0,2,0,2,null,{"$f":"SUM(L83:L94)","v":0},{"$f":"SUM(M83:M94)","v":1},{"$f":"SUM(N83:N94)","v":0},null,{"$f":"COUNTA(P83:P94)","v":0},{"$f":"COUNTA(Q83:Q94)","v":0},{"$f":"COUNTA(R83:R94)","v":3}]
["RUS","71000-76000 and  81000-86000",null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07"]
["CZE","71000-76000 and 81000-86000",null,null,"X","X",null,null,null,null,null,null,57,null,"ECC/REC/(05)07",null,null,null,null,null,null,100]
["FRA","71000-76000 and 81000-86000","X",null,null,"X",null,"X",null,null,null,null,0,null,"ECC/REC/(05)07"]
["GER","71000-76000 and 81000-86000","x",null,null,"x",null,null,null,null,null,null,null,0,"ECC/REC/(05)07",null,null,"x"]
["GRC","71000-76000 and 81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"No current use. Allocation for digital P-P links"]
["HUN","71000-76000 and 81000-86000",null,null,null,null,null,null,null,null,"71000-74000 and 81000-84000 MHz Common Civil and Non-Civil band for P-P links",null,null,null,"ECC/REC/(05)07"]
["IRL","71000-76000 and 81000-86000","X",null,null,null,null," X",null,null,null,null,5,null,"ECC/REC/(05)07\nNational Legislation: S.I. 370 of 2009",null,null," X",0.1,1,2.9," 0"]
["LVA","71000-76000 and 81000-86000","X",null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"Military band 71-74 GHz, 81-84 GHz. Fixed links 74-76GHz, 84-86 GHz"]
["LTU","71000-76000 and 81000-86000",null,null,"X","X",null,null,null,null,null,0,0,null,"ECC/REC/(05)07"]
["NOR","71000-76000 and 81000-86000","X","X",null,null,null,null,null,"X",null,null,4,null,"ECC/REC/(05)07",null,null,"x",1,1.8,3.4]
["POR","71000-76000 and 81000-86000","?","?",null,"X","X","X",null,null,"SRD, AM (75.5-76 GHz), Military (71-74 GHz and 81-84 GHz)",null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,"No use at the moment."]
["SRB","71000-76000 and 81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["SWE","71000-76000 and 81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,"Y","N",null,"Light Lic?"]
["CHE","71000-76000 and 81000-86000","X",null,null,"X",null,"X",null,null,null,null,"starts now",null,"ECC/REC/(05)07",null,null,null,null,null,null,"equipment not clear defined"]
["GBR","71000-76000 and 81000-86000","X",null,null,null,null,null,null,"X",null,null,30,null,"no channel plan",null,null,"X"]
["SVN","74000-76000 and 84000-86000","X",null,null,"X",null,null,null,"X",null,null,"planned",null,"ECC/REC/(05)07",null,null,"x"]
[null,null,{"$f":"COUNTA(C96:C111)","v":9},{"$f":"COUNTA(D96:D111)","v":2},3,7,1,4,0,3,null,{"$f":"SUM(L96:L111)","v":0},{"$f":"SUM(M96:M111)","v":96},{"$f":"SUM(N96:N111)","v":0},null,{"$f":"COUNTA(P96:P111)","v":0},{"$f":"COUNTA(Q96:Q111)","v":0},{"$f":"COUNTA(R96:R111)","v":5},{"$f":"PERCENTILE(S$96:S$111,[1]TOT!$S$1)","v":0.95499999999999996},{"$f":"PERCENTILE(T$96:T$111,[1]TOT!$S$1)","v":1.76},{"$f":"PERCENTILE(U$96:U$111,[1]TOT!$S$1)","v":3.375}]
["CZE","92000-95000","X",null,null,"X",null,null,null,null,null,null,3]
["HUN","92000-95000",null,null,null,null,null,null,null,null,null,null,null,null,"5.149"]
["LVA","92000-95000"]
["POR","92000-95000",null,null,null,null,null,null,null,"X"]
["RUS","92000-95000",null,null,"X"]
["SWE","92000-95000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N",null,"Light Lic?"]
["HUN",null,"X",null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,35]
["HUN",null,null,null,null,"X","X",null,null,null,"571000-589000 GHz Non-Civil P-P, P-MP systems",null,null,null,"ERC/REC 12-09"]
["HUN",null,null,null,null,null,null,null,null,null," 71000-74000 and 81000-84000 MHz Harmonized NATO band type 3. (reserved for military satellite systems)"]
[]
[null,null,{"$f":"COUNTA(C113:C119)","v":2},{"$f":"COUNTA(D113:D119)","v":0},1,2,0,0,0,1,null,{"$f":"SUM(L113:L118)","v":0},{"$f":"SUM(M113:M118)","v":3},{"$f":"SUM(N113:N118)","v":0},null,{"$f":"COUNTA(P113:P118)","v":0},{"$f":"COUNTA(Q113:Q118)","v":0},{"$f":"COUNTA(R113:R118)","v":0}]

{"sheet":"Alf Admins","index":33,"n_rows":1023,"n_cols":55,"rows_kept":1023,"cut":false,"hidden":false,"merged":[[1,4,1,7],[1,8,1,9],[1,10,1,14],[1,15,1,16],[1,18,3,18],[1,25,1,28],[2,8,2,9],[2,10,2,11],[2,19,2,21],[2,22,2,24],[1,19,1,24]]}
[1,{"$f":"A1+1","v":2},{"$f":"B1+1","v":3},4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,{"$f":"AO1+1","v":42},43,44,45,46,47,48,49,50,51,52,53,54,55]
["Respondent","Country code","Band index","Frequency band (MHz)","Licensing regime",null,null,null," Topo-logy",null,"Application",null,null,null,null,"Number of P-P links",null,"Number of CS","Channel/Frequency plan used (e.g. ERC/ECC Rec. ITU-R Rec.)","Link characteristics",null,null,null,null,null,"Future trends (e.g. in the next 5 years)"]
[null,null,null,null,null,null,null,null,"FWA",null,"Network Infrastruc-ture",null,null,null,null,null,null,null,null,"Capacity",null,null,"Hop length (km)"]
[null,null,null,null,"Link by link","Block","Light licensed","Licence exempt","P-P","P-MP","Mobile backhaul","Others","Broadcasting Infrastructure","No Information available on the application","Other (please indicate)","unidirection","bidirectional (1 bidirectional link counts 1)","(applicable only for P-MP and mesh networks)",null,"LOW (<10 Mbit/s)","MEDIUM (10 to 100 Mbit/s)","HIGH (>100 Mbit/s)","MIN","Typical figure","MAX","Anticipated growth/reduction (+/-%)","Currently congested","Planned reallocation to other service/application","Other (please describe)\n(see Question 3 of the Questionnaire)"]
["Austria","AUT",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,null,8,null,"T/R 13-01 Annex B","x",null,null,3,20,60]
["Austria","AUT",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"T/R 13-01 Annex C"]
["Austria","AUT",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Austria","AUT",0,"3400-3600","X",null,null,null,null,"X","X",null,null,null,null,null,null,240,"ERC/REC 14-03","X",null,null,3,15,30]
["Austria","AUT",0,"3600-4200","X",null,null,null,"X",null,"X",null,null,null,null,null,90,null,"ERC/REC 12-08",null,"X",null,13,50,100]
["Austria","AUT",0,"4400-5000","X",null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Austria","AUT",0,"4400-5000"]
["Austria","AUT",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,336,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",5,45,70]
["Austria","AUT",0,"7125-7750","X",null,null,null,"X",null,null,null,null,null,null,null,570,null,"ECC REC (02)06",null,"X","X",1,40,78]
["Austria","AUT",0,"7750-7900",null,null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Austria","AUT",0,"7900-8500","X",null,null,null,"X",null,"X",null,"X",null,null,null,73,null,"ECC REC (02)06",null,"X","X",1,35,60]
["Austria","AUT",0,"10000-10680","X",null,null,null,"X",null,"X",null,null,null,null,null,158,null,"ERC/REC 12-05",null,"x",null,1,30,80]
["Austria","AUT",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,21,null,"ERC/REC 12-06"]
["Austria","AUT",0,"11700-12500"]
["Austria","AUT",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,137,null,"ERC/REC 12-02",null,null,"x",3,25,52]
["Austria","AUT",0,"14250-14500"]
["Austria","AUT",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,631,null,"ERC/REC 12-07","x","x","x",1,15,44]
["Austria","AUT",0,"21200-22000","X",null,null,null,null,null,null,null,"X",null,"mo",null,null,null,"national"]
["Austria","AUT",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,2885,null,"T/R 13-02 Annexes A1, A2, A3","x","x","x",1,10,20]
["Austria","AUT",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,2365,null,"T/R 13-02 Annex B","x","x","x",1,6,24]
["Austria","AUT",0,"24500-26500"]
["Austria","AUT",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,156,null,"T/R 13-02 Annex C",null,null,"x",1,2,4]
["Austria","AUT",0,"27500-29500"]
["Austria","AUT",0,"31800-33400"]
["Austria","AUT",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,5273,null,"T/R 12-01","x","x","x",1,5,17]
["Austria","AUT",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Bosnia and Herzegovina","BIH",0,"370-400","X",null,null,null,null,null,null,null,"X",null,null,129,null,null,null,"X",null,null,1,30,100,null,null,null,"370-400 MHz: Planned migration of P-P links to 1350-1375/1492-1517 and 1375-1400/1427-1452 MHz"]
["Bosnia and Herzegovina","BIH",0,"1350-1375 and 1492-1517","X",null,null,null,null,null,null,null,"X",null,null,48,null,null,"T/R 13-01 Annex A","X",null,null,"0.5",7,70,"+15"]
["Bosnia and Herzegovina","BIH",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,null,null,"X",null,null,5,null,null,"T/R 13-01 Annex B","X",null,null,5,20,90,"+15"]
["Bosnia and Herzegovina","BIH",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,"X",null,null,27,null,null,"T/R 13-01 Annex C","X",null,null,"1",55,99,"+10"]
["Bosnia and Herzegovina","BIH",0,"3400-3600","X",null,null,null,null,null,"X",null,"X",null,null,9,1,null,"ERC/REC 14-03 Annex B","X","X",null,null,2,null,null,null,null,"3400-3600 MHz: Only two channels are available for P-P links out of FWA systems. We still do not have active implemented FWA systems.\n3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Bosnia and Herzegovina","BIH",0,"3400-3600",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,null,null,"X","X",null,null,null,"+25",null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Bosnia and Herzegovina","BIH",0,"3600-3800","X",null,null,null,null,null,null,null,"X",null,null,9,null,null,"ERC/REC 12-08",null,"X","X",null,null,null,null,null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Bosnia and Herzegovina","BIH",0,"3600-3800",null,"X",null,null,"X","X",null,null,null,null,null,null,null,65,null,null,null,"X",null,null,null,"+25"]
["Bosnia and Herzegovina","BIH",0,"3800-4200","X",null,null,null,null,null,null,null,"X",null,null,11,3,null,"ERC/REC 12-08 Annex B",null,null,null,27,35,85,"+40"]
["Bosnia and Herzegovina","BIH",0,"5850-5925"]
["Bosnia and Herzegovina","BIH",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,5,302,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",8,60,134,null,"X"]
["Bosnia and Herzegovina","BIH",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,113,null,"ECC REC (02)06",null,"X","X",4,40,90,null,"X"]
["Bosnia and Herzegovina","BIH",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,10,62,null,"ITU-R F.385",null,"X","X"]
["Bosnia and Herzegovina","BIH",0,"7725–8275","X",null,null,null,null,null,"X",null,"X",null,null,34,143,null,"ITU-R F.386, Annex 6",null,"X","X",4,38,83,null,"X",null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Bosnia and Herzegovina","BIH",0,"8275-8500","X",null,null,null,null,null,"X",null,null,null,null,null,17,null,"ITU-R F.386, Annex 2",null,"X",null,7,25,65,null,"X"]
["Bosnia and Herzegovina","BIH",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,103,null,null,"ERC/REC 12-05","X","X",null,1,27,80,"+15",null,null,"10000-10680 MHz: Shared band between P-P links and FWA. We still do not have active implemented FWA systems."]
["Bosnia and Herzegovina","BIH",0,"10000-10680",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC 12-05 Annex A"]
["Bosnia and Herzegovina","BIH",0,"10700-11700","X",null,null,null,null,null,"X",null,"X",null,null,37,38,null,"ERC/REC 12-06","X","X",null,1,25,64,"+15",null,null,"3400-3600, 3600-3800, 7725-8275, 10700-11700 MHz: Broadcast infrastructure P-P links are planned to migrate in 3800-4200 MHz"]
["Bosnia and Herzegovina","BIH",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/DEC(00)08"]
["Bosnia and Herzegovina","BIH",0,"11700-12500",null,"X",null,null,null,null,null,null,"X",null,null,null,null,16,null,null,null,null,null,null,null,"+10"]
["Bosnia and Herzegovina","BIH",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,31,null,"ERC/REC 12-02","X","X","X",2,20,34,"+15"]
["Bosnia and Herzegovina","BIH",0,"14250-14500"]
["Bosnia and Herzegovina","BIH",0,"14400-15350","X",null,null,null,null,null,"X",null,null,null,null,null,162,null,"ITU-R F.636","X","X",null,1,15,45,null,null,null,"14400-15350 MHz: Planned leaving of ITU rec. and fully harmonization according to ERC/REC 12-07"]
["Bosnia and Herzegovina","BIH",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,278,null,"ERC/REC 12-07","X","X",null,1,15,45]
["Bosnia and Herzegovina","BIH",0,"21200-22000","X",null,null,null,null,null,"X",null,null,null,null,null,256,null,null,"X","X","X","0.5",5,20,null,null,null,"21200-22000 MHz: Planned leaving of band and full harmonization according to T/R 13-02 Annexes A1, A2, A3"]
["Bosnia and Herzegovina","BIH",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,421,null,"T/R 13-02 Annexes A1, A2, A3","X","X","X","0.5",5,20,"+20"]
["Bosnia and Herzegovina","BIH",0,"24500-26500","X","X",null,null,null,null,"X",null,null,null,null,null,3,null,"T/R 13-02 Annex B","X","X","X",1,4,6,"+35",null,null,"24500-26500, 27500-29500 MHz: Shared band between P-P links and FWA. Actually, block assignments for P-P links in process. We still do not have active implemented FWA systems."]
["Bosnia and Herzegovina","BIH",0,"24500-26500",null,"X",null,null,"X","X"]
["Bosnia and Herzegovina","BIH",0,"27500-29500","X","X",null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,"+5",null,null,"24500-26500, 27500-29500 MHz: Shared band between P-P links and FWA. Actually, block assignments for P-P links in process. We still do not have active implemented FWA "]
["Bosnia and Herzegovina","BIH",0,"27500-29500",null,"X",null,null,"X","X"]
["Bosnia and Herzegovina","BIH",0,"31800-33400"]
["Bosnia and Herzegovina","BIH",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,1,23,null,"T/R 12-01","X",null,null,"0.1",1,5,"+5"]
["Bosnia and Herzegovina","BIH",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Croatia","HRV",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Croatia","HRV",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Croatia","HRV",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,"X",null,null,182,null,null,"National plan","X",null,null,0.09,8.9,55.6]
["Croatia","HRV",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,67,"ERC/REC 14-03",null,null,null,null,null,null,-30]
["Croatia","HRV",0,"3600-4200","X",null,null,null,null,null,null,null,"X",null,null,null,9,null,"ERC/REC 12-08",null,"X"]
["Croatia","HRV",0,"3600-4200","X",null,null,null,null,null,"X",null,null,null,null,1,70,null,null,null,null,"X",20.2,44.2,91.4,10]
["Croatia","HRV",0,"5850-5925"]
["Croatia","HRV",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,98,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",10.7,34.1,70.8,20,"x"]
["Croatia","HRV",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,171,null,"Bands 7125 - 7425 and 7425 - 7725 with diff. ch. arrangements",null,"X","X",3.8,37.700000000000003,91.4,30,"x"]
["Croatia","HRV",0,"7750-7900","X",null,null,null,null,null,"X",null,"X",null,null,null,146,null,"Band 7725 - 8275",null,null,"X",21.1,50.3,91.4,null,"x"]
["Croatia","HRV",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,14,null,"Band 8275 - 8500",null,"X",null,7.5,20.100000000000001,31.4]
["Croatia","HRV",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,2,null,null,"ERC/REC 12-05",null,"x"]
["Croatia","HRV",0,"10000-10680",null,"X",null,null,null,"X"]
["Croatia","HRV",0,"10700-11700","X",null,null,null,null,null,"X",null,null,null,null,null,8,null,"ERC/REC 12-06",null,null,"x",7.5,20.2,29.8]
["Croatia","HRV",0,"11700-12500"]
["Croatia","HRV",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,244,null,"ERC/REC 12-02",null,"x",null,1.5,19.2,49.2,20,"x"]
["Croatia","HRV",0,"12750-13250","X",null,null,null,null,null,null,null,"X",null,null,1]
["Croatia","HRV",0,"14250-14500"]
["Croatia","HRV",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,"X",null,null,20,null,null,"ERC/REC 12-07",null,null,null,0.6,9.9,22.7]
["Croatia","HRV",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,1220,null,"T/R 13-02 Annexes A1, A2, A3",null,"x",null,0.18,5.5,21.1,10]
["Croatia","HRV",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Croatia","HRV",0,"24500-26500"]
["Croatia","HRV",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Croatia","HRV",0,"27500-29500"]
["Croatia","HRV",0,"31800-33400"]
["Croatia","HRV",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,335,null,"T/R 12-01",null,"x",null,7.0000000000000007E-2,0.42,4.9000000000000004,20]
["Croatia","HRV",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Cyprus","CYP",0,"1350-1375 and 1492-1517","X",null,null,null," ",null,null,null,"X",null,null,13,null,null,"T/R 13-01 Annex A","X",null,null,0.9,null,58.65]
["Cyprus","CYP",0,"1350-1375 and 1492-1517","X",null,null,null," ",null,null,null,"X",null,null,17,null,null,null,"X",null,null,0.9,null,73.55]
["Cyprus","CYP",0,"1375-1400 and 1427-1452","X",null,null,null," ",null,null,null,"X",null,null,6,null,null,"T/R 13-01 Annex B","X",null,null,3.52,null,35.47]
["Cyprus","CYP",0,"1375-1400 and 1427-1452","X",null,null,null," ",null,null,null,"X",null,null,8,null,null,null,"X",null,null,22.62,null,74.209999999999994]
["Cyprus","CYP",0,"2025-2110 and 2200-2290",null,null,null," ",null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,"X"]
["Cyprus","CYP",0,"3400-3600","P.C.",null,null,null,null,null,null,null,null,null,null,null,null,null,"2008/411/EC"]
["Cyprus","CYP",0,"3600-4200","P.C. (3.6-3.8 GHz)",null,null,null,null,null,null,null,null,null,null,null,null,null,"2008/411/EC"]
["Cyprus","CYP",0,"4400-5000",null,null,null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X"]
["Cyprus","CYP",0,"4400-5000"]
["Cyprus","CYP",0,"5850-5925","X",null,null,null,null,null,null,null,"X",null,null,2,null,null,null,null,"X"," ","PORTABLE"]
["Cyprus","CYP",0,"5925-7125","X",null,null,null,null,null,"X",null,"X",null,null,17,27,null,"ERC/REC 14-01 and ERC/REC 14-02","X","X"," ",7.19,null,53]
["Cyprus","CYP",0,"7125-7750","X",null,null,null,null,null,"X",null,"x",null,null,8,48,null,"ECC REC (02)06","X","X"," ",0.49,null,63.77]
["Cyprus","CYP",0,"7750-7900",null,null,null," "]
["Cyprus","CYP",0,"7900-8500","X",null,null,null,null,null,null,null,"X",null,null,14,null,null,"ECC REC (02)06","X","X"," ",8.2899999999999991,null,40.020000000000003]
["Cyprus","CYP",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,56,null,null,"ERC/REC 12-05","X","X"," ",0.53,null,70]
["Cyprus","CYP",0,"10700-11700","X",null,null,null,null,null,"X",null,"X",null,null,3,30,null,"ERC/REC 12-06",null,"X"," ",2.0099999999999998,null,34.130000000000003]
["Cyprus","CYP",0,"11700-12500","X",null,null,null,null,null,null,null,"X",null,null,10,null,null,null,null,"X"," ",2.75,null,30.18]
["Cyprus","CYP",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,278,null,"ERC/REC 12-02","X","X"," ",0.28999999999999998,null,40.94,null,"X"]
["Cyprus","CYP",0,"14250-14500","X",null,null,null,null,null,null,null,"X",null,null,14,null,null,"ERC/REC 13-03",null,"X"," ",8.2899999999999991,null,36.46]
["Cyprus","CYP",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,"X",null,null,12,null,null,"ERC/REC 12-07",null,"X",null,0.45,null,38.17]
["Cyprus","CYP",0,"21200-22000","X",null,null,null,null,null,"X",null,null,null,null,null,97,null,null,"X","X"," ",0.2,null,18.27,null,"X"]
["Cyprus","CYP",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,738,null,"T/R 13-02 Annexes A1, A2, A3","X","X"," ",0.25,null,15.16,null,"X"]
["Cyprus","CYP",0,"22600-23000","X",null,null,null,null,null,"X",null,null,null,null,37,null,null,"National","X","X"," ",0.2,null,18.14,null,null,"X"]
["Cyprus","CYP",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Cyprus","CYP",0,"24500-26500"]
["Cyprus","CYP",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Cyprus","CYP",0,"27500-29500"]
["Cyprus","CYP",0,"31800-33400"]
["Cyprus","CYP",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 12-01"]
["Cyprus","CYP",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Czech Republic","CZE",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"T/R 13-01 Annex A"]
["Czech Republic","CZE",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"T/R 13-01 Annex B"]
["Czech Republic","CZE",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X",null,null,null,null,"MD shared",null,null,110,"T/R 13-01 Annex C",null,null,null,null,null,null,0]
["Czech Republic","CZE",0,"3400-3600","X","X",null,null,"X","X",null,null,null,null,null,null,null,667,"ERC/REC 14-03",null,null,null,null,null,null,100,null,null,"P-MP, FWA planned"]
["Czech Republic","CZE",0,"3600-3800","X",null,null,null,"X",null,null,null,null,null,null,null,150,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,"X","DEC EC/411/EC"]
["Czech Republic","CZE",0,"3800-4200","X",null,null,null,"X",null,null,null,null,null,null,null,479,null,"ERC/REC 12-08"]
["Czech Republic","CZE",0,"4400-5000",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,null,null,null,null,null,null,null,null,null,null,"civil/MD sharing"]
["Czech Republic","CZE",0,"4400-5000"]
["Czech Republic","CZE",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,null,null,null,null,null,null,null,null,null,null,"civil/MD sharing"]
["Czech Republic","CZE",0,"5925-7125","X",null,null,null,"X",null,null,null,null,null,null,null,1642,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Czech Republic","CZE",0,"7125-7750","X",null,null,null,"X",null,null,null,null,null,null,null,1050,null,"ECC REC (02)06",null,null,null,null,null,null,null,null,"x","civil/MD sharing"]
["Czech Republic","CZE",0,"7750-7900",null,null,null,null,null,null,null,null,null,null,"MD"]
["Czech Republic","CZE",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"ECC REC (02)06"]
["Czech Republic","CZE",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,"MD",null,null,null,"ERC/REC 12-05"]
["Czech Republic","CZE",0,"10000-10680","X",null,null,"X","X",null,null,null,null,null,null,null,21]
["Czech Republic","CZE",0,"10700-11700","X",null,null,null,null,"X",null,null,null,null,null,null,null,1845,"ERC/REC 12-06",null,null,null,null,null,null,20]
["Czech Republic","CZE",0,"11700-12500","X",null,null,null,"X",null,null,null,null,null,null,31,null,null,null,null,null,null,null,null,null,10]
["Czech Republic","CZE",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,1288,null,"ERC/REC 12-02",null,null,null,null,null,null,10]
["Czech Republic","CZE",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"sat. services planned"]
["Czech Republic","CZE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,20,null,"ERC/REC 12-07"]
["Czech Republic","CZE",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FS considered"]
["Czech Republic","CZE",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,3707,null,"T/R 13-02 Annexes A1, A2, A3",null,null,null,null,null,null,5]
["Czech Republic","CZE",0,"22600-22700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ENG/OB"]
["Czech Republic","CZE",0,"22700-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no utilisation"]
["Czech Republic","CZE",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAB"]
["Czech Republic","CZE",0,"24500-24745/25500-25753",null,"X",null,null,null,"X",null,null,null,null,null,null,null,133,"T/R 13-02 Annex B",null,null,null,null,null,null,10]
["Czech Republic","CZE",0,"24745-25500/25753-26500","X",null,null,null,"X",null,null,null,null,null,null,null,4537,null,null,null,null,null,null,null,null,10]
["Czech Republic","CZE",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,"MD"]
["Czech Republic","CZE",0,"26500-27500"]
["Czech Republic","CZE",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,41,"T/R 13-02 Annex C"]
["Czech Republic","CZE",0,"27500-29500","X","X",null,null,"X","X",null,null,null,null,null,null,189]
["Czech Republic","CZE",0,"31000-31300","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,5]
["Czech Republic","CZE",0,"31800-33400","X",null,null,null,"X",null,null,null,null,null,null,null,50,null,"ERC/REC/(01)02",null,null,null,null,null,null,50]
["Czech Republic","CZE",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,5603,null,"T/R 12-01",null,null,null,null,null,null,5]
["Czech Republic","CZE",0,"40500-43500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"yes",null,null,"P-P and P-MP planned"]
["Czech Republic","CZE",0,"47200-48500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["Czech Republic","CZE",0,"48500-50200","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["Czech Republic","CZE",0,"50400-51400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["Czech Republic","CZE",0,"51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["Czech Republic","CZE",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"incr. of utilisation expected"]
["Czech Republic","CZE",0,"57000-59000","X",null,null,null,"X",null,null,null,null,null,null,null,3,null,"ECC/REC/(09)01",null,null,null,null,null,null,"yes"]
["Czech Republic","CZE",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,"MD shared",null,null,null,"ECC/REC/(09)01"]
["Czech Republic","CZE",0,"71000-76000 and  81000-86000",null,null,null,"X","X",null,null,null,null,null,null,null,57,null,"ECC/REC/(05)07",null,null,null,null,null,null,100]
["Czech Republic","CZE",0,"92000-95000","X",null,null,null,"X",null,null,null,null,null,null,null,3]
["Denmark","DNK",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Denmark","DNK",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Denmark","DNK",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Denmark","DNK",0,"3400-3600","X",null,null,null,null,null,null,null,null,null,null,null,null,29,"ERC/REC 14-03"]
["Denmark","DNK",0,"3400-3600",null,"X",null,null,null,null,null,null,null,null,null,null,null,null," ",null,null,null,null,null,null,null,null,null,"No info"]
["Denmark","DNK",0,"3600-4200","X",null,null,null,null,null,null,null,null,null,null,null,null,21,"ERC/REC 12-08"]
["Denmark","DNK",0,"3600-4200",null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No info"]
["Denmark","DNK",0,"5850-5925"]
["Denmark","DNK",0,"5925-7125","X",null,null,null,null,null,null,null,null,null,null,null,22,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Denmark","DNK",0,"7125-7750","X",null,null,null,null,null,null,null,null,null,null,null,225,null,"ECC REC (02)06",null,null,null,20]
["Denmark","DNK",0,"7750-7900"]
["Denmark","DNK",0,"7900-8500","X",null,null,null,null,null,null,null,null,null,null,null,4," ","ECC REC (02)06",null,null,null,20]
["Denmark","DNK",0,"10000-10680","X",null,null,null,null,null,null,null,null,null,null,null,null,47,"ERC/REC 12-05"]
["Denmark","DNK",0,"10000-10680",null,"X",null,null,null,null,null,null,null,null,null,null,"No info"]
["Denmark","DNK",0,"10000-10680","X",null,null,null,null,null,null,null,null,null,null,null,1]
["Denmark","DNK",0,"10700-11700","X",null,null,null,null,null,null,null,null,null,null,null,null,1,"ERC/REC 12-06"]
["Denmark","DNK",0,"11700-12500"]
["Denmark","DNK",0,"12750-13250","X",null,null,null,null,null,null,null,null,null,null,null,4,null,"ERC/REC 12-02",null,null,null,12]
["Denmark","DNK",0,"14250-14500"]
["Denmark","DNK",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,null,null,null,null,299,null,"ERC/REC 12-07",null,null,null,12]
["Denmark","DNK",0,"22000-22600 and 23000-23600",null,"X",null,null,null,null,null,null,null,null,null,null,"No info",null,"T/R 13-02 Annexes A1, A2, A3"]
["Denmark","DNK",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,null,null,null,650]
["Denmark","DNK",0,"22600-23000","X",null,null,null,null,null,null,null,null,null,null,null,1]
["Denmark","DNK",0,"24250-24500","X",null,null,null,null,null,null,null,null,null,null,null,1]
["Denmark","DNK",0,"24500-26500",null,"X",null,null,null,null,null,null,null,null,null,null,null,"No info","T/R 13-02 Annex B"]
["Denmark","DNK",0,"24500-26500","X",null,null,null,null,null,null,null,null,null,null,null,null,135]
["Denmark","DNK",0,"27500-29500","X",null,null,null,null,null,null,null,null,null,null,null,null,18,"T/R 13-02 Annex C"]
["Denmark","DNK",0,"27500-29500"]
["Denmark","DNK",0,"31800-33400",null,"X",null,null,null,null,null,null,null,null,null,null,"No info",null,"ERC/REC/(01)02"]
["Denmark","DNK",0,"37000-39500","X",null,null,null,null,null,null,null,null,null,null,null,158,null,"T/R 12-01"]
["Denmark","DNK",0,"37000-39500",null,"X",null,null,null,null,null,null,null,null,null,null,"No info"]
["Denmark","DNK",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Denmark","DNK",0,"50400-51400","X",null,null,null,null,null,null,null,null,null,null,null,1]
["Estonia","EST",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Estonia","EST",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Estonia","EST",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Estonia","EST",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,null,null,null,"No info"]
["Estonia","EST",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"No info"]
["Estonia","EST",0,"5850-5925"]
["Estonia","EST",0,"5925-7125",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Estonia","EST",0,"7125-7750",null,null,null,null,null,null,null,null,null,null,null,null,62,null,"ECC REC (02)06",null,62,null,17,35,81]
["Estonia","EST",0,"7750-7900"]
["Estonia","EST",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,45,null,"ECC REC (02)06",null,45,null,15,35,40,"+20"]
["Estonia","EST",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Estonia","EST",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Estonia","EST",0,"11700-12500"]
["Estonia","EST",0,"12750-13250",null,null,null,null,null,null,null,null,null,null,null,null,80,null,"ERC/REC 12-02",null,80,null,11,22,34]
["Estonia","EST",0,"14250-14500"]
["Estonia","EST",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,60,null,"ERC/REC 12-07",null,60,null,12,23,33,"- 5"]
["Estonia","EST",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,788,null,"T/R 13-02 Annexes A1, A2, A3",null,788,null,3,14,24,"+25"]
["Estonia","EST",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Estonia","EST",0,"24500-26500"]
["Estonia","EST",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Estonia","EST",0,"27500-29500"]
["Estonia","EST",0,"31800-33400"]
["Estonia","EST",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,232,null,"T/R 12-01",169,63,null,0.7,5,10,"+10"]
["Estonia","EST",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Finland","FIN",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A",null,null,null,null,null,null,null,null,null,"Planned opening 2011-2012"]
["Finland","FIN",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,"X",null,null,null,null,null,4,null,"T/R 13-01 Annex B","X","X",null,null,null,null,null,null,null,"Planned closing 2011-2012"]
["Finland","FIN",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,"X",null,null,null,null,null,12,null,"T/R 13-01 Annex C","X","X"]
["Finland","FIN",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,540,"ERC/REC 14-03"]
["Finland","FIN",0,"3600-4200","X",null,null,null,null,null,"X",null,"X",null,null,null,160,null,"ERC/REC 12-08",null,null,"X"]
["Finland","FIN",0,"3600-4200",null,null,null,null,null,null,null,null,"X",null,null,40,null,null,"National","Analog","Analog",null,null,null,null,null,null,null,"Will be phased out"]
["Finland","FIN",0,"3600-4200","X",null,null,null,null,null,null,null,"X",null,null,120,null,null,"ITU-R F.382","Analog","Analog",null,null,null,null,null,null,null,"Will be phased out"]
["Finland","FIN",0,"5850-5925"]
["Finland","FIN",0,"5925-7125","X",null,null,null,null,null,"X",null,"X",null,null,null,160,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",10,30,63,0.8]
["Finland","FIN",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,130,null,"ITU-R F.385",null,"X","X",13,36,65,0.05]
["Finland","FIN",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,330,null,"National (ITU-R F.385 mod.)",null,"X","X",2,27,70,0.1]
["Finland","FIN",0,"7750-7900","X",null,null,null,null,null,null,null,"X",null,null,45,7,null,"National  ",null,"X"]
["Finland","FIN",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["Finland","FIN",0,"10000-10680","X",null,null,null,null,"X",null,null,null,null,null,null,null,11,"ERC/REC 12-05",null,"X"]
["Finland","FIN",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Finland","FIN",0,"11700-12500"]
["Finland","FIN",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,2120,null,"ERC/REC 12-02",null,"X","X",0.4,14,49,0.2,"x",null,"Local congestion"]
["Finland","FIN",0,"14250-14500"]
["Finland","FIN",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07"]
["Finland","FIN",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,1950,null,"ITU-R F.636",null,"X",null,0.1,8.6999999999999993,10.9,-0.15]
["Finland","FIN",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,2770,null,"T/R 13-02 Annexes A1, A2, A3",null,"X","X",0.1,4.5999999999999996,19,0.15,"x",null,"Local congestion"]
["Finland","FIN",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex B"]
["Finland","FIN",0,"24500-26500"]
["Finland","FIN",0,"27500-29500","X",null,null,null,null,null,"X",null,null,null,null,null,380,null,"T/R 13-02 Annex C",null,"X","X",0.1,1.1000000000000001,7.2,0.9,"x",null,"Local congestion"]
["Finland","FIN",0,"27500-29500"]
["Finland","FIN",0,"31800-33400","X",null,null,null,null,null,"X",null,null,null,null,null,1,null,"ERC/REC/(01)02",null,"X","X",null,null,null,100]
["Finland","FIN",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,45,null,"T/R 12-01",null,"X","X",0.2,1.7,6.1,0.1]
["Finland","FIN",0,"40500-43500","X",null,null,null,null,null,"X",null,null,null,null,null,null,null,"ECC/REC/(01)04",null,"X","X",null,null,null,null,null,null,"Opens 2011"]
["France","FRA",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["France","FRA",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,null,1259,null,"T/R 13-01 Annex B",1259,null,null,0.1,null,95,"+ 10 %"]
["France","FRA",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["France","FRA",0,"3400-3600","X","X",null,null,"X","X","X",null,null,null,null,null,236,1135,"ERC/REC 14-03",236,null,null,2,"20<x>80",135,"-30"]
["France","FRA",0,"3600-4200","X",null,null,null,"X",null,"X",null,null,null,null,null,11,null,"ERC/REC 12-08",null,null,11,2,"20<x>80",135,"-20"]
["France","FRA",0,"5850-5925"]
["France","FRA",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,3491,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,3491,0.5,"20-80",105,"+ 5 % ","X"]
["France","FRA",0,"7125-7750",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["France","FRA",0,"7750-7900"]
["France","FRA",0,"7900-8500","X",null,null,null,"X",null,"X",null,null,null,null,null,2529,null,"ECC REC (02)06",1322,947,260,0.04,"15<x>60",105,"- 10 %"]
["France","FRA",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UIT-RF-386-4"]
["France","FRA",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["France","FRA",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,524,null,"ERC/REC 12-06",null,null,524,1.5,"15<x>50",46,"+ 26 %"]
["France","FRA",0,"11700-12500"]
["France","FRA",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,6613,null,"ERC/REC 12-02",2401,3711,501,0.1,"5<x>35",103,"+ 2 %","X"]
["France","FRA",0,"14250-14500","X",null,null,null,"X",null,"X",null,null,null,null,null,374,null,null,374,null,null,10,"5<x>35",100,"-5%"]
["France","FRA",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07"]
["France","FRA",0,"22000-22600 and 23000-23600","X","X",null,null,"X",null,"X",null,null,null,null,null,12195,null,"T/R 13-02 Annexes A1, A2, A3",4614,7498,83,0.1,"3<x>20",32,"+ 9 %"]
["France","FRA",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IUT-RF 637-3"]
["France","FRA",0,"22600-23000","X",null,null,null,"X",null,"X",null,null,null,null,null,124,null,null,124,null,null,0.1,10,32,"+ 1%"]
["France","FRA",0,"24500-26500","X","X",null,null,"X","X","X",null,null,null,null,null,215,75,"T/R 13-02 Annex B",null,88,127,0.12,"3<x>20",15,"+ 3 %"]
["France","FRA",0,"24500-26500"]
["France","FRA",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["France","FRA",0,"27500-29500"]
["France","FRA",0,"31800-33400","X","X",null,null,"X",null,"X",null,null,null,null,null,null,null,"ERC/REC/(01)02"]
["France","FRA",0,"37000-39500","X","X",null,null,"X",null,"X",null,null,null,null,null,8304,null,"T/R 12-01",2223,6057,24,0.1,"0<x>6",15,"+8%"]
["France","FRA",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["France","FRA",0,"71000-76000 and  81000-86000","X",null,null,null,"X",null,"X",null,null,null,null,null,0,null,"ECC/REC/(05)07"]
["Germany","GER",0,"3400-3600",null,"x",null,null,null,"x",null,null,null,null,null,null,null,392,"ERC/REC 14-03",null,"x"]
["Germany","GER",0,"3600-3800",null,"x",null,null,null,"x",null,null,null,null,null,null,null,0,"ERC/REC 14-03",null,"x"]
["Germany","GER",0,"3800-4200","x",null,null,null,"x",null,null,null,null,null,null,269,null,null,"ERC/REC 12-08",null,null,"x",14.4,42,64.8]
["Germany","GER",0,"5925-6425","x",null,null,null,"x",null,null,null,null,null,null,994,null,null,"ERC/REC 14-01",null,null,"x",11.1,40,67.3]
["Germany","GER",0,"6425-7125","x",null,null,null,"x",null,null,null,null,null,null,2565,null,null,"ERC/REC 14-02",null,null,"x",4.3,30,103.9]
["Germany","GER",0,"7125-7425","x",null,null,null,"x",null,null,null,null,null,null,917,null,null,"ECC REC (02)06",null,"x",null,4.2,28,89.9]
["Germany","GER",0,"7425-7725","x",null,null,null,"x",null,null,null,null,null,null,3157,null,null,"ECC REC (02)06",null,null,"x",5.5,26,71.099999999999994,null,"x"]
["Germany","GER",0,"12750-13250","x",null,null,null,"x",null,null,null,null,null,null,4100,null,null,"ERC/REC 12-02",null,null,"x",0.99,12,48.5]
["Germany","GER",0,"14500-14620 and 15230-15350","x",null,null,null,"x",null,null,null,null,null,null,10235,null,null,"ERC/REC 12-07",null,"x",null,2.25,14,54.5,null,"x"]
["Germany","GER",0,"22000-22600 and 23000-23600","x",null,null,null,"x",null,null,null,null,null,null,19401,null,null,"ERC/REC 13-02 ",null,"x",null,0.13,8,51.1]
["Germany","GER",0,"24500-26500","x",null,null,null,"x","x",null,null,null,null,null,15880,null,null,"ERC/REC 13-02 ",null,"x",null,0.1,4,10.9]
["Germany","GER",0,"24500-26500",null,"x",null,null,null,null,null,null,null,null,null,null,null,836]
["Germany","GER",0,"27500-29500",null,"x",null,null,"x","x",null,null,null,null,null,1424,null,29,"ERC/REC 13-02 ",null,null,null,0.18,3,13.3]
["Germany","GER",0,"31000-31300",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,"x",null,null,null,null,null,null,null,"not open"]
["Germany","GER",0,"31800-33400","x",null,null,null,"x",null,null,null,null,null,null,1466,null,null,"ERC/REC/(01)02",null,"x",null,0.1,2.2999999999999998,6.8,20]
["Germany","GER",0,"37000-39500","x",null,null,null,"x",null,null,null,null,null,null,30594,null,null,"ERC/REC 12-01 ",null,"x",null,0.02,2.2999999999999998,13.2]
["Germany","GER",0,"40500-43500","x",null,null,null,"x",null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,"x",null,null,null,null,null,null,"will be opened 2011"]
["Germany","GER",0,"51400-52600","x",null,null,null,"x",null,null,null,null,null,null,null,null,0,"ERC/REC 12-11",null,"x"]
["Germany","GER",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,0,"ERC/REC 12-12",null,"x",null,null,null,null,null,null,null,"not open"]
["Germany","GER",0,"57100-58900",null,null,null,"x","x",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01","x"]
["Germany","GER",0,"59000-63000",null,null,null,"x","x",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,"x"]
["Germany","GER",0,"71000-76000 and  81000-86000","x",null,null,null,"x",null,null,null,null,null,null,null,null,0,"ECC/REC/(05)07",null,null,"x"]
["Greece","GRC",0,"1700-1710 and 1785-1800","X",null,null,null,null,null,null,null,"X",null,null,615,null,null,"national plan","X","X",null,0.4,14,90,null,"congested in urban areas"]
["Greece","GRC",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,"X",null,null,null,null,null,206,null,"T/R 13-01 Annex C","X","X",null,0.6,21,60,"reduction"]
["Greece","GRC",0,"3400-3600",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC 14-03","-",null,null,null,null,null,"4 issued licenses"]
["Greece","GRC",0,"3800-4200","X",null,null,null,null,null,"X",null,null,null,null,null,163,null,"ERC/REC 12-08 Annex B",null,"X","X",5,55,101,"reduction"]
["Greece","GRC",0,"5850-5925"]
["Greece","GRC",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,638,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",8,45,102,"stable"]
["Greece","GRC",0,"7425-7725","X",null,null,null,null,null,"X",null,null,null,null,null,1222,null,"ECC REC (02)06 Annex1","X","X","X",1,31,98,0.1]
["Greece","GRC",0,"7725–8275","X",null,null,null,null,null,"X",null,null,null,null,null,1157,null,"ITU-R F. 386-6 Annex 1",null,"X","X",2,40,150,0.1]
["Greece","GRC",0,"8275-8500 ","X",null,null,null,null,null,"X",null,null,null,null,null,170,null,"ITU-R F. 386-6 Annex 3","X","X",null,1.8,47,120,"stable"]
["Greece","GRC",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,107,null,null,"national plan",null,null,null,1.2,19,75]
["Greece","GRC",0,"10700-11700","X",null,null,null,null,null,"X",null,null,null,null,null,785,null,"ERC/REC 12-06",null,null,"X",1.7,19,63,0.3]
["Greece","GRC",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Greece","GRC",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,1004,null,"ERC/REC 12-02","X","X","X",1.5,16,55,0.5]
["Greece","GRC",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Greece","GRC",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,2863,null,"ERC/REC 12-07","X","X","X",0.5,15,75,0.5,"heavily used"]
["Greece","GRC",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Greece","GRC",0,"21200-22000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Use"]
["Greece","GRC",0,"22000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,1724,null,"T/R 13-02 Annex A","X","X","X","0.04",4,16,0.4]
["Greece","GRC",0,"22600-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,"No current FS use.\nAllocation for analogue links. SAP/SAB, ENG/OB"]
["Greece","GRC",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC REP 38",null,null,null,null,null,null,"-",null,null,"No current use.\nAllocation for analogue links. SAP/SAB, ENG/OB"]
["Greece","GRC",0,"24500-26500",null,"X",null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC 13-02","-",null,null,null,null,null,"-",null,null,"5 issued licenses"]
["Greece","GRC",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Greece","GRC",0,"27500-29500",null,null,null,null,"X","X",null,null,null,null,null,null,null,null,"ECC/DEC/(05)01","no current use",null,null,null,null,null,"-",null,null,"27828,5-27940,5 and 27940,5-28444,5 MHz paired with 28948,5-29452,5 new row by EETT allocated to digital P-P and P-MP links"]
["Greece","GRC",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No use"]
["Greece","GRC",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,984,null,"T/R 12-01",null,"X","X","0.05","1.5","6.8",0.2]
["Greece","GRC",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Use"]
["Greece","GRC",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12 Annex 3",null,null,null,null,null,null,"Maximum PFD=-26dBW/MHz",null,null,"No current use. Allocation for digital P-P links"]
["Greece","GRC",0,"57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-09 Annex A",null,null,null,null,null,null,"Radio Frequency Rights of Use not required. Maximum EIRP=15dBW",null,null,"No current use. Allocation for digital P-P links"]
["Greece","GRC",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"No current use. Allocation for digital P-P links"]
["Hungary","HUN",0,"1350-1375 and 1492-1517","X",null,null,null,"X","X","X",null,null,null,"Non-Civil P-P, P-MP systems",null,null,null,"T/R 13-01 Annex A",null,null,null,null,null,null,0.1]
["Hungary","HUN",0,"1375-1400 and 1427-1452","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"T/R 13-01 Annex B","X",null,null,null,20,null,0.1]
["Hungary","HUN",0,"1375-1400 and 1427-1452","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"X",null,null,null,20]
["Hungary","HUN",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,"2070-2110 and 2245-2290 MHz Non-Civil digital P-P links",null,3,null,"T/R 13-01 Annex C","X","X",null,null,20]
["Hungary","HUN",0,"3400-3600",null," ",null," ",null," ",null,null,null,null,null,null,null,null,"ERC/REC 14-03"]
["Hungary","HUN",0,"3400-3600",null,"X",null,"X",null,"X",null,null,null,null,null,null,null,383,"ECC/DEC/(07)02",null,null,null,null,null,null,"20"]
["Hungary","HUN",0,"3600-4200","X"," ",null," ","X",null,null,null,null,null,null,null,20,null,"ERC/REC 12-08",null,null,"X",null,30,null,"25"]
["Hungary","HUN",0,"3600-4200"]
["Hungary","HUN",0,"4400-5000","X",null,null,null,"X","X",null,null,null,null,"Harmonized NATO band type 1. Land military systems, Tactical Radio Relay",null,140,null,null,"X","X","X",null,null,null,null,null,null,"non-civil usage"]
["Hungary","HUN",0,"4400-5000"]
["Hungary","HUN",0,"5850-5925","X",null,null,null,"X","X","X",null,null,null,"Non-Civil BFWA systems",null,null,null,"ECC/DEC/(06)04"]
["Hungary","HUN",0,"5850-5925","X",null,null,null,"X"]
["Hungary","HUN",0,"5925-7125","X",null,null,null,"X",null,null,null,null,null,null,null,299,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,null,null,null,null,0.1]
["Hungary","HUN",0,"7125-7750","X",null,null,null,"X",null,null,null,"X",null,"7125-7250 MHz Non-Civil P-P links;  7125-7425 MHz Emergency Services\n7425-7725 MHz Civil P-P links 7725-7750 MHz Civil broadcasting infrastructure",null,171,null,"ECC REC (02)06","X","X","X",null,20]
["Hungary","HUN",0,"7125-7750",null,null,null,null,null,null,null,null,null,null,"7250-7750 MHz Satellite Systems downlink (military); Harmonized NATO band type 1."]
["Hungary","HUN",0,"7750-7900","X",null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,40,null,0.15]
["Hungary","HUN",0,"7900-8500","X",null,null,null,null,null,null,null,null,null,"7900-8400 MHz Satellite Systems uplink (military); Harmonized NATO band type 1.",null,null,null,"ECC REC (02)06"]
["Hungary","HUN",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,3,null,null,"X","X",null,null,20]
["Hungary","HUN",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,93,null,null,"ERC/REC 12-05",null,null,null,null,40]
["Hungary","HUN",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Hungary","HUN",0,"10700-11700","X",null,null,null,"X",null,null,null,null,null,null,null,186,null,"ERC/DEC/(00)08",null,null,"X",null,14]
["Hungary","HUN",0,"11700-12500",null,null,null,"X",null,null,null,null,"X",null,null,null,null,144,null,null,null,null,null,null,null,null,"x"]
["Hungary","HUN",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,1710,null,"ERC/REC 12-02",null,"X",null,null,12,null,null,"x"]
["Hungary","HUN",0,"14250-14500"]
["Hungary","HUN",0,"14500-14620 and 15230-15350"," ",null,null,null," ",null,null,null,null,null,null,null," ",null,"ERC/REC 12-07",null,null,null,null," "]
["Hungary","HUN",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,"15230-15350 MHz Non-Civil Digital P-P links",null,120,null,null,"X","X",null,null," ",null,null,"x",null,"non-civil usage"]
["Hungary","HUN",0,"21200-22000","X",null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,40,null,null,"X"]
["Hungary","HUN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,"22442-22600 MHz Emergency Services Digital P-P links",null,40,null,"T/R 13-02 Annexes A1, A2, A3","X","X",null,null,null,null,null,"x"]
["Hungary","HUN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,"23450-23600 MHz Emergency services Digital P-P links",null,3512,null,"T/R 13-02 Annexes A1, A2, A3","X","X",null,null,null,null,null,"x"]
["Hungary","HUN",0,"22600-23000","X",null,null,null,null,null,null,null,"X",null,null,1,null,null,null,null,null,null,null,40,null,null,"x"]
["Hungary","HUN",0,"24250-24500","X","X",null,null,"X","X",null,null,null,null,null,null,41,31,null,"X","X","X",null,7,null,0.25,"x",null,"ù"]
["Hungary","HUN",0,"24500-26500","X","X",null,null,"X","X",null,null,null,null,null,null,83,31,"T/R 13-02 Annex B","X","X","X",null,7,null,0.25,"x",null,"PMP systems"]
["Hungary","HUN",0,"24500-26500"]
["Hungary","HUN",0,"26500-27500",null,null,null,null,"X",null,null,null,null,null,"Land military systems. P-P links Harmonized NATO band type 2.(planned)",null,null,null,null,null,null,null,null,null,null,null,"X"]
["Hungary","HUN",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Hungary","HUN",0,"27500-29500"]
["Hungary","HUN",0,"31000-31300","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02","X","X","X",null,5,null,null,"x",null,"FDD mode PP systems"]
["Hungary","HUN",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,"x"]
["Hungary","HUN",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(04)06",null,null,null,null,null,null,null,"x"]
["Hungary","HUN",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,6454,null,"T/R 12-01","X","X","X",null,4]
["Hungary","HUN",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,"37926-38178 and 39186-39500 MHz Non-Civil P-P links.   39186-39500 MHz Emergency services. 37-39.5 GHz NJFA military requirement for existing and future fixed systems.",null,100,null,"ERC/DEC/(00)02","X","X","X"]
["Hungary","HUN",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Hungary","HUN",0,"48500-50200",null,null,null,null,"X",null,null,null,null,null,"Non-Civil Digital P-P links",null,null,null,"ERC/REC 12-10"]
["Hungary","HUN",0,"51400-52600","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,null,null,"30 original value"]
["Hungary","HUN",0,"55780-57000","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,30]
["Hungary","HUN",0,"57000-59000","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,null,null,"25 original"]
["Hungary","HUN",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,"59000-61000 MHz Harmonized NATO band type 2. (planned for P-P)",null,null,null,"ECC/REC/(09)01"]
["Hungary","HUN",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,"71000-74000 and 81000-84000 MHz Common Civil and Non-Civil band for P-P links",null,null,null,"ECC/REC/(05)07"]
["Hungary","HUN",0,"92000-95000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5.149"]
["Iceland","ICE",0,"1350-1375 and 1492-1517","x",null,null,null,"X",null,null,null,null,null,null,null,0,null,"T/R 13-01 Annex A",null,null,null,null,null,null,0]
["Iceland","ICE",0,"1375-1400 and 1427-1452","x",null,null,null,"X",null,null,null,null,null,null,null,2,null,"T/R 13-01 Annex B",null,null,null,null,25,null,0]
["Iceland","ICE",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,null,null,90,null,"T/R 13-01 Annex C",45,45,null,20,40,70,0]
["Iceland","ICE",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,20,"ERC/REC 14-03",null,null,null,null,10]
["Iceland","ICE",0,"3600-4200","X",null,null,null,"X",null,null,null,null,null,null,null,7,null,"ERC/REC 12-08",null,null,7,20,30,40,0]
["Iceland","ICE",0,"5850-5925"]
["Iceland","ICE",0,"5925-7125","X",null,null,null,"X",null,null,null,"X",null,null,6,16,null,"ERC/REC 14-01 and ERC/REC 14-02",3,null,15,10,30,50,0]
["Iceland","ICE",0,"7125-7750","X",null,null,null,"X",null,null,null,"X",null,null,23,65,null,"ECC REC (02)06",32,28,28,10,30,60,0]
["Iceland","ICE",0,"7750-7900"]
["Iceland","ICE",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["Iceland","ICE",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Iceland","ICE",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Iceland","ICE",0,"11700-12500"]
["Iceland","ICE",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,12,null,"ERC/REC 12-02",null,6,6,10,20,30,0]
["Iceland","ICE",0,"14250-14500"]
["Iceland","ICE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,120,null,"ERC/REC 12-07",57,57,6,5,15,25,25]
["Iceland","ICE",0,"17700-19700","X",null,null,null,"X",null,null,null,null,null,null,null,60,null,"ERC/REC 12-03",40,10,10,10,15,20,25]
["Iceland","ICE",0,"22000-22600 and 23000-23600","X",null,null,null,"x",null,null,null,null,null,null,null,18,null,"T/R 13-02 Annexes A1, A2, A3",5,11,2,1,6,25,25]
["Iceland","ICE",0,"24500-26500","X",null,null,null,"x",null,null,null,null,null,null,null,2,null,"T/R 13-02 Annex B",null,null,2,12,15,18,10]
["Iceland","ICE",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Iceland","ICE",0,"31800-33400"]
["Iceland","ICE",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,1,null,"T/R 12-01",1,null,null,null,5]
["Iceland","ICE",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Ireland","IRL",0,"1350-1375 and 1492-1517"," X",null,null,null,null,null," X",null,null,null,null,0,69,null,"T/R 13-01 Annex A"," X","X","X",0.02,23,83,48,null," X"]
["Ireland","IRL",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009 "]
["Ireland","IRL",0,"1375-1400 and 1427-1452"," X",null,null,null,null,null," X",null,null,null,null,37,18,null,"T/R 13-01 Annex B"," X",null,null,0.45,23,69," 0",null," X"]
["Ireland","IRL",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009 "]
["Ireland","IRL",0,"2025-2110 and 2200-2290","X",null,null,null,null,null," X",null,null,null,null,null,47,null,"T/R 13-01 Annex C"," X","X",null,1.5,24,66," 0"]
["Ireland","IRL",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Ireland","IRL",0,"3400-3600"," X",null,null,null,null," X",null,null,null,null,null,null,null,120,"ERC/REC 14-03",null,null,null,null,null,null," 66"]
["Ireland","IRL",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
["Ireland","IRL",0,"5850-5925"]
["Ireland","IRL",0,"5925-7125"," X",null,null,null,null,null," X",null,null,null,null,2,356,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null," X",8,40,90," 28"]
["Ireland","IRL",0,"7125-7750"," X",null,null,null,null,null," X",null,null,null,null,1,279,null,"ECC REC (02)06"," X","X","X",7,36,76," 57"]
["Ireland","IRL",0,"7750-7900"]
["Ireland","IRL",0,"7900-8500"," X",null,null,null,null,null," X",null,null,null,null,null,315,null,"ECC REC (02)06"," X","X","X",5,36,81," 48"]
["Ireland","IRL",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Ireland","IRL",0,"10000-10680"," X",null,null,null," X",null,null,null,null,null,null,null,null,30,"National Legislation: S.I. 79 of 2003\nNational Legislation: S.I. 530 of 2003 European Legislation: Decision 2008/411/EC ",null,null,null,null,null,null," 75"]
["Ireland","IRL",0,"10700-11700"," X",null,null,null,null,null,"X",null,null,null,null,null,648,null,"ERC/REC 12-06",null,"X","X",1.5,24,56," 39"]
["Ireland","IRL",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null," National Legislation: S.I. 370 of 2009"]
["Ireland","IRL",0,"11700-12500"]
["Ireland","IRL",0,"12750-13250"," X",null,null,null,null,null,"X",null,null,null,null,2,1078,null,"ERC/REC 12-02","X","X","X",1.5,19,53," 27"," X"]
["Ireland","IRL",0,"12750-13250",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Ireland","IRL",0,"14250-14500"]
["Ireland","IRL",0,"14500-14620 and 15230-15350"," X",null,null,null,null,null," X",null,null,null,null,null,1718,null,"ERC/REC 12-07\nNational Legislation: S.I. 370 of 2009"," X","X","X",1.7,17,53," 29"," X"]
["Ireland","IRL",0,"17700-19700"," X",null,null,null,null,null," X",null,null,null,null,null,686,null,"ERC/REC 12-03\nNational Legislation: S.I. 370 of 2009",null," X","X",0.3,9,45," 28"," X"]
["Ireland","IRL",0,"22000-22600 and 23000-23600"," X",null,null,null,null,null," X",null,null,null,null,null,2178,null,"T/R 13-02 Annexes A1, A2, A3"," X","X","X",0.2,6.7,24," 36"," X"]
["Ireland","IRL",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Ireland","IRL",0,"24500-26500"," X",null,null,null,"X",null," X",null,null,null,null,null,636,null,"T/R 13-02 Annex B"," X","X","X",0.05,5,17," 43"," X"]
["Ireland","IRL",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Ireland","IRL",0,"24500-26500",null," X",null,null,null,null," X",null,null,null,null,null,null,null," National Legislation: S.I. 762 of 2007"]
["Ireland","IRL",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
["Ireland","IRL",0,"24500-26500","X",null,null,null,null,"X",null,null,null,null,null,null,null,15,"National Legislation: S.I. 79 of 2003",null,null,null,null,null,null,55]
["Ireland","IRL",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 530 of 2003"]
["Ireland","IRL",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Ireland","IRL",0,"27500-29500"]
["Ireland","IRL",0,"31800-33400"]
["Ireland","IRL",0,"37000-39500"," X",null,null,null,null,null,"X",null,null,null,null,null,2924,null,"T/R 12-01"," X","X","X",1.6E-2,1.9,10.7," 31"," X"]
["Ireland","IRL",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"National Legislation: S.I. 370 of 2009"]
["Ireland","IRL",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Ireland","IRL",0,"57000-59000","X",null,null,null,null,null," X",null,null,null,null,null,1,null,"ECC/REC/(09)01\nNational Legislation: S.I. 370 of 2009"," X",null,null,1.4,1.4,1.4," 0"]
["Ireland","IRL",0,"71000-76000 and  81000-86000","X",null,null,null,null,null," X",null,null,null,null,null,5,null,"ECC/REC/(05)07\nNational Legislation: S.I. 370 of 2009",null,null," X",0.1,1,2.9," 0"]
["Italy","ITA",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Italy","ITA",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Italy","ITA",0,"1400-1525","X",null,null,null,null,null,"X",null,null,null,null,null,530,null,"national","X"]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X","X",null,null,null,null,12,21,null,"T/R 13-01 Annex C","x",null,null,6.71,30.92,64.77,0.15]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X","X",null,null,null,null,95,3,null,"T/R 13-01 Annex C",null,"x",null,3.28,52.12,238.26,0.15]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X","X",null,null,null,null,null,122,null,"T/R 13-01 Annex C",null,null,"x",0.49,67.06,238.26,0.15]
["Italy","ITA",0,"2025-2110 and 2200-2290","X",null,null,null,null,"X",null,null,null,null,null,null,null,10,"T/R 13-01 Annex C","X",null,null,null,null,null,0.05,"stable"]
["Italy","ITA",0,"2300-2400","X",null,null,null,"X",null,null,null,null,null,null,null,275,null,"national","X"]
["Italy","ITA",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,null,null,null,"No info"]
["Italy","ITA",0,"3600-4200","X",null,null,null,"X",null,"X",null,null,null,null,null,77,null,"ERC/REC 12-08",null,null,"X",13.6,60,238,-5]
["Italy","ITA",0,"3600-4200","X",null,null,null,null,null,"X",null,"X",null,null,105,9,null,"ERC/REC 12-08",null,"X","X",17.46,88.5,238.26,-5]
["Italy","ITA",0,"3600-4200",null,"X",null,null,null,null,"X",null,"X",null,null,null,210,null,"ERC/REC 12-08",null,null,"X",13.6,67.34,238.26,-5]
["Italy","ITA",0,"5850-5925","X",null,null,null,"X",null,null,null,"X",null,null,71,null,null,"national",null,null,"x",20,50,238,1,"yes"]
["Italy","ITA",0,"5850-5925",null,"X",null,null,null,null,"X",null,"X",null,null,116,null,null,"national",null,"x",null,9.4700000000000006,61.58,121.23,1,"yes"]
["Italy","ITA",0,"5925-7125","X",null,null,null,"X",null,"X",null,"X",null,null,102,808,null,"ERC/REC 14-01 and ERC/REC 14-02",null,"X","X",6.32,44,83,0.15,"almost"]
["Italy","ITA",0,"7750-7900"]
["Italy","ITA",0,"7900-8500","X",null,null,null,"X",null,"X",null,null,null,null,null,2231,null,"national",null,"X","X",null,30,null,0.1,"almost"]
["Italy","ITA",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,5,null,"national",null,null,"X"]
["Italy","ITA",0,"10000-10680","X",null,null,null,null,null,"X",null,"X",null,null,{"$f":"935+529+446","v":1910},34,null,"ERC/REC 12-05",null,"X",null,3,25,84,1,"yes"]
["Italy","ITA",0,"10000-10680","X",null,null,null,null,null,"X",null,"X",null,null,{"$f":"236+24","v":260},80,null,"ERC/REC 12-05",null,null,"x",5.5,35,50,1,"yes"]
["Italy","ITA",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,3110,null,"ERC/REC 12-06",null,"X","X",null,18,null,0.15,"yes"]
["Italy","ITA",0,"10700-11700","X",null,null,null,null,null,"X",null,"X",null,null,58,99,null,"ERC/REC 12-06",null,"X","X",3,22,60,0.15,"yes"]
["Italy","ITA",0,"11700-12500","X",null,null,null,null,null,"X",null,null,null,null,22,1,null,null,null,"x",null,1.97,27.6,62.94]
["Italy","ITA",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,6106,null,"ERC/REC 12-02",null,"X","X",7,16,30,0.15,"yes"]
["Italy","ITA",0,"14250-14500","X",null,null,null,null,null,null,null,"X",null,null,1030,null,null,"national",null,null,"X",3,11,27,0.05,"yes"]
["Italy","ITA",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,4070,null,"ERC/REC 12-07","X","X","X",7,16,33,0.15,"yes"]
["Italy","ITA",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,1562,null,"national",null,"X",null,null,null,null,null,"yes"]
["Italy","ITA",0,"17300-17700","X",null,null,null,"X",null,null,null,null,null,null,null,33,null,"national",null,"X"]
["Italy","ITA",0,"17700-19700","X","X",null,null,"X",null,"X",null,null,null,null,null,{"$f":"14300+1512","v":15812},null,"ERC/REC 12-03","X","X","X",0.3,6,12,0.25,"highly"]
["Italy","ITA",0,"17700-19700","X",null,null,null,null,null,"X",null,"X",null,null,71,35,null,null,null,"X","X",1.3,4,7.5,0.25]
["Italy","ITA",0,"21200-22000","X",null,null,null,null,null,"X",null,null,null,null,26,7,null,null,null,"X",null,0.19,2.44,7.25]
["Italy","ITA",0,"22000-22600 and 23000-23600","X","X",null,null,"X",null,"X",null,null,null,null,2,{"$f":"10970+1101","v":12071},null,"T/R 13-02 Annexes A1, A2, A3","X","X","X",2.1800000000000002,2.95,3.17,0.25,"yes"]
["Italy","ITA",0,"22600-23000","x",null,null,null,null,null,"X",null,null,null,null,1,null,null,null,null,"x",null,null,0.19]
["Italy","ITA",0,"24500-26500",null,"X",null,null,null,"X","X",null,null,null,null,null,null,"not known","T/R 13-02 Annex B",null,null,null,null,null,null,0.15,"not yet"]
["Italy","ITA",0,"24500-26500"]
["Italy","ITA",0,"27500-29500",null,"X",null,null,null,"X","X",null,null,null,null,null,null,"not known","T/R 13-02 Annex C",null,null,null,null,null,null,0.15,"not yet"]
["Italy","ITA",0,"27500-29500"]
["Italy","ITA",0,"31800-33400"]
["Italy","ITA",0,"37000-39500","X","X",null,null,"X",null,"X",null,null,null,null,null,10412,null,"T/R 12-01","X","X","X",null,"0,8/10",null,0.25,"yes"]
["Italy","ITA",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["Latvia","LVA",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Latvia","LVA",0,"1350-1375 and 1492-1517",null,"X",null,null,null,"X",null,null,null,null,null,null,null,30,"national plan","X",null,null,null,null,null,-50]
["Latvia","LVA",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Latvia","LVA",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,null,null,3,null,"T/R 13-01 Annex C","X",null,null,5,null,41]
["Latvia","LVA",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,69,"ERC/REC 14-03",null,"X",null,null,10,null,50]
["Latvia","LVA",0,"3600-4200",null,"X",null,null,null,"X",null,null,null,null,null,null,null,154,"ERC/REC 12-08",null,"X",null,null,10,null,50]
["Latvia","LVA",0,"4400-5000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band"]
["Latvia","LVA",0,"5850-5925",null,"X",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Planning BFWA  within 5725-5875 MHz band. BFWA  5905-5925 MHz"]
["Latvia","LVA",0,"5925-6245 and  6425-7125","X",null,null,null,"X",null,null,null,null,null,null,null,39,null,"ERC/REC 14-01 ",null,null,"X",22,30,36,100]
["Latvia","LVA",0,"5925-6245 and  6425-7125","X",null,null,null,"X",null,null,null,null,null,null,null,17,null,"ERC/REC 14-02",null,null,"X",28,35,52,100]
["Latvia","LVA",0,"7125-7800","X",null,null,null,"X",null,null,null,null,null,null,null,104,null,"ITU-R F.385",null,null,"X",14,35,54,50,null,null,"Military band 7250-7331 MHz"]
["Latvia","LVA",0,"7800-7900",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band 7850-7900 MHz"]
["Latvia","LVA",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,152,null,"ECC REC (02)06",null,null,"X",12,35,50,50,null,null,"Military band 7975-8024 MHz"]
["Latvia","LVA",0,"10000-10680","X",null,null,null,"X",null,null,null,null,null,null,null,105,null,"ERC/REC 12-05","X",null,null,null,null,null,-80,null,null,"10300-10500 MHz"]
["Latvia","LVA",0,"10000-10680",null,"X",null,null,null,"X",null,null,null,null,null,null,null,66,"ERC/REC 12-05 and ERC/REC 13-04",null,"X",null,null,10,null,50]
["Latvia","LVA",0,"10700-11700","X",null,null,null,null,null,null,null,"X",null,null,38,null,null,"ITU-R F.387",null,null,null,0.3,10,32,-50,null,null,"Analog fixed links"]
["Latvia","LVA",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BROADCASTING-SATELLITE"]
["Latvia","LVA",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,630,null,"ERC/REC 12-02",null,"X",null,2,35,47,20]
["Latvia","LVA",0,"12750-13250",null,"X",null,null,null,null,null,null,"X",null,null,null,null,7,"national plan","X",null,null,null,5,null,null,null,null,"MMDS"]
["Latvia","LVA",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FIXED-SATELLITE"]
["Latvia","LVA",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,48,null,"ERC/REC 12-07",null,"X",null,3,25,37,20]
["Latvia","LVA",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HDFSS"]
["Latvia","LVA",0,"17700-19700","X",null,null,null,"x",null,null,null,null,null,null,null,390,null,"ERC/REC 12-03",null,null,"X",1,20,43,20]
["Latvia","LVA",0,"21200-22000","X",null,null,null,"x",null,null,null,null,null,null,2,null,null,"national plan","X",null,null,3,5,8,100]
["Latvia","LVA",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,592,null,"T/R 13-02 Annexes A1, A2, A3",null,null,"X",0.15,15,25,30]
["Latvia","LVA",0,"22600-23000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAP/SAB "]
["Latvia","LVA",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAB/SAP, SRR"]
["Latvia","LVA",0,"24500-26500","X",null,null,null,"x",null,null,null,null,null,null,null,6,null,"T/R 13-02 Annex B",null,null,"X",1.4,5,6]
["Latvia","LVA",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,52,null,null,"X",null,null,5,null,50]
["Latvia","LVA",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Military band"]
["Latvia","LVA",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Latvia","LVA",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,51,null,null,null,"X",null,null,null,50]
["Latvia","LVA",0,"31000-31300","?",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,null,null,null,"Fixed links, FWA"]
["Latvia","LVA",0,"31800-33400",null,"X",null,null,"X",null,null,null,null,null,null,null,43,null,"ERC/REC/(01)02",null,null,"X",0.2,3,4.5999999999999996,100]
["Latvia","LVA",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,27,null,"T/R 12-01",null,null,"X",0.2,3,4.7,20]
["Latvia","LVA",0,"40500-43500",null,"X",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,null,null,null,"MWS (MVDS)"]
["Latvia","LVA",0,"47200-48500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SAP/SAB, HAPS "]
["Latvia","LVA",0,"48500-50200","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"Fixed links"]
["Latvia","LVA",0,"50400-51400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Future satellite and terrestrial applications"]
["Latvia","LVA",0,"51400-52600","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"Fixed links"]
["Latvia","LVA",0,"55780-57000","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"Fixed links"]
["Latvia","LVA",0,"57000-59000",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"SRD, Fixed links, FWA"]
["Latvia","LVA",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"SRD,  Military band 59-61 GHz"]
["Latvia","LVA",0,"71000-76000 and  81000-86000","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"Military band 71-74 GHz, 81-84 GHz. Fixed links 74-76GHz, 84-86 GHz"]
["Latvia","LVA",0,"92000-95000"]
["Lithuania","LTU",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"T/R 13-01 Annex A"]
["Lithuania","LTU",0,"1350-1375 and 1492-1517",null,"X",null,null,null,"X","X",null,null,null,null,null,null,8,"local",null,null,null,null,null,null,-100]
["Lithuania","LTU",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"T/R 13-01 Annex B"]
["Lithuania","LTU",0,"1375-1400 and 1427-1452",null,"X",null,null,null,"X","X",null,null,null,null,null,null,8,"local",null,null,null,null,null,null,-100]
["Lithuania","LTU",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,"X",null,null,5,null,"T/R 13-01 Annex C",5]
["Lithuania","LTU",0,"3400-3600","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 14-03"]
["Lithuania","LTU",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,402,"ERC/REC 14-03",null,null,null,null,null,null,50,null,null,"Fixed and mobile P-MP (BWA)"]
["Lithuania","LTU",0,"3600-4200","X",null,null,null,"X",null,null,null,null,"X",null,null,30,null,"ERC/REC 12-08",null,null,30]
["Lithuania","LTU",0,"3600-4200",null,"X",null,null,null,"X",null,null,null,"X",null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"3600-3800 future for BWA"]
["Lithuania","LTU",0,"5850-5925","X",null,null,null,"X",null,"X",null,null,null,null,null,29,null,null,29]
["Lithuania","LTU",0,"5850-5925",null,null,null,null,null,"X",null,null,null,"X",null,null,null,null,"5/10/20MHz",null,null,null,null,null,null,null,null,null,"5850-5875, 5905-5925 future P-MP"]
["Lithuania","LTU",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,137,null,"ERC/REC 14-01 and ERC/REC 14-02"]
["Lithuania","LTU",0,"5925-7125",null,null,null,null,null,"X",null,null,null,"X",null,null,null,null,"5/10/20MHz",null,null,null,null,null,null,null,null,null,"5925-6425 future for P-MP"]
["Lithuania","LTU",0,"7125-7750","X",null,null,null,"X",null,null,null,null,null,null,null,197,null,"ECC REC (02)06"]
["Lithuania","LTU",0,"7750-7900","X",null,null,null,"X",null,null,null,null,null,null,null,0,null,"local"]
["Lithuania","LTU",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,116,null,"ECC REC (02)06"]
["Lithuania","LTU",0,"10150-10300 and 10500-10650","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-05"]
["Lithuania","LTU",0,"10150-10300 and 10500-10650",null,"X",null,null,null,"X",null,null,null,null,null,null,null,6,"ERC/REC 12-05",null,null,null,null,null,null,100]
["Lithuania","LTU",0,"10300-10500","X",null,null,null,"X",null,"X",null,null,null,null,null,420,null,"ERC/REC 12-05",420]
["Lithuania","LTU",0,"10700-11700","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 12-06"]
["Lithuania","LTU",0,"11700-12500"]
["Lithuania","LTU",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,222,null,"ERC/REC 12-02"]
["Lithuania","LTU",0,"14250-14500"]
["Lithuania","LTU",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,262,null,"ERC/REC 12-07"]
["Lithuania","LTU",0,"17700-19700","X",null,null,null,"X",null,null,null,null,null,null,null,490,null,"ERC/REC 12-03"]
["Lithuania","LTU",0,"21200-22000","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"local"]
["Lithuania","LTU",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,1362,null,"T/R 13-02 Annexes A1, A2, A3"]
["Lithuania","LTU",0,"22600-23000","X",null,null,null,"X",null,null,null,"X",null,null,1,null,null,"local"]
["Lithuania","LTU",0,"24250-24500","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"local"]
["Lithuania","LTU",0,"24500-26500","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"T/R 13-02 Annex B"]
["Lithuania","LTU",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,84,"T/R 13-02 Annex B",null,null,null,null,null,null,30]
["Lithuania","LTU",0,"27500-29500","X",null,null,null,"X",null,null,null,null,null,null,null,20,null,"T/R 13-02 Annex C",null,20]
["Lithuania","LTU",0,"27500-29500",null,"X",null,null,null,"X",null,null,"X",null,null,null,null,8,"54MHz/3,2MHz",null,null,null,null,null,null,0,null,null,"LMDS (do not comply T/R 13-02)"]
["Lithuania","LTU",0,"31000-31300","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ECC/REC/(02)02"]
["Lithuania","LTU",0,"31800-33400","X",null,null,null,"X",null,null,null,null,null,null,null,28,null,"ERC/REC/(01)02"]
["Lithuania","LTU",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,268,null,"T/R 12-01",null,268]
["Lithuania","LTU",0,"40500-43500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,0,"ECC/REC/(01)04"]
["Lithuania","LTU",0,"48500-50200","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 12-10"]
["Lithuania","LTU",0,"51400-52600","X",null,null,null,"X",null,null,null,null,null,null,0,0,null,"ERC/REC 12-11"]
["Lithuania","LTU",0,"71000-76000 and  81000-86000",null,null,null,"X","X",null,null,null,null,null,null,0,0,null,"ECC/REC/(05)07"]
["Luxembourg","LUX",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"T/R 13-01 Annex A","X",null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Luxembourg","LUX",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"T/R 13-01 Annex B","X",null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Luxembourg","LUX",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Luxembourg","LUX",0,"3400-3600",null,"X",null,null,null,"X","X",null,null,null,null,null,null,3,"Nat. freq. Plan",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"3600-4200","X",null,null,null,"X",null,"X",null,"X",null,null,1,0,null,"Nat. freq. Plan",null,"X","X",null,"20-80",null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Luxembourg","LUX",0,"5925-7125","X",null,null,null,"X",null,"X",null,"X",null,null,10,2,null,"ERC/REC 14-01 and ERC/REC 14-02 and national plan",null,"X","X",3.4,"20-80",63,"N/A","NO","NO"]
["Luxembourg","LUX",0,"7125-7750","X",null,null,null,"X",null,"X",null,"X",null,null,0,26,null,"ECC REC (02)06",null,"X","X",7.9,"20-80",55.9,"N/A","NO","NO"]
["Luxembourg","LUX",0,"7750-7900","X",null,null,null,"X",null,"X",null,"X",null,null,0,0,null,"Nat. freq. plan",null,"X","X",null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"7900-8500","X",null,null,null,"X",null,"X",null,"X",null,null,4,6,null,"ECC REC (02)06",null,"X","X",5.0999999999999996,"20-80",62,"N/A","NO","NO"]
["Luxembourg","LUX",0,"10000-10680","X",null,null,null,"X",null,"X",null,"X",null,null,2,0,null,"ERC/REC 12-05",null,"X","X",32,"10-50",62,"N/A","NO","NO"]
["Luxembourg","LUX",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Luxembourg","LUX",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Luxembourg","LUX",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Luxembourg","LUX",0,"12750-13250","X",null,null,null,"X",null,"X",null,"X",null,null,8,22,null,"ERC/REC 12-02",null,"X","X",5.6,"5-35",32,"N/A","NO","NO"]
["Luxembourg","LUX",0,"12750-13250",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Luxembourg","LUX",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Luxembourg","LUX",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,"X",null,null,0,64,null,"ERC/REC 12-07",null,"X","X",1.4,"5-30",34.700000000000003,"N/A","NO","NO"]
["Luxembourg","LUX",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,null,0,47,null,"ERC/REC 12-03",null,null,"X",4.8,"4-25",24.1,"N/A","NO","NO"]
["Luxembourg","LUX",0,"17700-19700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Luxembourg","LUX",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,"X",null,null,1,243,null,"T/R 13-02 Annexes A1, A2, A3",null,"X",null,0.3,"3-20",15,"N/A","NO","NO"]
["Luxembourg","LUX",0,"22000-22600 and 23000-23600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Luxembourg","LUX",0,"24250-24500",null,"X",null,null,null,"X","X",null,"X",null,null,null,null,4,"Nat. freq. plan",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"24250-24500","X",null,null,null,"X",null,"X",null,"X",null,null,0,10,null,"Nat. freq. plan",null,"X",null,null,"2-15",null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"24500-26500",null,"X",null,null,null,"X","X",null,"X",null,null,null,null,4,"T/R 13-02 Annex B",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"24500-26500","X",null,null,null,"X",null,"X",null,"X",null,null,0,10,null,"Nat. freq. plan",null,"X",null,null,"2-15",null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C"]
["Luxembourg","LUX",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Luxembourg","LUX",0,"31000-31300","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ECC/REC/(02)02",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"31000-31300",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Luxembourg","LUX",0,"31800-33400","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC/(01)02",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan "]
["Luxembourg","LUX",0,"37000-39500","X",null,null,null,"X",null,"X",null,"X",null,null,1,110,null,"T/R 12-01",null,"X",null,0.13,"1-6",5.4,"N/A","NO","NO"]
["Luxembourg","LUX",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nat. freq. plan"]
["Luxembourg","LUX",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"///"]
["Luxembourg","LUX",0,"48500-50200","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-10",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"51400-52600","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-11",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"55780-57000","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ERC/REC 12-12",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"57000-59000","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"N/A","NO","NO"]
["Luxembourg","LUX",0,"59000-64000","X",null,null,null,"X",null,"X",null,null,null,null,0,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"N/A","NO","NO"]
["Netherlands","NLD",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Netherlands","NLD",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex B"]
["Netherlands","NLD",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,null,null,null,"X",null,2,7,null,"nat. plan 1427 - 1517","x",null,null,39.299999999999997,58.9,71.400000000000006,10]
["Netherlands","NLD",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Netherlands","NLD",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03"]
["Netherlands","NLD",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
["Netherlands","NLD",0,"5850-5925"]
["Netherlands","NLD",0,"5850-5925"]
["Netherlands","NLD",0,"5925-7125","X",null,null,null,null,null,null,null,null,"X",null,null,51,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",21.41,31.11,49.3,20]
["Netherlands","NLD",0,"7125-7750","X",null,null,null,null,null,null,null,null,"X",null,null,113,null,"ECC REC (02)06","X","X","X",10.4,27.7,55.6,20]
["Netherlands","NLD",0,"7750-7900"]
["Netherlands","NLD",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC REC (02)06"]
["Netherlands","NLD",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Netherlands","NLD",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Netherlands","NLD",0,"11700-12500"]
["Netherlands","NLD",0,"12750-13250","X",null,null,null,null,null,null,null,null,"X",null,null,201,null,"ERC/REC 12-02",null,"X","X",8.35,18.2,31.5]
["Netherlands","NLD",0,"14250-14500"]
["Netherlands","NLD",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,null,"X",null,null,116,null,"ERC/REC 12-07","x","x","x",7.71,14.7,34.9,20]
["Netherlands","NLD",0,"17700-19700","X",null,null,null,null,null,null,null,null,"X",null,null,1020,null,"ERC/REC 12-03",null,"x","x",7.7,5.27,34.9,20]
["Netherlands","NLD",0,"17700-19700","X",null,null,null,null,null,null,null,null,"X",null,null,43,null,"F-5958-8 Annex 8",null,"x","x",5.63,13.11,18.649999999999999,0]
["Netherlands","NLD",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,"X",null,null,1450,null,"T/R 13-02 Annexes A1, A2, A3","x","x","x",3,7.65,14.78,30]
["Netherlands","NLD",0,"24500-26500","x",null,null,null,null,null,null,null,null,"X",null,null,908,null,"T/R 13-02 Annex B","x","x","x",2.5499999999999998,6.42,14.52,30]
["Netherlands","NLD",0,"24500-26500",null,null,null,null,null,"x",null,null,null,"X",null,null,null,90,"T/R 13-02 Annex B",null,null,null,null,null,null,10]
["Netherlands","NLD",0,"27500-29500","X",null,null,null,null,null,null,null,null,"X",null,null,185,null,"T/R 13-02 Annex C",null,null,"x",2.52,4.21,6.8730000000000002,30]
["Netherlands","NLD",0,"27500-29500"]
["Netherlands","NLD",0,"31800-33400","X",null,null,null,null,null,null,null,null,"X",null,null,515,null,"ERC/REC/(01)02","x","x","x",0.253,3.57,6.27,30]
["Netherlands","NLD",0,"37000-39500","X",null,null,null,null,null,null,null,null,"X",null,null,6377,null,"T/R 12-01","x","x","x",0.05,2.15,10.266,30]
["Netherlands","NLD",0,"40500-43500","X",null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,100]
["Norway","NOR",0,"1350-1375 and 1492-1517","X",null,null,null,null,null,null,null,null,"X",null,8,46,null,"T/R 13-01 Annex A","x",null,null,1,12,42]
["Norway","NOR",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,null,null,null,"X",null,1,26,null,"T/R 13-01 Annex B","x",null,null,1,18,42.5]
["Norway","NOR",0,"2025-2110 and 2200-2290","X","X",null,null,null,null,null,null,null,null,"X",null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,null,"SAP/SAB"]
["Norway","NOR",0,"2025-2110 and 2200-2290","X",null,null,null,null,null,null,null,null,"X",null,null,2,null,null,null,"x",null,17,19.7,22,null,null,null,"Offshore"]
["Norway","NOR",0,"3410-3600",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 14-03 Annex A"]
["Norway","NOR",0,"3410-3600","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Norway","NOR",0,"3600-3800",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-08"]
["Norway","NOR",0,"3600-3800","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Norway","NOR",0,"3800-4200",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-08"]
["Norway","NOR",0,"3800-4200","X",null,null,null,null,null,null,null,null,"X",null,null,2,null,null,null,"X",null,2.5,2.7,2.9,null,null,null,null,null,"Offshore"]
["Norway","NOR",0,"5725-5795 and 5815-5850",null,null,null,"X",null,null,null,null,null,"X",null,null,null,null,"National plan"]
["Norway","NOR",0,"5925-7125","X","X",null,null,null,null,null,null,null,"X",null,null,146,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",2.8,37.5,123]
["Norway","NOR",0,"7125-7425","X",null,null,null,null,null,null,null,null,"X",null,null,135,null,null,null,null,"X",4.2,35.5,96]
["Norway","NOR",0,"7425-7725","X",null,null,null,null,null,null,null,null,"X",null,null,446,null,null,null,null,"X",1.2,32.299999999999997,113]
["Norway","NOR",0,"7900-8200",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ECC REC (02)06"]
["Norway","NOR",0,"10000-10680",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-05"]
["Norway","NOR",0,"10700-11700",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ITU rec F.387-10"]
["Norway","NOR",0,"10700-11700","X",null,null,null,null,null,null,null,null,"X",null,null,234,null,null,null,null,"x",0.5,23,66.5]
["Norway","NOR",0,"12750-13250",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-02"]
["Norway","NOR",0,"12750-13250","X",null,null,null,null,null,null,null,null,"X",null,null,1240,null,null,null,"X","X",0.1,14.7,90]
["Norway","NOR",0,"14250-14500"]
["Norway","NOR",0,"14500-14620 and 15230-15350"]
["Norway","NOR",0,"17700-19700",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-03"]
["Norway","NOR",0,"17700-19700","X",null,null,null,null,null,null,null,null,"X",null,null,387,null,null,null,null,"x",0.5,10.199999999999999,44.8]
["Norway","NOR",0,"22000-22600 and 23000-23600",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annexes A1, A2, A3"]
["Norway","NOR",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,"X",null,2,64,null,null,null,null,"x",0.3,5.7,25.4]
["Norway","NOR",0,"24500-26500",null,"x",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annex B"]
["Norway","NOR",0,"24500-26500","x",null,null,null,null,null,null,null,null,"X",null,3,65,null,null,null,"x","x",0.5,4.8,21.1]
["Norway","NOR",0,"27500-29500",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 13-02 Annex C"]
["Norway","NOR",0,"27500-29500","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Norway","NOR",0,"31800-33400",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC/(01)02"]
["Norway","NOR",0,"31800-33400","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Norway","NOR",0,"37000-39500",null,"x",null,null,null,null,null,null,null,"X",null,null,null,null,"T/R 12-01 Annex A"]
["Norway","NOR",0,"37000-39500","X",null,null,null,null,null,null,null,null,"X",null,null,64,null,null,null,null,"x",0.1,3.6,16.399999999999999]
["Norway","NOR",0,"37000-39500"]
["Norway","NOR",0,"40500-43500",null,"X",null,null,null,null,null,null,null,"X",null,null,null,null,"ECC/REC/(01)04 Annex A"]
["Norway","NOR",0,"40500-43500","X",null,null,null,null,null,null,null,null,"X",null,null,0]
["Norway","NOR",0,"48500-50200","X","X",null,null,null,null,null,null,null,"X",null,null,0,null,"ERC/REC 12-10"]
["Norway","NOR",0,"55780-57000","X","X",null,null,null,null,null,null,null,"X",null,null,0,null,"ERC/REC 12-09"]
["Norway","NOR",0,"57000-64000","X","X",null,null,null,null,null,null,null,"X",null,null,1,null,"ECC/REC/(09)01",null,null,1,null,0.4]
["Norway","NOR",0,"71000-76000 and  81000-86000","X","X",null,null,null,null,null,null,null,"X",null,null,4,null,"ECC/REC/(05)07",null,null,"x",1,1.8,3.4]
["Portugal","PRT",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,null,null,null,55,null,"T/R 13-01 Annex A","X",null,null,12,"40",57,5]
["Portugal","PRT",0,"1350-1375 and 1492-1517","X",null,null,null,null,"X",null,null,null,null,null,null,null,9,"T/R 13-01 Annex A","X",null,null,2,"10",18,0]
["Portugal","PRT",0,"1375-1400 and 1427-1452","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"T/R 13-01 Annex B","X",null,null,null,"40",null,"No use at the moment."]
["Portugal","PRT",0,"1517-1525","X",null,null,null,null,null,null,null,"X",null,null,365,null,null,"National plan (STL)","X",null,null,null,"15",null,5]
["Portugal","PRT",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,"TCR, SAP/SAB",null,11,null,"T/R 13-01 Annex C","X",null,null,2,"40",193,0]
["Portugal","PRT",0,"2025-2110 and 2200-2290","X",null,null,null,"X",null,null,null,null,null,"TCR, SAP/SAB",null,2,null,"National plan",null,"X",null,20,"40",64,0]
["Portugal","PRT",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,64,"ERC/REC 14-03","X",null,null,null,"20",null," BWA"]
["Portugal","PRT",0,"3600-4200",null,"X",null,null,null,"X",null,null,null,null,"VSAT (3.8-4.2 GHz)",null,null,null,"ERC/REC 12-08","X","X",null,null,"20",null,null,null,null,"BWA in 3.3 -3.6GHz and FSS in 3.8-4.2GHz"]
["Portugal","PRT",0,"4400-5000",null,null,null,null,null,null,null,null,null,"X","Military"]
["Portugal","PRT",0,"4400-5000"]
["Portugal","PRT",0,"5850-5925",null,null,null,"X",null,null,null,null,null,null,"ISM, SRD"]
["Portugal","PRT",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,"VSAT, SRD",2,8,null,"ERC/REC 14-01 ",null,"X","X",40,40,88,50]
["Portugal","PRT",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,"VSAT, SRD",null,59,null,"ERC/REC 14-02",null,"X","X",15,40,84,10]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS, Military (7.25-7.3 GHz)",null,7,null,"7 LOW: ITU-R F.385","X",null,null,15,"30",53,0]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS, Military (7.25-7.3 GHz)",null,287,null,"7 LOW: ECC REC (02)06","X","X","X",6,"30",63,10]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,40,null,"7 HIGH: ITU-R F.385","X","X",null,3,"22",71,-50]
["Portugal","PRT",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,30,null,"7 HIGH: ECC REC (02)06","X","X","X",15,"30",78,50]
["Portugal","PRT",0,"7750-7900","X",null,null,null,"X",null,"X",null,null,null,null,null,26,null,"8 LOW: ITU-R F.386",null,"X","X",2,"30",75,50]
["Portugal","PRT",0,"7900-8500","X",null,null,null,"X",null,null,null,"X",null,"FSS, EESS, Military (7.975-8.025 GHz)",7,9,null,"8 HIGH: ITU-R F.386","X",null,null,6,"40",88,-100]
["Portugal","PRT",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,"AM, SAP/SAB, SRD",null,null,null,"ERC/REC 12-05"]
["Portugal","PRT",0,"10700-11700","X",null,null,null,"X",null,"X",null,"X",null,"FSS, VSAT, SNG, SIT, AES, Euteltracs",null,117,null,"ERC/REC 12-06",null,"X","X",2,"20",41,5]
["Portugal","PRT",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,"RAD-S, SIT"]
["Portugal","PRT",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,49,null,"ITU-R F.497","X",null,null,2,"25",46,-50]
["Portugal","PRT",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,368,null,"ERC/REC 12-02","X","X","X",1,"15",57,10]
["Portugal","PRT",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,"FSS, VSAT, SNG, AES"]
["Portugal","PRT",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,362,null,"ERC/REC 12-07","X","X",null,1,"15",37,5]
["Portugal","PRT",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,"FSS, HDFSS"]
["Portugal","PRT",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,131,null,"ITU-R F.595","X",null,null,2,"10",29,10]
["Portugal","PRT",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,"FSS",null,1087,null,"ERC/REC 12-03",null,"X","X",0,"7",35,20]
["Portugal","PRT",0,"21200-22000",null,null,null,null,null,null,null,null,null,null,"SRR"]
["Portugal","PRT",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,"SRR",null,10,null,"Report 936-2 Annex 6","X",null,null,1,"5",12,-100]
["Portugal","PRT",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,"SRR",null,908,null,"T/R 13-02 Annexes A1","X","X","X",null,"5",12,10]
["Portugal","PRT",0,"22600-23000","X",null,null,null,"X",null,"?",null,null,null,"SRR",null,null,null,"T/R 13-02 Annexes A2, A3",null,null,null,null,null,null,"no use at the moment"]
["Portugal","PRT",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,"SRR, SRD"]
["Portugal","PRT",0,"24500-26500",null,"X",null,null,null,"X","X",null,null,null,"SRR, SRD, Military (25.25-25.492 GHz and 26.25-27.5 GHz)",null,null,125,"T/R 13-02 Annex B","X","X",null,null,"5",null,0]
["Portugal","PRT",0,"24500-26500"]
["Portugal","PRT",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,"SRR, SRD, Military (26.25-27.5 GHz)"]
["Portugal","PRT",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,"FSS, HDFSS",null,null,21,"T/R 13-02 Annex C",null,"X",null,null,"5",null,0]
["Portugal","PRT",0,"27500-29500"]
["Portugal","PRT",0,"31000-31300",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02",null,null,null,null,null,null,"Planned"]
["Portugal","PRT",0,"31800-33400","X",null,null,null,"X","X",null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,null,null,"Not used at the moment."]
["Portugal","PRT",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,"FS",null,617,null,"T/R 12-01","X","X","X",0,"2",6,5]
["Portugal","PRT",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,"MWS, MVDS",null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"Planned "]
["Portugal","POR",0,"47200-48500",null,null,null,null,null,null,null,null,null,null,"HDFSS (47.5-47.9 GHz)"]
["Portugal","POR",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,"HDFSS (48.2-48.54 GHz and 49.44-50.2 GHz)",null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,"Planned"]
["Portugal","POR",0,"50400-51400",null,null,null,null,null,null,null,null,null,"X"]
["Portugal","POR",0,"51400-52600",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,"Planned"]
["Portugal","POR",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,"EESS",null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,"Planned"]
["Portugal","POR",0,"57000-59000","?","?",null,null,"X","X","X",null,null,null,"EESS, SRD",null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"No use at the moment."]
["Portugal","POR",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,"SRD, ISM, Military (59-61 GHz)",null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Planned"]
["Portugal","POR",0,"71000-76000 and  81000-86000","?","?",null,null,"X","X","X",null,null,null,"SRD, AM (75.5-76 GHz), Military (71-74 GHz and 81-84 GHz)",null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,"No use at the moment."]
["Portugal","POR",0,"92000-95000",null,null,null,null,null,null,null,null,null,"X"]
["Russia","RUS",0,"1350-1375 and 1492-1517","X","X",null,null,null,null,"X",null,null,null,null,null,25,49,"T/R 13-01 Annex A","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Russia","RUS",0,"1375-1400 and 1427-1452","X","X",null,null,null,null,"X",null,null,null,null,null,30,49,"T/R 13-01 Annex B","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Russia","RUS",0,"2025-2110 and 2200-2290","X","X",null,null,null,null,"X",null,null,null,null,null,73,1,"T/R 13-01 Annex C","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Russia","RUS",0,"3400-3600","X","X",null,null,null,"X","X",null,"X",null,null,null,2190,8033,"ERC/REC 14-03","X","X",null,40,80,90,"Currently no frequencies are assigned to P-P links. In the near future  frequency assignments to the fixed service are not planned."]
["Russia","RUS",0,"3600-4200","X","X",null,null,null,null,"X",null,"X",null,null,null,688,null,"ERC/REC 12-08","X","X","X",40,80,90]
["Russia","RUS",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.635 ITU-R"]
["Russia","RUS",0,"4400-5000","X","X",null,null,null,null,"X",null,"X",null,null,null,344,null,"F.382 ITU-R","X","X","X",40,80,90]
["Russia","RUS",0,"5850-5925","X","X",null,null,null,"X","X",null,"X",null,null,null,1350,623,null,"X","X","X",30,70,90]
["Russia","RUS",0,"5925-7125","X","X",null,null,"X","X","X",null,"X",null,null,null,3411,1942,"ERC/REC 14-01 and ERC/REC 14-02","X","X","X",30,55,65]
["Russia","RUS",0,"5925-7125",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.383 ITU-R"]
["Russia","RUS",0,"7125-7750","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",10495,null,"F.385 ITU-R","X","X","X",30,55,65]
["Russia","RUS",0,"7750-7900","No","No"]
["Russia","RUS",0,"7900-8500","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",4584,null,"F.386 ITU-R","X","X","X",30,55,65]
["Russia","RUS",0,"10000-10680","X","X",null,null,null,"X","X",null,"X",null,null,"less than 1%",247,1490,"ERC/REC 12-05","X","X","X",15,30,40]
["Russia","RUS",0,"10700-11700","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",1207,null,"ERC/REC 12-06","X","X","X",15,30,40]
["Russia","RUS",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.387 ITU-R"]
["Russia","RUS",0,"11700-12500","No","No"]
["Russia","RUS",0,"12750-13250","X","X",null,null,null,null,"X",null,"X",null,null,"less than 1%",16553,null,"ERC/REC 12-02 e ITU-R F.497","X","X","X",10,25,35]
["Russia","RUS",0,"14250-14500","X","X",null,null,null,null,null,null,null,null,null,null,150,null,null,"X","X","X",8,20,30]
["Russia","RUS",0,"14500-14620 and 15230-15350","X","X",null,null,null,null,"X",null,"X",null,null,12,13320,null,"ERC/REC 12-07 e ITU-R F.636","X","X","X",8,20,30]
["Russia","RUS",0,"17300-17700","No","No"]
["Russia","RUS",0,"17700-19700","X","X",null,null,null,null,null,null,null,null,null,null,24277,null,"ERC/REC 12-03 and ITU-R F.595-9 ","X","X","X",5,12,20]
["Russia","RUS",0,"21200-23600","X","X",null,null,null,null,null,null,null,null,null,null,16816,null,"F.637 ITU-R","X","X","X",2,4,8]
["Russia","RUS",0,"24250-24500","No","No",null,null,null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["Russia","RUS",0,"24500-26500","X","X",null,null,null,"X","X",null,null,null,null,null,447,null,"T/R 13-02 Annex B","X","X","X",2,4,8]
["Russia","RUS",0,"24500-26500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["Russia","RUS",0,"26500-27500","X","X",null,null,null,"X","X",null,null,null,null,null,26,null,"F.748 ITU-R","X","X","X",2,4,8]
["Russia","RUS",0,"27500-29500","X","X",null,null,null,"X","X",null,null,null,null,null,1,null,"T/R 13-02 Annex C","X","X","X",2,4,8]
["Russia","RUS",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.748 ITU-R"]
["Russia","RUS",0,"31000-31300","No","No",null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(02)02"]
["Russia","RUS",0,"31800-33400","No","No",null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02"]
["Russia","RUS",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(04)06"]
["Russia","RUS",0,"36000-37000","X","X",null,null,null,null,"X",null,null,null,null,null,132,null,"F.749 ITU-R","X","X","X",0.1,3,5]
["Russia","RUS",0,"37000-39500","X","X",null,null,null,null,"X",null,null,null,null,null,16865,null,"T/R 12-01","X","X","X",0.1,3,5]
["Russia","RUS",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.749 ITU-R"]
["Russia","RUS",0,"40500-43500","X","X",null,null,null,"X","X",null,null,null,null,null,73,null,"ECC/REC/(01)04","X","X","X",0.1,3,5]
["Russia","RUS",0,"47200-48500"]
["Russia","RUS",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10"]
["Russia","RUS",0,"50400-51400"]
["Russia","RUS",0,"51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11"]
["Russia","RUS",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12"]
["Russia","RUS",0,"57000-59000","X","X",null,null,null,null,"X",null,null,null,null,null,420,null,"ECC/REC/(09)01","X","X",null,0.1,1,2]
["Russia","RUS",0,"57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"F.1497 ITU-R"]
["Russia","RUS",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01"]
["Russia","RUS",0,"71000-76000 and  81000-86000",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07"]
["Russia","RUS",0,"92000-95000",null,null,null,"X"]
["Serbia","SRB",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["Serbia","SRB",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["Serbia","SRB",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defense systems"]
["Serbia","SRB",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,51,"ERC/REC 14-03",null,null,null,null,null,null,50]
["Serbia","SRB",0,"3600-3800",null,"X",null,null,null,"X",null,null,null,null,null,null,null,1,"ERC/REC 12-08"]
["Serbia","SRB",0,"3800-4200","X",null,null,null,null,null,"X",null,null,null,null,null,3,null,"ITU-R F.382-8",null,null,"X",72.09,74.02,77.89]
["Serbia","SRB",0,"4400-5000",null,null,null,null,null,null,null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"defence systems"]
["Serbia","SRB",0,"4400-5000"]
["Serbia","SRB",0,"5850-5925",null,null,null,"X",null,null,null,null,null,null,"X",null,null,null,"ERC/REC 70-03",null,null,null,null,null,null,null,null,null,"SRD"]
["Serbia","SRB",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,205,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,"X",17,45,79,30]
["Serbia","SRB",0,"7125-7725","X",null,null,null,null,null,"X",null,null,null,null,null,138,null,"ITU-R F.385-9 base","X","X","X",11.67,37.979999999999997,104.2,150]
["Serbia","SRB",0,"7725–8275","X",null,null,null,null,null,"X",null,null,null,null,null,8,null,"ITU-R F.386-8 annex 6",null,"X","X",9.44,35.68,70.27,300]
["Serbia","SRB",0,"8275-8500","X",null,null,null,null,null,"X",null,null,null,null,null,10,null,"ITU-R F.386-8 annex 2",null,"X","X",21,53.77,98.71,300]
["Serbia","SRB",0,"10000-10680","X",null,null,null,null,null,null,null,"X",null,null,76,3,null,"national plan","X",null,null,0.7,24.72,114.99,20]
["Serbia","SRB",0,"10700-11700","X",null,null,null,null,null,"X",null,null,null,null,null,48,null,"ERC/REC 12-06",null,null,"X",7.13,15.72,37.700000000000003,300]
["Serbia","SRB",0,"11700-12500",null,"X",null,null,null,null,null,null,"X",null,null,null,null,15,null,null,null,"X"]
["Serbia","SRB",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,564,null,"ERC/REC 12-02","X","X","X",2.15,19.579999999999998,58.65,50]
["Serbia","SRB",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it have not been used yet"]
["Serbia","SRB",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,433,null,"ERC/REC 12-07","X","X","X",1.35,16.98,39.26,20]
["Serbia","SRB",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["Serbia","SRB",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,459,null,"ERC/REC 12-03 and ITU-R F.595-9 ","X","X","X",0.91,10.029999999999999,35.159999999999997,100]
["Serbia","SRB",0,"21200-22000","X",null,null,null,null,null,null,null,"X",null,null,3,null,null,"ITU-R F.637-3 annex 5 ","X",null,null,3.11,4.9800000000000004,7.15]
["Serbia","SRB",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,1288,null,"T/R 13-02 Annexes A1","X","X","X",0.14000000000000001,4.74,24.41,100]
["Serbia","SRB",0,"22600-23000","X",null,null,null,null,null,null,null,"X",null,null,94,null,null,"ITU-R F.637-3 annex 5 ","X",null,null,0.21,2.5,11.87]
["Serbia","SRB",0,"24500-26500","X",null,null,null,null,null,"X",null,null,null,null,null,660,null,"T/R 13-02 Annex B","X","X","X",0.6,2.21,12.5,100]
["Serbia","SRB",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,4]
["Serbia","SRB",0,"26500-27500",null,null,null,null,null,null,null,null,null,"X"]
["Serbia","SRB",0,"27500-29500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["Serbia","SRB",0,"27500-29500"]
["Serbia","SRB",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,null,null,null,"it have not been used yet"]
["Serbia","SRB",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,426,null,"T/R 12-01","X","X","X",0.16,1.4,4.8600000000000003,300]
["Serbia","SRB",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,null,null,null,"it has not been used yet"]
["Serbia","SRB",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-10",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Serbia","SRB",0,"51400-52600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-11",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Serbia","SRB",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Serbia","SRB",0,"57000-59000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Serbia","SRB",0,"59000-64000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Serbia","SRB",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,null,null,null,"It has not been used yet"]
["Slovak Republic","SVK",0,"1375-1400 and 1427-1452",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovak Republic","SVK",0,"1427-1530","X",null,null,null,null,"X",null,null,null,null,null,null,null,null,"Rep.CCIR 379-5, DS 65,5MHz","x",null,null,null,null,null,-100,null,"x","no new links"]
["Slovak Republic","SVK",0,"1427-1530",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"relocation to other band"]
["Slovak Republic","SVK",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovak Republic","SVK",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,null,null,null,198,"ERC/REC 14-03","X",null,null,null,null,null,10]
["Slovak Republic","SVK",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,null,null,null,"N.A. FWA planned"]
["Slovak Republic","SVK",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovak Republic","SVK",0,"5925-6425","X",null,null,null,"X",null,"X",null,null,null,null,null,81,null,"ERC/REC 14-01 ",null,null,"X",8.5,20,54,25]
["Slovak Republic","SVK",0,"6430-7110","X",null,null,null,"X",null,"X",null,null,null,null,null,2,null,"ERC/REC 14-02",null,null,"X",44,49,54,"0-100 ",null,null,"expected growth"]
["Slovak Republic","SVK",0,"7125-7425","X",null,null,null,"X",null,"X",null,null,null,null,null,30,null,"ECC REC (02)06",null,null,"X",17,25,44.5,50]
["Slovak Republic","SVK",0,"7125-7425","X",null,null,null,"X",null,"X",null,null,null,null,null,14,null,"ITU-R F.385, DS 161MHz","X","X",null,7,25,58,-100,null,"x","no new links"]
["Slovak Republic","SVK",0,"7425-7725","X",null,null,null,"X",null,"X",null,null,null,null,null,70,null,"ITU-R F.385-9, DS 161MHz","X","X",null,5,25,55,10]
["Slovak Republic","SVK",0,"7700-8300","X",null,null,null,"X",null,"X",null,null,null,null,null,35,null,"ITU-R F.386-4, Annex 1",null,null,"X",8,30,58,-100,null,"x","no new links"]
["Slovak Republic","SVK",0,"10000-10680",null,"X",null,null,null,"X",null,null,null,null,null,null,null,110,"ERC/REC 12-05","x","x",null,null,null,null,10]
["Slovak Republic","SVK",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,0,null,"ERC/REC 12-06",null,null,"x",null,null,null,100,null,null,"operation expected"]
["Slovak Republic","SVK",0,"11700-12500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovak Republic","SVK",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,620,null,"ERC/REC 12-02","X","X","X",4,15,48,20]
["Slovak Republic","SVK",0,"14250-14500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovak Republic","SVK",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,230,null,"ERC/REC 12-07","x","x",null,9.5,15,48,10]
["Slovak Republic","SVK",0,"17300-17700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovak Republic","SVK",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,null,null,2170,null,"ERC/REC 12-03","x","x","x",1,10,38,20]
["Slovak Republic","SVK",0,"21200-22000","X",null,null,null,"X",null,null,null,"X",null,null,0,null,null,"ITU-R F.637",null,null,null,null,null,null,null,null,null,"currently no links"]
["Slovak Republic","SVK",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,1582,null,"T/R 13-02 Annex A1","x","x","x",0.5,5,13,10]
["Slovak Republic","SVK",0,"22600-23000","x",null,null,null,"X",null,null,null,"X",null,null,0,null,null,"ITU-R F.637",null,null,null,null,null,null,null,null,null,"currently no links"]
["Slovak Republic","SVK",0,"24250-24500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovak Republic","SVK",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,1230,null,"T/R 13-02 Annex B","x","x","x",0.1,3.5,8,20]
["Slovak Republic","SVK",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,40,null,"x","x",null,null,null,null,10]
["Slovak Republic","SVK",0,"26500-27500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N.A."]
["Slovak Republic","SVK",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,110,null,"T/R 13-02 Annex C","x","x","x",0.2,2.5,4.5,10]
["Slovak Republic","SVK",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,15,null,"x","x",null,null,null,null,10]
["Slovak Republic","SVK",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC/(01)02",null,null,null,null,null,null,100,null,null,"operation expected"]
["Slovak Republic","SVK",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,1600,null,"T/R 12-01","x","x","x",0.1,2,9,20]
["Slovak Republic","SVK",0,"40500-43500",null,"X",null,null,null,"X",null,null,"X",null,null,null,null,3,"ECC/REC/(01)04",null,"x"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,"X",null,null,52,null,null,"T/R 13-01 Annex A","x",null,null,2,15,52,100,null,null,"From band 1517.5 - 1530 MHz"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517",null,"X",null,null,null,null,null,null,null,"X",null,null,"N/A",null,"T/R 13-01 Annex A","x",null,null,5,20,90,0,"x",null,null,"assigned all SVN (2MHz Ch.1)"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517","X",null,null,null,null,"X","X",null,null,null,null,null,null,17,"T/R 13-01 Annex A","x",null,null,5,15,50,2,"x"]
["Slovenia","SVN",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,"X",null,null,null,null,null,20,null,"T/R 13-01 Annex A","x",null,null,5,20,90,10,"x"]
["Slovenia","SVN",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,"X",null,null,12,null,null,"T/R 13-01 Annex B","x",null,null,2,15,52,200,null,null,"From band 1517.5 - 1530 MHz"]
["Slovenia","SVN",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,"X",null,null,null,null,null,1,null,"T/R 13-01 Annex B",null,null,null,5,10,30,200]
["Slovenia","SVN",0,"1517-1525","X",null,null,null,"X",null,null,null,"X",null,null,92,null,null,"national (500kHz)","x",null,null,2,15,52,-50,null,"x","realocated into 1.4 GHz bands"]
["Slovenia","SVN",0,"1525-1530","X",null,null,null,"X",null,null,null,"X",null,null,6,null,null,"national (500kHz)","x",null,null,2,15,52,-100,null,"x","realocated into 1.4 GHz bands"]
["Slovenia","SVN",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Slovenia","SVN",0,"3400-3600",null,"X",null,null,null,"X",null,null,null,null,"BWA",null,null,10,"ERC/REC 14-03",null,"X",null,5,30,70,400]
["Slovenia","SVN",0,"3600-3800","X",null,null,null,"X",null,null,null,"X",null,null,null,2,null,"ERC/REC 12-08",null,null,"X",null,null,null,-100,null,"x","BWA"]
["Slovenia","SVN",0,"3600-3800","X",null,null,null,"X",null,null,null,"X",null,null,1,null,null,"ERC/REC 12-08",null,null,"X",10,45,90,-100,null,"x","BWA"]
["Slovenia","SVN",0,"3600-3800",null,"X",null,null,null,"X",null,null,null,null,"BWA",null,null,"planned","ERC/REC 12-08",null,"X",null,null,null,null,">400",null,null,"BWA"]
["Slovenia","SVN",0,"3800-4200","X",null,null,null,"X",null,null,null,"X",null,null,null,18,null,"ERC/REC 12-08",null,null,"X",30,60,90,null,"X*",null,"congested in backbone directions"]
["Slovenia","SVN",0,"3800-4200","X",null,null,null,"X",null,null,null,"X",null,null,18,null,null,"ERC/REC 12-08",null,null,"X",10,30,90,null,"X*",null,"congested in backbone directions"]
["Slovenia","SVN",0,"5850-5925"]
["Slovenia","SVN",0,"5925–6425 ","X",null,null,null,"X",null,"X",null,null,null,null,null,6,null,"ERC/REC 14-01 ",null,null,"X",12,50,75,30]
["Slovenia","SVN",0,"5925–6425 ","X",null,null,null,"X",null,null,null,"X",null,null,null,2,null,"ERC/REC 14-01 ",null,null,null,20,55,65,50]
["Slovenia","SVN",0,"5925–6425 ",null,"X",null,null,"X",null,null,null,"X",null,null,null,4,null,"ERC/REC 14-01 ",null,null,null,5,25,65,0,"x"]
["Slovenia","SVN",0,"6425-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,14,null,"ERC/REC 14-02",null,null,"X",20,40,50,50]
["Slovenia","SVN",0,"7125-7425","X",null,null,null,"X",null,"X",null,null,null,null,null,23,null,"ECC REC (02)06",null,null,"X",10,25,45,10,"x"]
["Slovenia","SVN",0,"7125-7425","X",null,null,null,"X",null,null,null,"X",null,null,null,43,null,"ECC REC (02)06",null,null,"X",5,25,65,5,"x"]
["Slovenia","SVN",0,"7425–7725","X",null,null,null,"X",null,"X",null,null,null,null,null,26,null,"ECC REC (02)06",null,null,"X",10,25,45,20]
["Slovenia","SVN",0,"7425–7725","X",null,null,null,"X",null,null,null,"X",null,null,null,5,null,"ECC REC (02)06",null,null,"X",3,25,60,30]
["Slovenia","SVN",0,"7725–8275","X",null,null,null,"X",null,null,null,"X",null,null,6,42,null,"ITU-R F 386-8 An6  (29.65 MHz, DS 311.32 MHz)",null,null,"X",15,35,60,5,"x*",null,"congested in backbone directions"]
["Slovenia","SVN",0,"8275-8500","X",null,null,null,"X",null,"X",null,null,null,null,null,14,null,"ITU-R F.386-8 An2 (28 MHz , DS 119 MHz, 14 MHz, DS 126 MHz)",null,"X",null,20,35,70,30,"x*",null,"congested in backbone directions"]
["Slovenia","SVN",0,"10000-10680","X",null,null,null,"X",null,null,null,"X",null,null,53,null,null,"ERC/REC 12-05",null,"x","x",2,25,65,-100,null,"x","BWA when SAP/SAB P to P video links analogue cease operation"]
["Slovenia","SVN",0,"10000-10680","X",null,null,null,"X",null,null,null,"X",null,null,null,8,null,"ERC/REC 12-05",null,"x","x",2,25,62,-100,null,"x","BWA when SAP/SAB P to P video links analogue cease operation"]
["Slovenia","SVN",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,13,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",7,40,46,50,null,null,null,"In accordance with CEPT and ITU limitations"]
["Slovenia","SVN",0,"10700-11700","X",null,null,null,"X",null,null,null,"X",null,null,3,null,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",35,40,46,5,null,null,null,"In accordance with CEPT and ITU limitations"]
["Slovenia","SVN",0,"10700-11700","X",null,null,null,"X",null,null,null,"X",null,null,null,3,null,"ERC/REC 12-06, ITU-R F.387",null,null,"x",33,40,47,5,null,null,null,"In accordance with CEPT and ITU limitations"]
["Slovenia","SVN",0,"11700-12500",null,"X",null,null,null,"X",null,null,null,null,"MMDS",null,null,20,"National (200/400 MHz)",null,null,"x",5,30,40,10,null,null,null,"assigned for local/regional coverage"]
["Slovenia","SVN",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,178,null,"ERC/REC 12-02",null,"X","X",2,25,54,5,"x"]
["Slovenia","SVN",0,"12750-13250","X",null,null,null,"X",null,null,null,"X",null,null,null,21,null,"ERC/REC 12-02",null,null,"X",5,20,40,5,"x"]
["Slovenia","SVN",0,"14250-14500"]
["Slovenia","SVN",0,"14500-14620 and 15230-15350",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07",null,null,null,null,null,null,null,null,null,"Defence systems:","Land military systems (FS, MS)"]
["Slovenia","SVN",0,"14613-14725 and 15033-15145","X",null,null,null,"X",null,"X",null,null,null,null,null,82,null,"ITU-R F.636-3 (Ch. 5,6,7,8)",null,"x",null,7,25,45,-10,null,"x"]
["Slovenia","SVN",0,"14613-14725 and 15033-15145",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-07",null,null,null,null,null,null,null,null,"x","Defence systems:","Land military systems (FS, MS)"]
["Slovenia","SVN",0,"17700-19700","X",null,null,null,"X",null,"X",null,null,null,null,null,361,null,"ERC/REC 12-03",null,null,"x",5,15,35,20,"x**",null,"congested in urban/sub urban regions"]
["Slovenia","SVN",0,"17700-19700",null,"X",null,null,"X",null,"X",null,null,null,null,null,300,null,"ERC/REC 12-03",null,"x","x",5,15,35,0,"x**",null,"congested in urban/sub urban regions"]
["Slovenia","SVN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,767,null,"T/R 13-02 Annex A1",null,"x",null,3,7,10,5,"x**",null,"congested in urban/sub urban regions"]
["Slovenia","SVN",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,10,null,"T/R 13-02 Annex A1",null,null,"x",2,4,5,20,"x**",null,"congested in urban/sub urban regions"]
["Slovenia","SVN",0,"22600-23000","x",null,null,null,"X",null,"X",null,null,null,null,null,"planned",null,"T/R 13-02 Annex A2","x","x"]
["Slovenia","SVN",0,"22600-23000",null,null,null,null,"X",null,null,null,"X","X",null,"planned",null,null,"T/R 13-02 Annex A3","x","x"]
["Slovenia","SVN",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,109,null,"T/R 13-02 Annex B (25.165-25.557 GHz/>26.173 GHz)",null,"x",null,3,6,8,100,null,null,null,"used instead of the congested 23 GHz band"]
["Slovenia","SVN",0,"24500-26500","X",null,null,null,null,"X","X",null,null,null,null,null,null,22,"T/R13-02 AnnexB (25.053-25.165GHz/26.061-26.173GHz)",null,"x",null,null,null,null,-5]
["Slovenia","SVN",0,"24500-26500",null,"X",null,null,null,"X",null,null,null,null,"BWA",null,null,"planned","T/R13-02 Annex B (24.549–25.053GHz/25.557–26.061GHz)",null,"x","x",1,3,5,null,null,null,"BWA"]
["Slovenia","SVN",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,"planned",null,"T/R 13-02 Annex C (27.8285 – 27.9405 GHz/28.8365 – 28.9485 GHz)",null,"x",null,0.5,3,5]
["Slovenia","SVN",0,"27500-29500",null,"X",null,null,null,"X",null,null,null,null,null,null,null,"planned","T/R13-02 Annex C (27.9405 – 28.4445 GHz/28.9485 – 29.4525 GHz)",null,"x","x",0.3,2,4]
["Slovenia","SVN",0,"31800-33400","x",null,null,null,"X",null,"X",null,null,null,null,null,"planned Upper part",null,"ERC/REC/(01)02",null,"x","x",0.2,2,4]
["Slovenia","SVN",0,"31800-33400",null,"x",null,null,null,"X",null,null,null,null,"BWA",null,"planned Lower part",null,"ERC/REC/(01)02/ ECC/REC/(04)06",null,"x","x",0.2,1,3,null,null,null,"BWA"]
["Slovenia","SVN",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,580,null,"T/R 12-01",null,"x",null,0.1,2,4,30,"x***",null,null,"HI/LO problem"]
["Slovenia","SVN",0,"37000-39500","X",null,null,null,"X",null,"X"]
["Slovenia","SVN",0,"40500-43500",null,"X",null,null,null,"X",null,null,null,null,"MWS",null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"planned Upper part",null,null,"MWS"]
["Slovenia","SVN",0,"40500-43500","X",null,null,null,"X",null,"X",null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"planned Lower part (only small part)"]
["Slovenia","SVN",0,"48500-50200",null,null,null,null,null,null,null,null,null,null,null,null,"planned",null,"ERC/REC 12-10"]
["Slovenia","SVN",0,"51400-52600","X",null,null,null,"X",null,"X",null,null,null,null,null,"planned",null,"ERC/REC 12-11",null,"x","x",0.1,2,4]
["Slovenia","SVN",0,"55780-57000",null,null,null,null,null,null,null,null,null,null,null,null,"planned",null,"ERC/REC 12-12"]
["Slovenia","SVN",0,"57000-59000",null,null,null,"X","X",null,null,null,null,null,null,null,"N/A",null,"ECC/REC/(09)01",null,null,"x",null,1,null,"N/A"]
["Slovenia","SVN",0,"74000-76000 and 84000-86000","X",null,null,null,"X",null,null,null,null,"X",null,null,"planned",null,"ECC/REC/(05)07",null,null,"x"]
["Sweden","SWE",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,null,null,59,99,null,"T/R 13-01 Annex B",null,null,null,null,null,null,null,"N"]
["Sweden","SWE",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Sweden","SWE",0,"3400-3600",null,"X",null,null,"X","X","X",null,"X",null,"X",null,null,null,"ERC/REC 14-03",null,null,null,null,null,null,"Y","N",null,"IMT-?"]
["Sweden","SWE",0,"3600-4200",null,"X",null,null,"X","X","X",null,"X",null,"X",null,null,null,"ERC/REC 12-08",null,null,null,null,null,null,"Y","N",null,"IMT-?"]
["Sweden","SWE",0,"5850-5925"]
["Sweden","SWE",0,"5925-7125","X",null,null,null,"X",null,null,null,null,null,null,null,952,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,null,null,null,null,null,"Y"]
["Sweden","SWE",0,"7425-7725","X",null,null,null,"X",null,null,null,null,null,null,null,1421,null,null,null,"X",null,null,null,null,null,"Y"]
["Sweden","SWE",0,"7900-8500","X",null,null,null,"X",null,null,null,null,null,null,null,494,null,"ECC REC (02)06",null,"X",null,null,null,null,"Y","N"]
["Sweden","SWE",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05\nNew ITU-R Rec under dev.",null,null,null,null,null,null,"Y","N",null,"Blockassignment?"]
["Sweden","SWE",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,7,1,null,"ERC/REC 12-06"]
["Sweden","SWE",0,"11700-12500"]
["Sweden","SWE",0,"12750-13250","X",null,null,null,"X",null,null,null,null,null,null,null,775,null,"ERC/REC 12-02",null,null,null,null,null,null,null,"Y"]
["Sweden","SWE",0,"14250-14500"]
["Sweden","SWE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,null,null,null,null,null,null,2629,null,"Nat ch.plan(expdate 2016)",null,null,null,null,null,null,null,"Y"]
["Sweden","SWE",0,"17700-19700","X",null,null,null,"X",null,null,null,null,null,null,null,2242,null,"ERC/REC 12-03",null,null,null,null,null,null,"Y","N"]
["Sweden","SWE",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,null,null,null,null,null,null,1322,null,"T/R 13-02 Annexes A1, A2, A3",null,null,null,null,null,null,null,"Y"]
["Sweden","SWE",0,"24500-26500",null,"X",null,null,"X","X","X",null,null,null,null,null,5601,null,"T/R 13-02 Annex B",null,null,null,null,null,null,"Y"]
["Sweden","SWE",0,"24500-26500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null," ERC / REC / (00) 05",null,null,null,null,null,null,null,"N"]
["Sweden","SWE",0,"27500-29500",null,"X",null,null,"X","X","X",null,null,null,null,null,null,null,"T/R 13-02 Annex C",null,null,null,null,null,null,"Y"]
["Sweden","SWE",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,1887,null,"ERC/REC/(01)02"]
["Sweden","SWE",0,"31800-33400","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"ECC/REC/(04)06",null,null,null,null,null,null,"Y","N"]
["Sweden","SWE",0,"37000-39500",null,null,null,null,null,null,null,null,null,null,null,null,6188,null,"T/R 12-01"]
["Sweden","SWE",0,"37000-39500","X",null,null,null,"X",null,null,null,null,null,null,null,null,null,"T/R 12-01",null,null,null,null,null,null,"Y","N"]
["Sweden","SWE",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04\n(New ITU-R Rec under dev.)",null,null,null,null,null,null,"Y","N",null,"Blockassignments?"]
["Sweden","SWE",0,"55780-57000",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"ERC/REC 12-12",null,null,null,null,null,null,null,"N"]
["Sweden","SWE",0,"57000-59000",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Y","N",null,"Exemption"]
["Sweden","SWE",0,"59000-64000",null,null,null,"X","X",null,null,null,null,null,null,null,null,null,"ECC/REC/(09)01",null,null,null,null,null,null,"Y","N",null,"Exemption"]
["Sweden","SWE",0,"71000-76000 and  81000-86000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(05)07",null,null,null,null,null,null,"Y","N",null,"Light Lic?"]
["Sweden","SWE",0,"92000-95000",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N",null,"Light Lic?"]
["switzerland","CHE",0,"1350-1375 and 1492-1517","X",null,null,null,"X",null,null,null,null,"X",null,null,15,null,"T/R 13-01 Annex A",15,null,null,20,null,30.5,"reduction"]
["switzerland","CHE",0,"1375-1400 and 1427-1452","X",null,null,null,"X",null,null,null,null,"X",null,null,152,null,"T/R 13-01 Annex B",152,null,null,20,null,61.9,"reduction"]
["switzerland","CHE",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,"No civil FS use",null,null,null,"T/R 13-01 Annex C"]
["switzerland","CHE",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ERC/REC 14-03"]
["switzerland","CHE",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ERC/REC 12-08"]
["switzerland","CHE",0,"4400-5000",null,null,null,null,null,null,null,null,null,null,"No civil FS use"]
["switzerland","CHE",0,"4400-5000"]
["switzerland","CHE",0,"5850-5925",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast"]
["Switzerland","CHE",0,"5925-7125","X",null,null,null,"X",null,"X",null,null,null,null,null,60,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,60,30,39.700000000000003,81.7,"growth"]
["Switzerland","CHE",0,"7125-7750","X",null,null,null,"X",null,"X",null,null,null,null,null,171,null,"ECC REC (02)06",70,81,20,20,30.2,99.5,"growth"]
["Switzerland","CHE",0,"7750-7900",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast"]
["Switzerland","CHE",0,"7900-8500",null,null,null,null,null,null,null,null,null,null,"ENG-Outside Broadcast",null,null,null,"ECC REC (02)06"]
["Switzerland","CHE",0,"10000-10680","X",null,null,null,"X",null,"X",null,null,null,null,null,64,null,"ERC/REC 12-05",18,46,null,15,18.3,48.5,"growth"]
["Switzerland","CHE",0,"10700-11700","X",null,null,null,"X",null,"X",null,null,null,null,null,80,null,"ERC/REC 12-06",null,null,80,10,14.9,34.9,"growth",null,null,"heavily used by FSS"]
["Switzerland","CHE",0,"11700-12500"]
["Switzerland","CHE",0,"12750-13250","X",null,null,null,"X",null,"X",null,null,null,null,null,470,null,"ERC/REC 12-02",174,290,6,10,14.2,46.4,"unchanged",null,null,"heavily used by FSS"]
["Switzerland","CHE",0,"14250-14500"]
["Switzerland","CHE",0,"14500-14620 and 15230-15350","X",null,null,null,"X",null,"X",null,null,null,null,null,263,null,"ERC/REC 12-07",110,153,null,10,14.6,37.1,"unchanged"]
["switzerland","CHE",0,"22000-22600 and 23000-23600","X",null,null,null,"X",null,"X",null,null,null,null,null,1900,null,"T/R 13-02 Annexes A1, A2, A3",787,1113,null,5,7.4,29.9,"unchanged","city areas congested, HIGH/LOW situation",null,"problem: SRR"]
["switzerland","CHE",0,"24500-26500","X",null,null,null,"X",null,"X",null,null,null,null,null,38,null,"T/R 13-02 Annex B",null,null,38,2,2.9,5.9,"growth",null,null,"problem: SRR"]
["switzerland","CHE",0,"24500-26500"]
["switzerland","CHE",0,"27500-29500","X",null,null,null,"X",null,"X",null,null,null,null,null,"starts now",null,"T/R 13-02 Annex C",null,null,null,null,null,null,"growth"]
["switzerland","CHE",0,"27500-29500"]
["switzerland","CHE",0,"31800-33400","X",null,null,null,"X",null,"X",null,null,null,null,null,102,null,"ERC/REC/(01)02",null,69,33,0.5,2.2999999999999998,4.5999999999999996,"growth"]
["switzerland","CHE",0,"37000-39500","X",null,null,null,"X",null,"X",null,null,null,null,null,3134,null,"T/R 12-01",1248,1886,null,1,2.6,7.9,"unchanged","city areas congested, HIGH/LOW situation"]
["switzerland","CHE",0,"40500-43500","X",null,null,null,"X",null,"X",null,null,null,null,null,null,null,"ECC/REC/(01)04",null,null,null,null,null,null,"growth. Starts now"]
["switzerland","CHE",0,"51400-52600",null,"X",null,null,"X",null,"X",null,null,null,null,null,837,null,"ERC/REC 12-11",193,644,null,0.15,0.8,2.8,"growth"]
["switzerland","CHE",0,"55780-57000",null,"X",null,null,"X",null,"X",null,null,null,null,null,0,null,"ERC/REC 12-12",null,null,null,null,null,null,"no equipment available"]
["switzerland","CHE",0,"57000-58000",null,"X",null,null,"X",null,"X",null,null,null,null,null,292,null,"ECC/REC/(09)01",292,null,null,0.1,0.3,2.2000000000000002,"reduction"]
["switzerland","CHE",0,"58000-63000",null,null,null,"X",null,null,null,null,null,null,null,null,0,null,"ECC/REC/(09)01",null,null,null,null,null,null,"no equipment available"]
["switzerland","CHE",0,"71000-76000 and  81000-86000","X",null,null,null,"X",null,"X",null,null,null,null,null,"starts now",null,"ECC/REC/(05)07",null,null,null,null,null,null,"equipment not clear defined"]
["Telia","TELIASON",0,"1350-1375 and 1492-1517",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex A"]
["Telia","TELIASON",0,"1375-1400 and 1427-1452","X",null,null,null,null,null,"X",null,null,null,null,null,17,null,"T/R 13-01 Annex B","X",null,null,4,null,19,0,null,null,null,"IDR140"]
["Telia","TELIASON",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C"]
["Telia","TELIASON",0,"3400-3600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 14-03"]
["Telia","TELIASON",0,"3600-4200",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-08"]
["Telia","TELIASON",0,"5850-5925"]
["Telia","TELIASON",0,"5925-7125","X",null,null,null,null,null,"X",null,null,null,null,null,19,null,"ERC/REC 14-01 and ERC/REC 14-02",null,null,19,6,null,40,null,"X"]
["Telia","TELIASON",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,22,null,"ECC REC (02)06",null,22,null,15,null,42,null,"X",null,null,"NEC 770"]
["Telia","TELIASON",0,"7125-7750","X",null,null,null,null,null,"X",null,null,null,null,null,128,null,null,74,54,null,7,null,80,null,"X",null,null,"Eric sson ML"]
["Telia","TELIASON",0,"7750-7900"]
["Telia","TELIASON",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,8,null,"ECC REC (02)06",null,8,null,16,null,68,null,"X",null,null,"NEC 770"]
["Telia","TELIASON",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,37,null,null,null,11,26,13,null,68,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"7900-8500","X",null,null,null,null,null,"X",null,null,null,null,null,1,null,null,null,null,1,null,34,null,"++",null,null,null,"Ericsson TN"]
["Telia","TELIASON",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["Telia","TELIASON",0,"10700-11700",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-06"]
["Telia","TELIASON",0,"11700-12500"]
["Telia","TELIASON",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,302,null,"ERC/REC 12-02",210,null,92,3,null,50,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,22,null,null,null,null,22,9,null,42,"-",null,null,null,"NERA Citylink"]
["Telia","TELIASON",0,"12750-13250","X",null,null,null,null,null,"X",null,null,null,null,null,80,null,null,32,48,null,5,null,29,0,null,null,null,"Eric sson ML"]
["Telia","TELIASON",0,"14250-14500"]
["Telia","TELIASON",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,944,null,"ERC/REC 12-07",620,324,null,1,null,39,"-",null,null,null,"Eric sson ML"]
["Telia","TELIASON",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,"X",null,null,null,null,null,93,null,null,93,null,null,3,null,30,null,"X",null,null,"NEC Pasolink"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,3,null,"ERC/REC 12-03",null,null,3,9,null,11,null,"X",null,null,"NEC 900"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,23,null,null,null,null,23,3,null,14,0,null,null,null,"NERA Citylink"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,738,null,null,null,645,93,4,null,28,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"17700-19700","X",null,null,null,null,null,"X",null,null,null,null,null,1,null,null,null,null,1,null,9,null,"++",null,null,null,"Ericsson TN"]
["Telia","TELIASON",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,506,null,"T/R 13-02 Annexes A1, A2, A3",303,203,null,1,null,18,"-",null,null,null,"Eric sson ML"]
["Telia","TELIASON",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,"X",null,null,null,null,null,338,null,null,null,316,22,3,null,17,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"24500-26500",null,"X",null,null,null,null,"X",null,null,null,null,null,161,null,"T/R 13-02 Annex B",99,18,44,2,null,10,"-",null,null,null,"Eric sson ML"]
["Telia","TELIASON",0,"24500-26500",null,"X",null,null,null,null,null,null,null,null,null,null,629,null,null,null,574,55,1,null,12,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"27500-29500",null,"X",null,null,null,null,"X",null,null,null,null,null,6,null,"T/R 13-02 Annex C",null,null,6,1,null,4,"++",null,null,null,"Ericsson TN"]
["Telia","TELIASON",0,"27500-29500"]
["Telia","TELIASON",0,"31800-33400","X",null,null,null,null,null,"X",null,null,null,null,null,1085,null,"ERC/REC/(01)02",null,996,89,0.2,null,8.6999999999999993,"+",null,null,null,"NEC NEO"]
["Telia","TELIASON",0,"37000-39500","X",null,null,null,null,null,"X",null,null,null,null,null,173,null,"T/R 12-01",95,78,null,0.1,null,5.4,0,null,null,null,"Ericsson ML"]
["Telia","TELIASON",0,"40500-43500",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECC/REC/(01)04"]
["UK","GBR",0,"1350-1375 and 1492-1517","X",null,null,null,null,null,null,null,null,"X",null,860,null,null,"T/R 13-01 Annex A","X"]
["UK","GBR",0,"2025-2110 and 2200-2290",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T/R 13-01 Annex C",null,null,null,null,null,null,null,null,null,"row missing in the questionnaire"]
["UK","GBR",0,"3600-4200","X",null,null,null,null,null,null,null,null,"X",null,40,null,null,"ERC/REC 12-08",null,"X","X"]
["UK","GBR",0,"5925-6425","X",null,null,null,null,null,null,null,null,"X",null,220,null,null,"ERC/REC 14-01 ",null,null,"X"]
["UK","GBR",0,"6425-7125","X",null,null,null,null,null,null,null,null,"X",null,330,null,null,"ERC/REC 14-02",null,"X","X"]
["UK","GBR",0,"7425-7900","X",null,null,null,null,null,null,null,null,"X",null,940,null,null,"ITU-R F.385-9","X","X","X"]
["UK","GBR",0,"10000-10680",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ERC/REC 12-05"]
["UK","GBR",0,"11700-12500"]
["UK","GBR",0,"12750-13250","X",null,null,null,null,null,null,null,null,"X",null,3840,340,null,"ERC/REC 12-02","X","X","X"]
["UK","GBR",0,"14250-14500"]
["UK","GBR",0,"14500-14620 and 15230-15350","X",null,null,null,null,null,null,null,null,"X",null,2050,2050,null,"ERC/REC 12-07","X","X","X"]
["UK","GBR",0,"22000-22600 and 23000-23600","X",null,null,null,null,null,null,null,null,"X",null,4750,null,null,"T/R 13-02 ","X","X","X"]
["UK","GBR",0,"24500-26500","X",null,null,null,null,null,null,null,null,"X",null,3570,null,null,"T/R 13-02","X","X","X"]
["UK","GBR",0,"24500-26500"]
["UK","GBR",0,"27500-29500"]
["UK","GBR",0,"27500-29500"]
["UK","GBR",0,"31000-31300","X",null,null,null,null,null,null,null,null,null,"X",null,null,null,"national arrangement"]
["UK","GBR",0,"31800-33400",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"it have not been used yet"]
["UK","GBR",0,"37000-39500","X",null,null,null,null,null,null,null,null,"X",null,12050,null,null,"T/R 12-01","X","X","X"]
["UK","GBR",0,"51400-52600","X",null,null,null,null,null,null,null,null,null,null,0,null,null,"ERC/REC 12-11"]
["UK","GBR",0,"55780-57000","X",null,null,null,null,null,null,null,null,null,null,0,null,null,"ERC/REC 12-12"]
["UK","GBR",0,"57000-59000",null,null,null,"X",null,null,null,null,null,"X",null,null,null,null,"no channel plan"]
["UK","GBR",0,"59000-64000",null,null,null,"X",null,null,null,null,null,"X",null,null,null,null,"no channel plan"]
["UK","GBR",0,"71000-76000 and  81000-86000","X",null,null,null,null,null,null,null,null,"X",null,null,30,null,"no channel plan",null,null,"X"]